{"text_format":"1","workbook":"xlsx","n_sheets":18,"sheets":["Please read","Consolidated BOM","Channel (common)","Channel (frequency)","Voice preamp","Carrier preamp","Internal exc. (left)","Internal exc. (right)","VUV detector","Output, PWM, bridging","Slew-freeze","DC-DC supply","LDO supply","Misc.","Baskets","Channel (calc)","Minimum Order Count","Resistor pricing"],"not_rendered":{"charts":0,"images":6,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Please read","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Consolidated BOM","index":1,"n_rows":271,"n_cols":22,"rows_kept":271,"cut":false,"hidden":false,"merged":[[1,2,2,2]]}
[]
[null,"Last update:","DC/DC supply"]
[null,"2020-03-18"]
[null,"21:36:44"]
[]
[null,"Worksheet:","First Row:","Last Row:"]
[null,"Channel (common)",5,49]
[null,"Channel (calc)",5,292]
[null,"Voice preamp",5,47]
[null,"Carrier preamp",5,47]
[null,"Internal exc. (left)",5,84]
[null,"Internal exc. (right)",5,84]
[null,"VUV detector",5,52]
[null,"Output, PWM, bridging",5,69]
[null,"Slew-freeze",5,54]
[null,"DC-DC supply",5,30]
[null,"Misc.",5,19]
[]
[null,null,null,null,null,null,null,null,null,null,null,"count: 18","count: 1","count: 1","count: 1","count: 1","count: 1","count: 1","count: 1","count: 1","count: 1","count: 1"]
[null,"Type","Identifier","Count","Min. Count","Body Type","Suggested Product","Distri- butor","Order #","Unit price [€]","Total [€]","Channel (common)","Channel (frequency)","Voice preamp","Carrier preamp","Internal exc. (left)","Internal exc. (right)","VUV detector","Output, PWM, bridging","Slew-freeze","DC-DC supply","Misc."]
[1,"IC","78L05",1,null,"TO-92","LM78L05ACZXA","Mouser","511-L78L05ACZ",0.33200000000000002,{"$f":"IF(D21>=E21,D21*J21,E21*J21)","v":0.33200000000000002},null,null,null,null,null,null,null,"IC12"]
[1,"IC","79L05",1,null,"TO-92","LM79L05ACZ","Mouser","511-L79L05ACZ",0.35799999999999998,0.35799999999999998,null,null,null,null,null,null,null,"IC13"]
[1,"IC","CD40106",2,null,"DIL14","CD40106BE","Mouser","595-CD40106BE",0.44500000000000001,0.89,null,null,null,null,null,null,"IC8","IC11"]
[1,"IC","CD4050",1,null,"DIL16","CD4050BE","Mouser","595-CD4050BE",0.46300000000000002,0.46300000000000002,null,null,null,null,null,null,null,"IC9"]
[1,"IC","CD4053",18,null,"DIL16","CD4053BE","Mouser","595-CD4053BE",0.372,6.6959999999999997,"IC5"]
[1,"IC","CD4093",2,null,"DIL14","CD4093BE","Mouser","595-CD4093BE",0.42799999999999999,0.85599999999999998,null,null,null,null,null,null,"IC7",null,"IC5"]
[2,"IC","IRF7319",1,null,"SO-8","IRF7319TRPBF","Mouser","942-IRF7319TRPBF",0.79500000000000004,0.79500000000000004,null,null,null,null,null,null,null,null,null,"IC1"]
[1,"IC","LM13700",2,null,"DIL16","LM13700N","Mouser","926-LM13700N/NOPB",1.82,3.64,null,null,null,null,"IC6","IC6"]
[1,"IC","LM319",5,null,"DIL14","LM319N","Mouser","512-LM319N",0.498,2.4900000000000002,null,null,null,null,"IC4","IC4",null,"IC8, IC10","IC4"]
[4,"IC","LM3916",3,null,"DIL18","LM3916",null,"LM3916",1.98,5.9399999999999995,null,null,"IC5","IC5, IC9"]
[5,"IC","MC33079",36,null,"DIL14","MC33079PG","Rochester","MC33079",0.62,22.32,"IC1, IC2"]
[1,"IC","NE5532",17,10,"DIL8","NE5532AP","Mouser","595-NE5532AP",0.81399999999999995,13.837999999999999,null,null,"IC1, IC2, IC3","IC1, IC2, IC3, IC6, IC7","IC8","IC8","IC6","IC1, IC2, IC3, IC4, IC5, IC6"]
[1,"IC","THAT300",2,null,"DIL14","THAT300P14-U","Mouser","887-300P14-U",7.95,15.9,null,null,null,null,"IC2","IC2"]
[1,"IC","TL072",8,null,"DIL8","TL072IP","Mouser","595-TL072IP",0.59399999999999997,4.7519999999999998,null,null,"IC4","IC4, IC8","IC1","IC1","IC1","IC7, IC16"]
[1,"IC","TL074",51,null,"DIL14","TL074CN","Mouser","595-TL074CN",0.46800000000000003,23.868000000000002,"IC3, IC4",null,null,null,"IC3, IC5, IC7","IC3, IC5, IC7","IC2, IC3, IC4, IC5","IC14, IC15","IC1, IC2, IC3"]
[1,"Transistor","2N3904",47,100,"TO-92","2N3904BU","Mouser","512-2N3904BU",5.0999999999999997E-2,5.0999999999999996,"T1, T2",null,null,null,"T1, T2","T1, T2","T1, T2",null,"T1, T2, T3","T2, T3"]
[1,"Transistor","2N3906",4,null,"TO-92","2N3906BU","Mouser","512-2N3906BU",0.23599999999999999,0.94399999999999995,null,null,null,null,"T3","T3",null,null,null,"T1, T4"]
[1,"JFET","J105",2,null,"TO-92","J105","Mouser","512-J105",0.55300000000000005,1.1060000000000001,null,null,null,null,"J1","J1"]
[1,"JFET","J113",17,5,"TO-92","J113","Mouser","512-J113",0.249,4.2329999999999997,null,null,null,"J1","J2, J3","J2, J3, J4, J5","J1, J2, J3, J4","J1, J2, J3, J4","J1, J2"]
[1,"Diode","1N4148",76,100,"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,1.7999999999999998,"D1, D2",null,"D1, D2, D3, D4","D1, D2, D3, D4, D5, D6, D7, D8","D1, D2","D1, D2","D1, D2, D3, D4, D5, D6, D7, D8, D9, D10, D11, D12","D1, D2, D3, D4","D1, D2, D3, D4, D5, D6, D7, D8"]
[1,"Diode","1N4001",1,null,"DO-41","1N4001RLG","Mouser","863-1N4001RLG",0.183,0.183,null,null,null,null,null,null,null,"D5"]
[2,"Diode","SB540",1,null,"DO-201AD","SB540","Mouser","512-SB540",0.46,0.46,null,null,null,null,null,null,null,null,null,"D1"]
[1,"Resistor","10 Ω",1,null,"0204/0207","MFR-12FTF52-10R","Mouser","603-MFR-12FTF52-10R",0.122,0.122,null,null,null,null,null,null,null,null,"R34"]
[1,"Resistor","47 Ω, 250 mW",181,100,"0204/0207","MFR-12FTF52-47R","Mouser","603-MFR-12FTF52-47R",2.1000000000000001E-2,3.8010000000000002,"R59, R60, R61, R62, R63, R64, R65",null,"R23, R24","R23, R24","R8, R69, R70, R71, R72, R73, R74, R75, R76, R77, R78, R82, R83","R8, R69, R70, R71, R72, R73, R74, R75, R76, R77, R78, R82, R83","R76, R77, R78, R79, R80, R81, R82","R73, R85, R86, R87, R88, R89, R90, R91, R92, R93","R54, R55, R56, R57, R58, R59, R60, R61"]
[1,"Resistor","100 Ω",19,10,"0204/0207","MFR-12FTF52-100R","Mouser","603-MFR-12FTF52-100R",0.06,1.1399999999999999,"R46",null,null,null,null,null,"R49"]
[1,"Resistor","220 Ω",1,null,"0204/0207","MFR-12FTF52-220R","Mouser","603-MFR-12FTF52-220R",0.11899999999999999,0.11899999999999999,null,null,null,null,null,null,null,"R95"]
[1,"Resistor","430 Ω",2,null,"0204/0207","MFR-12FTF52-430R","Mouser","603-MFR-12FTF52-430R",0.11899999999999999,0.23799999999999999,null,null,null,null,"R41","R41"]
[1,"Resistor","470 Ω",5,null,"0204/0207","MFR-12FTF52-470R","Mouser","603-MFR-12FTF52-470R",0.11899999999999999,0.59499999999999997,null,null,null,null,"R40","R40",null,"R45, R46, R75"]
[1,"Resistor","510 Ω",3,null,"0204/0207","MFR-12FTF52-510R","Mouser","603-MFR-12FTF52-510R",0.11899999999999999,0.35699999999999998,null,null,"R20","R20, R50"]
[1,"Resistor","560 Ω",4,null,"0204/0207","MFR-12FTF52-560R","Mouser","603-MFR-12FTF52-560R",0.11899999999999999,0.47599999999999998,null,null,null,null,null,null,null,"R21, R22, R33, R34"]
[1,"Resistor","750 Ω",18,10,"0204/0207","MFR-12FTF52-750R","Mouser","603-MFR-12FTF52-750R",0.06,1.08,"R26"]
[1,"Resistor","820 Ω",2,null,"0204/0207","MFR-12FTF52-820R","Mouser","603-MFR-12FTF52-820R",0.11899999999999999,0.23799999999999999,null,null,null,null,"R9","R9"]
[1,"Resistor","1 kΩ",24,10,"0204/0207","MFR-12FTF52-1K","Mouser","603-MFR-12FTF52-1K",4.5999999999999999E-2,1.1040000000000001,"R43",null,"R3, R33","R3, R33","R34","R34"]
[1,"Resistor","1.5 kΩ",2,null,"0204/0207","MFR-12FTF52-1K5","Mouser","603-MFR-12FTF52-1K5",0.11899999999999999,0.23799999999999999,null,null,null,null,null,null,"R5, R23"]
[1,"Resistor","2.2 kΩ",34,10,"0204/0207","MFR-12FTF52-2K2","Mouser","603-MFR-12FTF52-2K2",0.06,2.04,"R58",null,null,null,"R6, R11","R6, R11","R73, R75","R84","R23, R38, R39, R46, R50, R53","R1, R4, R8"]
[1,"Resistor","3.3 kΩ",41,100,"0204/0207","MFR-12FTF52-3K3","Mouser","603-MFR-12FTF52-3K3",2.1000000000000001E-2,2.1,"R52, R53",null,null,null,"R60, R81","R60, R81",null,"R50"]
[1,"Resistor","3.9 kΩ",1,null,"0204/0207","MFR-12FTF52-3K9","Mouser","603-MFR-12FTF52-3K9",0.11899999999999999,0.11899999999999999,null,null,null,null,null,null,"R3"]
[1,"Resistor","4.7 kΩ",33,10,"0204/0207","MFR-12FTF52-4K7","Mouser","603-MFR-12FTF52-4K7",4.5999999999999999E-2,1.518,"R42",null,null,null,"R33, R44, R46, R59","R33, R44, R46, R59","R13, R36, R46","R39, R81","R9, R25"]
[1,"Resistor","5.1 kΩ",18,10,"0204/0207","MFR-12FTF52-5K1","Mouser","603-MFR-12FTF52-5K1",0.06,1.08,"R49"]
[1,"Resistor","5.6 kΩ",6,10,"0204/0207","MFR-12FTF52-5K6","Mouser","603-MFR-12FTF52-5K6",0.06,0.6,null,null,null,null,"R36, R37","R36, R37","R21, R22"]
[1,"Resistor","6.8 kΩ",16,10,"0204/0207","MFR-12FTF52-6K8","Mouser","603-MFR-12FTF52-6K8",0.06,0.96,null,"500 Hz:  R39\n640 Hz:  R39\n810 Hz:  R39\n1030 Hz:  R39\n1310 Hz:  R39\n1660 Hz:  R39\n2110 Hz:  R39\n2680 Hz:  R39\n3410 Hz:  R39\n4330 Hz:  R39\n5500 Hz:  R39\n7000 Hz:  R39",null,null,null,null,"R19","R47, R48, R59"]
[1,"Resistor","7.5 kΩ",5,null,"0204/0207","MFR-12FTF52-7K5","Mouser","603-MFR-12FTF52-7K5",0.11899999999999999,0.59499999999999997,null,null,"R21","R21, R51",null,null,null,null,"R15, R49"]
[1,"Resistor","8.2 kΩ",40,100,"0204/0207","MFR-12FTF52-8K2","Mouser","603-MFR-12FTF52-8K2",2.1000000000000001E-2,2.1,"R40, R50",null,null,null,null,null,"R14, R34, R47","R60"]
[1,"Resistor","10 kΩ",246,100,"0204/0207","MFR-12FTF52-10K","Mouser","603-MFR-12FTF52-10K",2.1000000000000001E-2,5.1660000000000004,"R27, R28, R29, R30, R31, R32, R33, R34, R41, R51, R54","120 Hz:  R39\n150 Hz:  R39\n190 Hz:  R39\n240 Hz:  R39\n310 Hz:  R39\n390 Hz:  R39","R11","R11, R41","R58","R58","R1, R15, R16, R24, R25, R35, R48, R58, R59, R60, R61, R62, R63, R64, R65, R71","R29, R30, R31, R32, R49, R52, R53, R54, R55, R56, R61, R64, R67, R77","R21, R22","R2, R3, R6, R7, R10"]
[1,"Resistor","12 kΩ",3,null,"0204/0207","MFR-12FTF52-12K","Mouser","603-MFR-12FTF52-12K",0.11899999999999999,0.35699999999999998,null,null,null,null,"R42","R42","R33"]
[1,"Resistor","15 kΩ",50,100,"0204/0207","MFR-12FTF52-15K","Mouser","603-MFR-12FTF52-15K",2.1000000000000001E-2,2.1,"R47, R48",null,"R22","R22, R52","R35, R43","R35, R43","R11, R12, R18, R44, R45","R1, R2"]
[1,"Resistor","18 kΩ",7,10,"0204/0207","MFR-12FTF52-18K","Mouser","603-MFR-12FTF52-18K",0.06,0.6,null,null,null,null,"R27, R28, R29","R27, R28, R29",null,"R37"]
[1,"Resistor","20 kΩ",36,100,"0204/0207","MFR-12FTF52-20K","Mouser","603-MFR-12FTF52-20K",1.6E-2,1.6,"R55","500 Hz:  R38\n640 Hz:  R38\n810 Hz:  R38\n1030 Hz:  R38\n1310 Hz:  R38\n1660 Hz:  R38\n2110 Hz:  R38\n2680 Hz:  R38\n3410 Hz:  R38\n4330 Hz:  R38\n5500 Hz:  R38\n7000 Hz:  R38",null,null,null,null,"R66, R67","R58, R62, R63, R76"]
[1,"Resistor","22 kΩ",25,10,"0204/0207","MFR-12FTF52-22K","Mouser","603-MFR-12FTF52-22K",0.06,1.5,"R57",null,"R12","R12, R42","R57","R57","R2, R17"]
[1,"Resistor","24 kΩ",36,100,"0204/0207","MFR-12FTF52-24K","Mouser","603-MFR-12FTF52-24K",2.1000000000000001E-2,2.1,"R44","500 Hz:  R37\n640 Hz:  R37\n810 Hz:  R37\n1030 Hz:  R37\n1310 Hz:  R37\n1660 Hz:  R37\n2110 Hz:  R37\n2680 Hz:  R37\n3410 Hz:  R37\n4330 Hz:  R37\n5500 Hz:  R37\n7000 Hz:  R37","R7",null,"R50","R50",null,"R51, R57, R94"]
[1,"Resistor","27 kΩ",10,10,"0204/0207","MFR-12FTF52-27K","Mouser","603-MFR-12FTF52-27K",0.06,0.6,null,"120 Hz:  R38\n150 Hz:  R38\n190 Hz:  R38\n240 Hz:  R38\n310 Hz:  R38\n390 Hz:  R38",null,null,null,null,"R4, R50","R9, R10"]
[1,"Resistor","30 kΩ",1,null,"0204/0207","MFR-12FTF52-30K","Mouser","603-MFR-12FTF52-30K",0.11899999999999999,0.11899999999999999,null,null,null,null,null,null,null,null,"R41"]
[1,"Resistor","33 kΩ",30,10,"0204/0207","MFR-12FTF52-33K","Mouser","603-MFR-12FTF52-33K",0.06,1.7999999999999998,"R25","120 Hz:  R37\n150 Hz:  R37\n190 Hz:  R37\n240 Hz:  R37\n310 Hz:  R37\n390 Hz:  R37","R13","R13, R43","R17","R17",null,null,"R13"]
[1,"Resistor","36 kΩ",4,null,"0204/0207","MFR-12FTF52-36K","Mouser","603-MFR-12FTF52-36K",0.11899999999999999,0.47599999999999998,null,null,null,null,"R30","R30","R31, R32"]
[1,"Resistor","39 kΩ",1,null,"0204/0207","MFR-12FTF52-39K","Mouser","603-MFR-12FTF52-39K",0.11899999999999999,0.11899999999999999,null,null,null,null,null,null,null,"R65"]
[1,"Resistor","47 kΩ",79,100,"0204/0207","MFR-12FTF52-47K","Mouser","603-MFR-12FTF52-47K",2.1000000000000001E-2,2.1,"R35, R45",null,"R1, R5, R6, R8, R9, R31, R35, R36","R1, R5, R6, R7, R8, R9, R31, R35, R36, R37, R38, R39","R19, R47,  R56","R19, R47,  R56","R72, R74","R3, R4, R5, R6, R7, R8, R82","R10, R31, R32, R33, R37, R45, R51, R52"]
[1,"Resistor","56 kΩ",4,null,"0204/0207","MFR-12FTF52-56K","Mouser","603-MFR-12FTF52-56K",0.11899999999999999,0.47599999999999998,null,null,null,null,"R14","R14",null,null,"R12, R17"]
[1,"Resistor","62 kΩ",2,null,"0204/0207","MFR-12FTF52-62K","Mouser","603-MFR-12FTF52-62K",0.11899999999999999,0.23799999999999999,null,null,null,null,"R65","R65"]
[1,"Resistor","75 kΩ",3,null,"0204/0207","MFR-12FTF52-75K","Mouser","603-MFR-12FTF52-75K",0.11899999999999999,0.35699999999999998,null,null,null,null,null,null,null,"R40",null,"R5, R9"]
[1,"Resistor","91 kΩ",2,null,"0204/0207","MFR-12FTF52-91K","Mouser","603-MFR-12FTF52-91K",0.11899999999999999,0.23799999999999999,null,null,null,null,null,null,null,null,"R16, R27"]
[1,"Resistor","100 kΩ",137,100,"0204/0207","MFR-12FTF52-100K","Mouser","603-MFR-12FTF52-100K",2.1000000000000001E-2,2.8770000000000002,"R56, R66",null,"R10, R14, R15, R16, R17","R10, R14, R15, R16, R17, R25, R26, R40, R44, R45, R46, R47","R1, R2, R5, R16, R18, R21, R22, R23, R55, R61, R62, R63, R64, R80","R1, R2, R5, R16, R18, R21, R22, R23, R55, R61, R62, R63, R64, R80","R6, R7, R8, R9, R10, R20, R26, R27, R28, R29, R30, R38, R39, R40, R41, R42, R43, R52, R53, R68, R69, R70","R11, R12, R13, R14, R15, R16, R23, R24, R25, R26, R27, R35, R36, R38, R41, R42, R66, R68, R69, R70, R79, R80","R1, R2, R3, R8, R19, R26, R28, R29, R30, R36, R44, R48"]
[1,"Resistor","120 kΩ",1,null,"0204/0207","MFR-12FTF52-120K","Mouser","603-MFR-12FTF52-120K",0.11899999999999999,0.11899999999999999,null,null,null,null,null,null,null,null,"R18"]
[1,"Resistor","150 kΩ",7,10,"0204/0207","MFR-12FTF52-150K","Mouser","603-MFR-12FTF52-150K",0.06,0.6,null,null,null,null,"R4, R20, R31","R4, R20, R31",null,null,"R14"]
[1,"Resistor","180 kΩ",2,null,"0204/0207","MFR-12FTF52-180K","Mouser","603-MFR-12FTF52-180K",0.11899999999999999,0.23799999999999999,null,null,null,null,null,null,null,"R19, R20"]
[1,"Resistor","200 kΩ",13,10,"0204/0207","MFR-12FTF52-200K","Mouser","603-MFR-12FTF52-200K",0.06,{"$f":"IF(D85>=E85,D85*J85,E85*J85)","v":0.78},null,null,"R4, R18, R19, R34","R4, R18, R19, R34, R48, R49",null,null,null,"R17, R18","R4"]
[1,"Resistor","220 kΩ",12,10,"0204/0207","MFR-12FTF52-220K","Mouser","603-MFR-12FTF52-220K",0.06,0.72,null,null,null,null,"R12, R32, R54","R12, R32, R54, R66, R67, R68",null,"R74","R6, R47"]
[1,"Resistor","330 kΩ",3,null,"0204/0207","MFR-12FTF52-330K","Mouser","603-MFR-12FTF52-330K",0.11899999999999999,0.35699999999999998,null,null,null,null,"R15","R15","R51"]
[1,"Resistor","390 kΩ",2,null,"0204/0207","MFR-12FTF52-390K","Mouser","603-MFR-12FTF52-390K",0.11899999999999999,0.23799999999999999,null,null,null,null,"R13","R13"]
[1,"Resistor","470 kΩ",3,null,"0204/0207","MFR-12FTF52-470K","Mouser","603-MFR-12FTF52-470K",0.11899999999999999,0.35699999999999998,null,null,null,null,"R53","R53",null,null,"R24"]
[1,"Resistor","820 kΩ",2,null,"0204/0207","MFR-12FTF52-820K","Mouser","603-MFR-12FTF52-820K",0.11899999999999999,0.23799999999999999,null,null,null,null,"R24","R24"]
[1,"Resistor","1 MΩ",35,100,"0204/0207","MFR-12FTF52-1M","Mouser","603-MFR-12FTF52-1M",2.1000000000000001E-2,2.1,null,null,"R2, R32","R2, R32","R25, R26, R38, R39, R45, R48, R49, R51, R52","R25, R26, R38, R39, R45, R48, R49, R51, R52","R54, R55, R56, R57","R43, R44, R71, R72, R78, R83","R5, R7, R11"]
[1,"Resistor","1.5 MΩ",4,null,"0204/0207","MFR-12FTF52-1M5","Mouser","603-MFR-12FTF52-1M5",0.17899999999999999,0.71599999999999997,null,null,null,null,"R10, R79","R10, R79"]
[1,"Resistor","2.2 MΩ, 5%",2,null,"0204/0207","MFR-12FTF52-2M2","Mouser","603-MFR-12FTF52-2M2",0.17899999999999999,0.35799999999999998,null,null,null,null,null,null,"R37",null,"R40"]
[1,"Resistor","3.3 MΩ, 5%",1,null,"0204/0207","MFR-12FTF52-3M3","Mouser","603-MFR-12FTF52-3M3",0.17899999999999999,0.17899999999999999,null,null,null,null,null,null,null,null,"R35"]
[1,"Resistor","4.7 MΩ, 5%",18,10,"0204/0207","MFR-12FTF52-4M7","Mouser","603-MFR-12FTF52-4M7",0.111,1.998,"R36"]
[1,"Resistor","6.8 MΩ",2,null,"0204/0207","MFR-12FTF52-6M8","Mouser","603-MFR-12FTF52-6M8",0.13600000000000001,0.27200000000000002,null,null,null,null,"R3","R3"]
[1,"Resistor-F","196 Ω",2,null,"0204/0207","MFR-25FBF52-196R","Mouser","603-MFR-25FBF52-196R",0.10199999999999999,0.20399999999999999,null,"7000 Hz:  R10, R22"]
[1,"Resistor-F","237 Ω",2,null,"0204/0207","MFR-25FBF52-237R","Mouser","603-MFR-25FBF52-237R",0.10199999999999999,0.20399999999999999,null,"7000 Hz:  R7, R19"]
[1,"Resistor-F","249 Ω",4,null,"0204/0207","MFR-25FBF52-249R","Mouser","603-MFR-25FBF52-249R",0.10199999999999999,0.40799999999999997,null,"1660 Hz:  R10, R22\n5500 Hz:  R10, R22"]
[1,"Resistor-F","287 Ω",2,null,"0204/0207","MFR-25FBF52-287R","Mouser","603-MFR-25FBF52-287R",0.10199999999999999,0.20399999999999999,null,"7000 Hz:  R4, R16"]
[1,"Resistor-F","301 Ω",6,10,"0204/0207","MFR-25FBF52-301R","Mouser","603-MFR-25FBF52-301R",5.3999999999999999E-2,0.54,null,"1660 Hz:  R7, R19\n5500 Hz:  R7, R19\n7000 Hz:  R1, R13"]
[1,"Resistor-F","316 Ω",4,null,"0204/0207","MFR-25FBF52-316R","Mouser","603-MFR-25FBF52-316R",0.10199999999999999,0.40799999999999997,null,"1310 Hz:  R10, R22\n4330 Hz:  R10, R22"]
[1,"Resistor-F","348 Ω",2,null,"0204/0207","MFR-25FBF52-348R","Mouser","603-MFR-25FBF52-348R",0.10199999999999999,0.20399999999999999,null,"390 Hz:  R10, R22"]
[1,"Resistor-F","365 Ω",4,null,"0204/0207","MFR-25FBF52-365R","Mouser","603-MFR-25FBF52-365R",0.10199999999999999,0.40799999999999997,null,"1660 Hz:  R4, R16\n5500 Hz:  R4, R16"]
[1,"Resistor-F","383 Ω",8,10,"0204/0207","MFR-25FBF52-383R","Mouser","603-MFR-25FBF52-383R",5.3999999999999999E-2,0.54,null,"1310 Hz:  R7, R19\n1660 Hz:  R1, R13\n4330 Hz:  R7, R19\n5500 Hz:  R1, R13"]
[1,"Resistor-F","402 Ω",4,null,"0204/0207","MFR-25FBF52-402R","Mouser","603-MFR-25FBF52-402R",0.10199999999999999,0.40799999999999997,null,"1030 Hz:  R10, R22\n3410 Hz:  R10, R22"]
[1,"Resistor-F","422 Ω",2,null,"0204/0207","MFR-25FBF52-422R","Mouser","603-MFR-25FBF52-422R",0.10199999999999999,0.20399999999999999,null,"390 Hz:  R7, R19"]
[1,"Resistor-F","442 Ω",2,null,"0204/0207","MFR-25FBF52-442R","Mouser","603-MFR-25FBF52-442R",0.10199999999999999,0.20399999999999999,null,"310 Hz:  R10, R22"]
[1,"Resistor-F","464 Ω",4,null,"0204/0207","MFR-25FBF52-464R","Mouser","603-MFR-25FBF52-464R",0.10199999999999999,0.40799999999999997,null,"1310 Hz:  R4, R16\n4330 Hz:  R4, R16"]
[1,"Resistor-F","487 Ω",8,10,"0204/0207","MFR-25FBF52-487R","Mouser","603-MFR-25FBF52-487R",5.3999999999999999E-2,0.54,null,"1030 Hz:  R7, R19\n1310 Hz:  R1, R13\n3410 Hz:  R7, R19\n4330 Hz:  R1, R13"]
[1,"Resistor-F","511 Ω",6,10,"0204/0207","MFR-25FBF52-511R","Mouser","603-MFR-25FBF52-511R",5.3999999999999999E-2,0.54,null,"390 Hz:  R4, R16\n810 Hz:  R10, R22\n2680 Hz:  R10, R22"]
[1,"Resistor-F","536 Ω",4,null,"0204/0207","MFR-25FBF52-536R","Mouser","603-MFR-25FBF52-536R",0.10199999999999999,0.40799999999999997,null,"310 Hz:  R7, R19\n390 Hz:  R1, R13"]
[1,"Resistor-F","562 Ω",2,null,"0204/0207","MFR-25FBF52-562R","Mouser","603-MFR-25FBF52-562R",0.10199999999999999,0.20399999999999999,null,"240 Hz:  R10, R22"]
[1,"Resistor-F","590 Ω",4,null,"0204/0207","MFR-25FBF52-590R","Mouser","603-MFR-25FBF52-590R",0.10199999999999999,0.40799999999999997,null,"1030 Hz:  R4, R16\n3410 Hz:  R4, R16"]
[1,"Resistor-F","619 Ω",8,10,"0204/0207","MFR-25FBF52-619R","Mouser","603-MFR-25FBF52-619R",5.3999999999999999E-2,0.54,null,"810 Hz:  R7, R19\n1030 Hz:  R1, R13\n2680 Hz:  R7, R19\n3410 Hz:  R1, R13"]
[1,"Resistor-F","649 Ω",6,10,"0204/0207","MFR-25FBF52-649R","Mouser","603-MFR-25FBF52-649R",5.3999999999999999E-2,0.54,null,"310 Hz:  R4, R16\n640 Hz:  R10, R22\n2110 Hz:  R10, R22"]
[1,"Resistor-F","681 Ω",4,null,"0204/0207","MFR-25FBF52-681R","Mouser","603-MFR-25FBF52-681R",0.10199999999999999,0.40799999999999997,null,"240 Hz:  R7, R19\n310 Hz:  R1, R13"]
[1,"Resistor-F","715 Ω",2,null,"0204/0207","MFR-25FBF52-715R","Mouser","603-MFR-25FBF52-715R",0.10199999999999999,0.20399999999999999,null,"190 Hz:  R10, R22"]
[1,"Resistor-F","750 Ω",4,null,"0204/0207","MFR-25FBF52-750R","Mouser","603-MFR-25FBF52-750R",0.10199999999999999,0.40799999999999997,null,"810 Hz:  R4, R16\n2680 Hz:  R4, R16"]
[1,"Resistor-F","787 Ω",8,10,"0204/0207","MFR-25FRF52-787R","Mouser","603-MFR-25FRF52-787R",5.3999999999999999E-2,0.54,null,"640 Hz:  R7, R19\n810 Hz:  R1, R13\n2110 Hz:  R7, R19\n2680 Hz:  R1, R13"]
[1,"Resistor-F","825 Ω",4,null,"0204/0207","MFR-25FBF52-825R","Mouser","603-MFR-25FBF52-825R",0.10199999999999999,0.40799999999999997,null,"240 Hz:  R4, R16\n500 Hz:  R10, R22"]
[1,"Resistor-F","866 Ω",4,null,"0204/0207","MFR-25FBF52-866R","Mouser","603-MFR-25FBF52-866R",0.10199999999999999,0.40799999999999997,null,"190 Hz:  R7, R19\n240 Hz:  R1, R13"]
[1,"Resistor-F","909 Ω",2,null,"0204/0207","MFR-25FBF52-909R","Mouser","603-MFR-25FBF52-909R",0.10199999999999999,0.20399999999999999,null,"150 Hz:  R10, R22"]
[1,"Resistor-F","953 Ω",4,null,"0204/0207","MFR-25FBF52-953R","Mouser","603-MFR-25FBF52-953R",0.10199999999999999,0.40799999999999997,null,"640 Hz:  R4, R16\n2110 Hz:  R4, R16"]
[1,"Resistor-F","1 kΩ",6,10,"0204/0207","MFR-25FBF52-1K","Mouser","603-MFR-25FBF52-1K",5.3999999999999999E-2,0.54,null,"500 Hz:  R7, R19\n640 Hz:  R1, R13\n2110 Hz:  R1, R13"]
[1,"Resistor-F","1.05 kΩ",2,null,"0204/0207","MFR-25FBF52-1K05","Mouser","603-MFR-25FBF52-1K05",0.10199999999999999,0.20399999999999999,null,"190 Hz:  R4, R16"]
[1,"Resistor-F","1.1 kΩ",4,null,"0204/0207","MFR-25FBF52-1K1","Mouser","603-MFR-25FBF52-1K1",0.10199999999999999,0.40799999999999997,null,"150 Hz:  R7, R19\n190 Hz:  R1, R13"]
[1,"Resistor-F","1.15 kΩ",2,null,"0204/0207","MFR-25FBF52-1K15","Mouser","603-MFR-25FBF52-1K15",0.10199999999999999,0.20399999999999999,null,"120 Hz:  R10, R22"]
[1,"Resistor-F","1.21 kΩ",2,null,"0204/0207","MFR-25FBF52-1K21","Mouser","603-MFR-25FBF52-1K21",0.10199999999999999,0.20399999999999999,null,"500 Hz:  R4, R16"]
[1,"Resistor-F","1.27 kΩ",2,null,"0204/0207","MFR-25FBF52-1K27","Mouser","603-MFR-25FBF52-1K27",0.10199999999999999,0.20399999999999999,null,"500 Hz:  R1, R13"]
[1,"Resistor-F","1.33 kΩ",2,null,"0204/0207","MFR-25FBF52-1K33","Mouser","603-MFR-25FBF52-1K33",0.10199999999999999,0.20399999999999999,null,"150 Hz:  R4, R16"]
[1,"Resistor-F","1.4 kΩ",4,null,"0204/0207","MFR-25FBF52-1K4","Mouser","603-MFR-25FBF52-1K4",0.10199999999999999,0.40799999999999997,null,"120 Hz:  R7, R19\n150 Hz:  R1, R13"]
[1,"Resistor-F","1.69 kΩ",2,null,"0204/0207","MFR-25FBF52-1K69","Mouser","603-MFR-25FBF52-1K69",0.10199999999999999,0.20399999999999999,null,"120 Hz:  R4, R16"]
[1,"Resistor-F","1.78 kΩ",2,null,"0204/0207","MFR-25FBF52-1K78","Mouser","603-MFR-25FBF52-1K78",0.10199999999999999,0.20399999999999999,null,"120 Hz:  R1, R13"]
[1,"Resistor-F","6.81 kΩ",2,null,"0204/0207","MFR-25FBF52-6K81","Mouser","603-MFR-25FBF52-6K81",0.10199999999999999,0.20399999999999999,null,"7000 Hz:  R11, R23"]
[1,"Resistor-F","8.66 kΩ",8,10,"0204/0207","MFR-25FBF52-8K66","Mouser","603-MFR-25FBF52-8K66",5.3999999999999999E-2,0.54,null,"1660 Hz:  R11, R23\n5500 Hz:  R11, R23\n7000 Hz:  R5, R17\n7000 Hz:  R8, R20"]
[1,"Resistor-F","9.09 kΩ",2,null,"0204/0207","MFR-25FBF52-9K09","Mouser","603-MFR-25FBF52-9K09",0.10199999999999999,0.20399999999999999,null,"7000 Hz:  R2, R14"]
[1,"Resistor-F","11 kΩ",12,10,"0204/0207","MFR-25FBF52-11K","Mouser","603-MFR-25FBF52-11K",5.3999999999999999E-2,0.64800000000000002,null,"1310 Hz:  R11, R23\n1660 Hz:  R5, R17\n1660 Hz:  R8, R20\n4330 Hz:  R11, R23\n5500 Hz:  R5, R17\n5500 Hz:  R8, R20"]
[1,"Resistor-F","11.5 kΩ",4,null,"0204/0207","MFR-25FBF52-11K5","Mouser","603-MFR-25FBF52-11K5",0.10199999999999999,0.40799999999999997,null,"1660 Hz:  R2, R14\n5500 Hz:  R2, R14"]
[1,"Resistor-F","12.1 kΩ",2,null,"0204/0207","MFR-25FBF52-12K1","Mouser","603-MFR-25FBF52-12K1",0.10199999999999999,0.20399999999999999,null,"390 Hz:  R11, R23"]
[1,"Resistor-F","14 kΩ",12,10,"0204/0207","MFR-25FBF52-14K","Mouser","603-MFR-25FBF52-14K",5.3999999999999999E-2,0.64800000000000002,null,"1030 Hz:  R11, R23\n1310 Hz:  R5, R17\n1310 Hz:  R8, R20\n3410 Hz:  R11, R23\n4330 Hz:  R5, R17\n4330 Hz:  R8, R20"]
[1,"Resistor-F","14.7 kΩ",4,null,"0204/0207","MFR-25FBF52-14K7","Mouser","603-MFR-25FBF52-14K7",0.10199999999999999,0.40799999999999997,null,"1310 Hz:  R2, R14\n4330 Hz:  R2, R14"]
[1,"Resistor-F","15.4 kΩ",6,10,"0204/0207","MFR-25FBF52-15K4","Mouser","603-MFR-25FBF52-15K4",5.3999999999999999E-2,0.54,null,"310 Hz:  R11, R23\n390 Hz:  R5, R17\n390 Hz:  R8, R20"]
[1,"Resistor-F","16.2 kΩ",2,null,"0204/0207","MFR-25FBF52-16K2","Mouser","603-MFR-25FBF52-16K2",0.10199999999999999,0.20399999999999999,null,"390 Hz:  R2, R14"]
[1,"Resistor-F","17.8 kΩ",14,10,"0204/0207","MFR-25FBF52-17K8","Mouser","603-MFR-25FBF52-17K8",5.3999999999999999E-2,0.75600000000000001,null,"810 Hz:  R11, R23\n1030 Hz:  R5, R17\n1030 Hz:  R8, R20\n2680 Hz:  R11, R23\n3410 Hz:  R5, R17\n3410 Hz:  R8, R20\n7000 Hz:  R6, R18"]
[1,"Resistor-F","18.7 kΩ",6,10,"0204/0207","MFR-25FBF52-18K7","Mouser","603-MFR-25FBF52-18K7",5.3999999999999999E-2,0.54,null,"1030 Hz:  R2, R14\n3410 Hz:  R2, R14\n7000 Hz:  R3, R15"]
[1,"Resistor-F","19.6 kΩ",6,10,"0204/0207","MFR-25FBF52-19K6","Mouser","603-MFR-25FBF52-19K6",5.3999999999999999E-2,0.54,null,"240 Hz:  R11, R23\n310 Hz:  R5, R17\n310 Hz:  R8, R20"]
[1,"Resistor-F","20.5 kΩ",2,null,"0204/0207","MFR-25FBF52-20K5","Mouser","603-MFR-25FBF52-20K5",0.10199999999999999,0.20399999999999999,null,"310 Hz:  R2, R14"]
[1,"Resistor-F","22.6 kΩ",18,10,"0204/0207","MFR-25FBF52-22K6","Mouser","603-MFR-25FBF52-22K6",5.3999999999999999E-2,{"$f":"IF(D149>=E149,D149*J149,E149*J149)","v":0.97199999999999998},null,"640 Hz:  R11, R23\n810 Hz:  R5, R17\n810 Hz:  R8, R20\n1660 Hz:  R6, R18\n2110 Hz:  R11, R23\n2680 Hz:  R5, R17\n2680 Hz:  R8, R20\n5500 Hz:  R6, R18\n7000 Hz:  R12, R24"]
[1,"Resistor-F","23.7 kΩ",8,10,"0204/0207","MFR-25FBF52-23K7","Mouser","603-MFR-25FBF52-23K7",5.3999999999999999E-2,0.54,null,"810 Hz:  R2, R14\n1660 Hz:  R3, R15\n2680 Hz:  R2, R14\n5500 Hz:  R3, R15"]
[1,"Resistor-F","24.9 kΩ",6,10,"0204/0207","MFR-25FBF52-24K9","Mouser","603-MFR-25FBF52-24K9",5.3999999999999999E-2,0.54,null,"190 Hz:  R11, R23\n240 Hz:  R5, R17\n240 Hz:  R8, R20"]
[1,"Resistor-F","26.1 kΩ",2,null,"0204/0207","MFR-25FBF52-26K1","Mouser","603-MFR-25FBF52-26K1",0.10199999999999999,0.20399999999999999,null,"240 Hz:  R2, R14"]
[1,"Resistor-F","28.7 kΩ",20,10,"0204/0207","MFR-25FBF52-28K7","Mouser","603-MFR-25FBF52-28K7",5.3999999999999999E-2,1.08,null,"500 Hz:  R11, R23\n640 Hz:  R5, R17\n640 Hz:  R8, R20\n1310 Hz:  R6, R18\n1660 Hz:  R12, R24\n2110 Hz:  R5, R17\n2110 Hz:  R8, R20\n4330 Hz:  R6, R18\n5500 Hz:  R12, R24\n7000 Hz:  R9, R21"]
[1,"Resistor-F","30.1 kΩ",8,10,"0204/0207","MFR-25FBF52-30K1","Mouser","603-MFR-25FBF52-30K1",5.3999999999999999E-2,0.54,null,"640 Hz:  R2, R14\n1310 Hz:  R3, R15\n2110 Hz:  R2, R14\n4330 Hz:  R3, R15"]
[1,"Resistor-F","31.6 kΩ",8,10,"0204/0207","MFR-25FBF52-31K6","Mouser","603-MFR-25FBF52-31K6",5.3999999999999999E-2,0.54,null,"150 Hz:  R11, R23\n190 Hz:  R5, R17\n190 Hz:  R8, R20\n390 Hz:  R6, R18"]
[1,"Resistor-F","33.2 kΩ",4,null,"0204/0207","MFR-25FBF52-33K2","Mouser","603-MFR-25FBF52-33K2",0.10199999999999999,0.40799999999999997,null,"190 Hz:  R2, R14\n390 Hz:  R3, R15"]
[1,"Resistor-F","36.5 kΩ",16,10,"0204/0207","MFR-25FBF52-36K5","Mouser","603-MFR-25FBF52-36K5",5.3999999999999999E-2,0.86399999999999999,null,"500 Hz:  R5, R17\n500 Hz:  R8, R20\n1030 Hz:  R6, R18\n1310 Hz:  R12, R24\n1660 Hz:  R9, R21\n3410 Hz:  R6, R18\n4330 Hz:  R12, R24\n5500 Hz:  R9, R21"]
[1,"Resistor-F","38.3 kΩ",6,10,"0204/0207","MFR-25FBF52-38K3","Mouser","603-MFR-25FBF52-38K3",5.3999999999999999E-2,0.54,null,"500 Hz:  R2, R14\n1030 Hz:  R3, R15\n3410 Hz:  R3, R15"]
[1,"Resistor-F","40.2 kΩ",10,10,"0204/0207","MFR-25FBF52-40K2","Mouser","603-MFR-25FBF52-40K2",5.3999999999999999E-2,0.54,null,"120 Hz:  R11, R23\n150 Hz:  R5, R17\n150 Hz:  R8, R20\n310 Hz:  R6, R18\n390 Hz:  R12, R24"]
[1,"Resistor-F","42.2 kΩ",4,null,"0204/0207","MFR-25FBF52-42K2","Mouser","603-MFR-25FBF52-42K2",0.10199999999999999,0.40799999999999997,null,"150 Hz:  R2, R14\n310 Hz:  R3, R15"]
[1,"Resistor-F","46.4 kΩ",12,10,"0204/0207","MFR-25FBF52-46K4","Mouser","603-MFR-25FBF52-46K4",5.3999999999999999E-2,0.64800000000000002,null,"810 Hz:  R6, R18\n1030 Hz:  R12, R24\n1310 Hz:  R9, R21\n2680 Hz:  R6, R18\n3410 Hz:  R12, R24\n4330 Hz:  R9, R21"]
[1,"Resistor-F","48.7 kΩ",4,null,"0204/0207","MFR-25FBF52-48K7","Mouser","603-MFR-25FBF52-48K7",0.10199999999999999,0.40799999999999997,null,"810 Hz:  R3, R15\n2680 Hz:  R3, R15"]
[1,"Resistor-F","51.1 kΩ",10,10,"0204/0207","MFR-25FBF52-51K1","Mouser","603-MFR-25FBF52-51K1",5.3999999999999999E-2,0.54,null,"120 Hz:  R5, R17\n120 Hz:  R8, R20\n240 Hz:  R6, R18\n310 Hz:  R12, R24\n390 Hz:  R9, R21"]
[1,"Resistor-F","53.6 kΩ",4,null,"0204/0207","MFR-25FTE52-53K6","Mouser","603-MFR-25FTE52-53K6",0.10199999999999999,0.40799999999999997,null,"120 Hz:  R2, R14\n240 Hz:  R3, R15"]
[1,"Resistor-F","59 kΩ",12,10,"0204/0207","MFR-25FBF52-59K","Mouser","603-MFR-25FBF52-59K",5.3999999999999999E-2,0.64800000000000002,null,"640 Hz:  R6, R18\n810 Hz:  R12, R24\n1030 Hz:  R9, R21\n2110 Hz:  R6, R18\n2680 Hz:  R12, R24\n3410 Hz:  R9, R21"]
[1,"Resistor-F","61.9 kΩ",4,null,"0204/0207","MFR-25FBF52-61K9","Mouser","603-MFR-25FBF52-61K9",0.10199999999999999,0.40799999999999997,null,"640 Hz:  R3, R15\n2110 Hz:  R3, R15"]
[1,"Resistor-F","64.9 kΩ",6,10,"0204/0207","MFR-25FBF52-64K9","Mouser","603-MFR-25FBF52-64K9",5.3999999999999999E-2,0.54,null,"190 Hz:  R6, R18\n240 Hz:  R12, R24\n310 Hz:  R9, R21"]
[1,"Resistor-F","68.1 kΩ",2,null,"0204/0207","MFR-25FBF52-68K1","Mouser","603-MFR-25FBF52-68K1",0.10199999999999999,0.20399999999999999,null,"190 Hz:  R3, R15"]
[1,"Resistor-F","75 kΩ",10,10,"0204/0207","MFR-25FBF52-75K","Mouser","603-MFR-25FBF52-75K",5.3999999999999999E-2,0.54,null,"500 Hz:  R6, R18\n640 Hz:  R12, R24\n810 Hz:  R9, R21\n2110 Hz:  R12, R24\n2680 Hz:  R9, R21"]
[1,"Resistor-F","78.7 kΩ",2,null,"0204/0207","MFR-25FRF52-78K7","Mouser","603-MFR-25FRF52-78K7",0.10199999999999999,0.20399999999999999,null,"500 Hz:  R3, R15"]
[1,"Resistor-F","82.5 kΩ",6,10,"0204/0207","MFR-25FBF52-82K5","Mouser","603-MFR-25FBF52-82K5",5.3999999999999999E-2,0.54,null,"150 Hz:  R6, R18\n190 Hz:  R12, R24\n240 Hz:  R9, R21"]
[1,"Resistor-F","86.6 kΩ",2,null,"0204/0207","MFR-25FBF52-86K6","Mouser","603-MFR-25FBF52-86K6",0.10199999999999999,0.20399999999999999,null,"150 Hz:  R3, R15"]
[1,"Resistor-F","95.3 kΩ",6,10,"0204/0207","MFR-25FBF52-95K3","Mouser","603-MFR-25FBF52-95K3",5.3999999999999999E-2,0.54,null,"500 Hz:  R12, R24\n640 Hz:  R9, R21\n2110 Hz:  R9, R21"]
[1,"Resistor-F","105 kΩ",6,10,"0204/0207","MFR-25FBF52-105K","Mouser","603-MFR-25FBF52-105K",5.3999999999999999E-2,0.54,null,"120 Hz:  R6, R18\n150 Hz:  R12, R24\n190 Hz:  R9, R21"]
[1,"Resistor-F","110 kΩ",2,null,"0204/0207","MFR-25FBF52-110K","Mouser","603-MFR-25FBF52-110K",0.10199999999999999,0.20399999999999999,null,"120 Hz:  R3, R15"]
[1,"Resistor-F","121 kΩ",2,null,"0204/0207","MFR-25FBF52-121K","Mouser","603-MFR-25FBF52-121K",0.10199999999999999,0.20399999999999999,null,"500 Hz:  R9, R21"]
[1,"Resistor-F","133 kΩ",4,null,"0204/0207","MFR-25FBF52-133K","Mouser","603-MFR-25FBF52-133K",0.10199999999999999,0.40799999999999997,null,"120 Hz:  R12, R24\n150 Hz:  R9, R21"]
[1,"Resistor-F","169 kΩ",2,null,"0204/0207","MFR-25FBF52-169K","Mouser","603-MFR-25FBF52-169K",0.10199999999999999,0.20399999999999999,null,"120 Hz:  R9, R21"]
[4,"Tempco","2 kΩ, 3300 ppm/°C",3,null,null,null,"Thonk","tempco",1.61,4.83,null,null,null,null,"R7","R7",null,null,"R20"]
[1,"Ceramic","22 pF",17,10,"RM2.5","K220J15C0GF53L2","Mouser","594-K220J15C0GF53L2",0.27100000000000002,4.6070000000000002,null,null,"C5, C6","C5, C6, C15, C16","C9","C9",null,"C1, C2, C3, C4, C5, C6, C11, C12, C14"]
[1,"Ceramic","100 pF",9,10,"RM2.5","K101J15C0GF53L2","Mouser","594-K101J15C0GF53L2",8.6999999999999994E-2,0.86999999999999988,null,null,null,null,"C1, C6, C17","C1, C6, C17","C26, C27","C19"]
[1,"Ceramic","220 pF",2,null,"RM2.5/RM5.0","C315C221M5R5TA","Mouser","80-C315C221M5R",0.27900000000000003,0.55800000000000005,null,null,null,null,"C16","C16"]
[1,"Ceramic","470 pF",2,10,"RM2.5/RM5.0","K471J15C0GF53L2","Mouser","594-K471J15C0GF53L2",0.105,1.05,null,null,null,null,"C15","C15"]
[2,"Ceramic","1 nF, 2 kV",2,null,"SMD 1808","C1808C102MGRACAUTO","Mouser","80-C1808C102MGRAUTO",1.51,3.02,null,null,null,null,null,null,null,null,null,"C2, C3"]
[1,"Ceramic","1 nF",3,5,"RM2.5","R82EC1100AA50K","Mouser","80-R82EC1100AA50K",0.21,1.05,null,null,null,null,null,null,null,"C26, C27, C29"]
[1,"Ceramic","1.5 nF",4,null,"RM2.5","C315C152K1R5TA","Mouser","80-C315C152K1R",0.30599999999999999,1.224,null,null,null,null,null,null,"C22, C23, C24, C25"]
[1,"Ceramic","10 nF",96,100,"SMD (1206 or 0805)","08055A103JAT2A","Mouser","581-08055A103JAT2A",0.224,22.400000000000002,null,"2110 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n2680 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n3410 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n4330 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n5500 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n7000 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16"]
[1,"Ceramic","10 nF",2,10,"RM2.5","K103K15X7RF53L2","Mouser","594-K103K15X7RF53L2",0.314,3.14,null,null,null,"C19",null,"C18"]
[1,"Ceramic","33 nF",96,100,"SMD (1206 or 0805)","CGA5F2C0G1H333J085AA","Mouser","810-CGA5F2C0G1H333J",0.16,16,null,"500 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n640 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n810 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n1030 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n1310 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n1660 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16"]
[1,"Ceramic","100 nF",415,500,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,12,"C18, C19, C20, C21, C23, C24, C25, C26, C27, C28, C29, C30, C31, C32, C33, C34",null,"C22, C23, C24, C25, C26, C27, C28, C29, C30","C22, C23, C24, C25, C26, C27, C28, C29, C30, C34, C35, C36, C37, C38, C39, C40","C2, C22, C23, C26, C27, C28, C29, C32, C33, C34, C35, C38, C39, C42, C43","C2, C22, C23, C26, C27, C28, C29, C32, C33, C34, C35, C38, C39, C42, C43","C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16, C17, C18, C19, C20, C21, C30, C31, C34, C35, C38, C39, C40, C41, C42, C43, C44, C45, C47, C48","C20, C25, C31, C32, C33, C34, C35, C36, C37, C38, C39, C40, C41, C42, C46, C48, C49, C51, C54, C55, C56, C57, C58, C59, C60, C63, C64","C8, C9, C11, C12, C15, C16, C19, C20, C21, C22, C25","C8, C9"]
[1,"Ceramic","100 nF",96,100,"SMD (1206 or 0805)","GRM31C5C1H104JA01L","Mouser","81-GRM31C5C1H104JA1L",0.32700000000000001,32.700000000000003,null,"120 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n150 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n190 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n240 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n310 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16\n390 Hz:  C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16"]
[2,"Ceramic","10 µF, 25 V",5,null,"SMD 1812","C4532X7R1E106M250KA","Mouser","810-C4532X7R1E106M",1.18,5.8999999999999995,null,null,null,null,null,null,null,null,null,"C1, C4, C5, C6, C7"]
[1,"Film","1 nF",3,5,"RM2.5/RM5.0","R82EC1100AA50K","Mouser","80-R82EC1100AA50K",0.21,1.05,null,null,null,null,"C14","C14",null,null,"C6"]
[1,"Film","2.2 nF",2,5,"RM2.5/RM5.0","R82EC1220DQ50J","Mouser","80-R82EC1220DQ50J",0.26200000000000001,1.31,null,null,null,null,"C13","C13"]
[1,"Film","4.7 nF",3,5,"RM2.5/RM5.0","R82EC1470CK50J","Mouser","80-R82EC1470CK50J",0.253,1.2650000000000001,null,null,null,null,"C12","C12",null,null,"C7"]
[1,"Film","10 nF",8,5,"RM2.5/RM5.0","R82EC2100AA50J","Mouser","80-R82EC2100AA50J",0.218,1.744,null,null,null,null,"C11","C11","C1, C2, C3","C13, C30","C5"]
[1,"Film","22 nF",2,5,"RM2.5/RM5.0","R82EC2220AA50J","Mouser","80-R82EC2220AA50J",0.218,1.0900000000000001,null,null,null,null,"C10","C10"]
[1,"Film","47 nF",2,5,"RM2.5/RM5.0","R82EC2470AA60J","Mouser","80-R82EC2470AA60J",0.218,1.0900000000000001,null,null,null,null,"C5","C5"]
[1,"Film","100 nF",11,5,"RM2.5/RM5.0","R82EC3100AA70J","Mouser","80-R82EC3100AA70J",0.14099999999999999,1.5509999999999999,null,null,"C1, C11","C1, C11","C3, C8","C3, C8",null,null,"C3, C4, C10"]
[1,"Film","220 nF",44,50,"RM2.5/RM5.0","R82DC3220Z360K","Mouser","80-82DC3220Z360K",0.10299999999999999,5.1499999999999995,"C17, C22",null,"C7","C7, C17",null,null,null,"C22, C23, C24, C28","C1"]
[1,"Film","330 nF",2,5,"RM2.5/RM5.0","R82DC3330AA60K","Mouser","80-R82DC3330AA60K",0.26200000000000001,1.31,null,null,null,null,null,null,null,"C52, C53"]
[1,"Film","1 µF",11,10,"RM2.5/RM5.0","R82DC4100Z360K","Mouser","80-R82DC4100Z360K",0.27900000000000003,3.0690000000000004,null,null,"C3, C4, C13, C14","C3, C4, C13, C14","C4","C4",null,"C21"]
[1,"Electrolytic","2.2 µF/25 V, max. ⌀ 5 mm",3,3,"RM2.0","Würth 860020672006","Mouser","710-860020672006",0.1,0.30000000000000004,null,null,null,null,"C7","C7",null,null,"C2"]
[1,"Electrolytic","3.3 µF/50 V, max. ⌀ 5 mm",3,3,"RM2.0","Würth 860020672007","Mouser","710-860020672007",0.1,0.30000000000000004,null,null,"C8","C8, C18"]
[1,"Electrolytic","10 µF/50 V, max. ⌀ 5 mm",4,5,"RM2.0","Würth 860020672010","Mouser","710-860020672010",0.1,0.5,null,null,"C2, C12","C2, C12"]
[1,"Electrolytic","22 µF/25 V, max. ⌀ 5 mm",17,10,"RM2.0","Würth 860010572003","Mouser","710-860010572003",8.8999999999999996E-2,1.5129999999999999,null,null,null,null,null,null,"C46","C7, C8, C9, C10, C15, C16, C17, C18, C47","C13, C14, C17, C18, C23, C24, C26"]
[1,"Electrolytic","47 µF/35 V, max. ⌀ 5 mm",135,100,"RM2.0","Würth 860010572005","Mouser","710-860010572005",7.0999999999999994E-2,9.5849999999999991,"C35, C36, C37, C38, C39, C40",null,null,null,"C20, C21, C24, C25, C30, C31, C36, C37, C40, C41","C20, C21, C24, C25, C30, C31, C36, C37, C40, C41","C28, C29, C32, C33","C45, C61, C62"]
[1,"Electrolytic","100 µF/25 V, max. ⌀ 7 mm",13,10,"RM2.5","Würth 860010473007","Mouser","710-860010473007",0.111,1.4430000000000001,null,null,"C20, C21, C31, C32","C20, C21, C31, C32",null,null,"C36, C37","C43, C44, C50"]
[4,"Potentiometer","100 kΩ lin, Alpha 9 mm, right angled (side adjust)",5,null,null,"RD901F-20-15R1-B100K","Small Bear (US) or Thonk (EU)","100k-lin-single",1.38,6.8999999999999995,null,null,null,null,"P1, P2","P1, P2",null,null,"P1"]
[4,"Potentiometer","100 kΩ log, Alpha 9 mm, right angled (side adjust), stereo",2,null,null,"Alpha 9-PC-STE-100k log, RD902F-20-15R1-A100K","Small Bear (US) or banzaimusic.com (EU)","100k-log-dual",2.8,5.6,null,null,null,"P1",null,null,null,"P2"]
[4,"Potentiometer","100 kΩ log, Alpha 9 mm, right angled (side adjust)",43,null,null,"RD901F-20-15R1-A100K","Small Bear (US) or Thonk (EU)","100k-log-single",1.17,50.309999999999995,"P1, P2",null,"P1",null,"P3, P4","P3, P4",null,"P1, P3"]
[1,"Trimmer","1k Ω",1,null,null,"PT 10 LV 1K","Mouser","531-PT10V-1K",0.50800000000000001,0.50800000000000001,null,null,null,null,null,null,null,null,"TR3"]
[1,"Trimmer","10 kΩ",6,null,null,"PT 10 LH 10K","Mouser","531-PT10H-10K",0.51800000000000002,{"$f":"IF(D213>=E213,D213*J213,E213*J213)","v":3.1080000000000001},null,null,null,null,"TR5","TR5",null,"TR1, TR2, TR3, TR5"]
[1,"Trimmer","10 kΩ",3,null,null,"PT 10 LV 10K","Mouser","531-PT10V-10K",0.52900000000000003,1.5870000000000002,null,null,null,null,null,null,"TR2",null,"TR1, TR2"]
[1,"Trimmer","20 kΩ",1,null,null,"PT 10 LV 20K","Mouser","531-PT10V-20K",0.50800000000000001,0.50800000000000001,null,null,null,null,null,null,null,null,"TR4"]
[1,"Trimmer","25 kΩ",57,50,null,"PT 10 LH 25K","Mouser","531-PT10H-25K",0.48699999999999999,27.759,"TR1, TR2, TR3",null,null,null,null,null,null,"TR4, TR6, TR7"]
[1,"Trimmer","100 kΩ",11,null,null,"PT 10 LH 100K","Mouser","531-PT10H-100K",0.50800000000000001,5.5880000000000001,null,null,"TR1","TR1, TR2","TR6, TR7, TR8, TR9","TR6, TR7, TR8, TR9"]
[1,"Trimmer","100 kΩ",1,null,null,"PT 10 LV 100K","Mouser","531-PT10V-100K",0.51800000000000002,0.51800000000000002,null,null,null,null,null,null,"TR1"]
[1,"Trimmer","250 kΩ",2,null,null,"PT 10 LH 250K","Mouser","531-PT10H-250K",0.50800000000000001,1.016,null,null,null,null,"TR10","TR10"]
[1,"Trimmer, multi-turn","100 Ω",4,null,null,"T93XA101KT20","Mouser","72-T93XA-100",1.56,6.24,null,null,null,null,"TR1, TR3","TR1, TR3"]
[1,"Trimmer, multi-turn","2.2 kΩ",2,null,null,"T93XA202KT20","Mouser","72-T93XA-2K",1.48,2.96,null,null,null,null,"TR2","TR2"]
[1,"Trimmer, multi-turn","100 kΩ",41,10,null,"T93XA104KT20","Mouser","72-T93XA-100K",1.23,50.43,"TR4, TR5",null,null,null,"TR4","TR4",null,"TR8, TR9, TR10"]
[1,"LED","LED green, 2.4 V, 2 mA",18,5,"3 mm LED","TLLG4401","Mouser","78-TLLG4401",0.3,5.3999999999999995,null,null,"LED1, LED2, LED3, LED4, LED5, LED6","LED1, LED2, LED3, LED4, LED5, LED6, LED11, LED12, LED13, LED14, LED15, LED16"]
[1,"LED","LED red, 2.4 V, 2 mA",34,25,"3 mm LED","TLLR4401","Mouser","78-TLLR4401",0.3,10.199999999999999,"LED",null,"LED8, LED9, LED10","LED8, LED9, LED10, LED18, LED19, LED20",null,null,null,"LED1",null,null,"5x front panel"]
[1,"LED","LED yellow, 2.4 V, 2 mA",3,5,"3 mm LED","TLLY4401","Mouser","78-TLLY4401",0.36699999999999999,1.835,null,null,"LED7","LED7, LED17"]
[5,"IC Socket","8 pins",23,null,null,"110-99-308-41-001000","Mouser","575-199308",0.38,8.74,null,null,"IC1, IC2, IC3, IC5","IC1, IC2, IC3, IC5, IC6, IC7","IC1, IC8","IC1, IC8","IC1, IC6","IC1, IC2, IC3, IC4, IC5, IC6, IC16"]
[5,"IC Socket","14 pins",98,null,null,"110-99-314-41-001000","Mouser","575-199314",0.49299999999999999,48.314,"IC1, IC2, IC3, IC4",null,null,null,"IC2, IC3, IC4, IC5, IC7","IC2, IC3, IC4, IC5, IC7","IC2, IC3, IC4, IC5, IC7, IC8","IC8, IC10, IC11, IC14, IC15","IC1, IC2, IC3, IC4, IC5"]
[5,"IC Socket","16 pins",21,null,null,"110-99-316-41-001000","Mouser","575-199316",0.42799999999999999,8.9879999999999995,"IC5",null,null,null,"IC6","IC6",null,"IC9"]
[5,"IC Socket","18 pins",3,null,null,"110-44-318-41-001000","Mouser","575-11044318",0.79500000000000004,2.3850000000000002,null,null,"IC4","IC4, IC8"]
[4,"Jack","3.5 mm jack",39,null,null,"CL13845G","Farnell",2766196,1.26,49.14,"CV-IN, CV-OUT",null,null,null,"CV-IN","CV-IN",null,null,"CV-IN"]
[1,"Jack","6.35 mm jack",7,null,null,"ACJS-MHDR","Mouser","523-ACJS-MHDR",1.1599999999999999,8.1199999999999992,null,null,"LINE-IN, MIC","LINE-IN, MIC",null,null,null,"FLTR-OUT, VOCODER-OUT","FOOT-SW"]
[1,"Connector","2x8 wire-to-board connector, RM2.54 mm",19,null,null,"Würth 61201623021","Mouser","710-61201623021",0.65,12.35,"1x",null,null,null,null,null,null,"1x"]
[1,"Connector","2x2 board-to-board connector, angled, RM2.54 mm",40,25,null,"Würth 61300421021","Mouser","710-61300421021",0.39,15.600000000000001,"2x",null,null,null,"2x","2x"]
[1,"Connector","2x8 board-to-board connector, angled, RM2.54 mm",19,10,null,"Würth 61301621021","Mouser","710-61301621021",0.871,16.548999999999999,"1x",null,null,null,null,null,null,"1x"]
[4,"Connector","EHR-2",57,100,null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,3.1199999999999997,null,null,"4x","11x","5x","6x","11x","11x","7x","2x"]
[4,"Connector","EHR-3",21,100,null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,3.45,null,null,"1x","1x","2x","2x","2x","1x","1x","11x"]
[1,"Connector","Jumper",40,null,null,"M7582-05","Mouser","855-M7582-05",9.7000000000000003E-2,3.88,"2x",null,null,null,"2x","2x"]
[4,"Connector","SEH-001T-P0.6",175,10,null,"SEH-001T-P0.6","Farnell",1863249,2.4400000000000002E-2,4.2700000000000005,null,null,"11x","25x","16x","18x","28x","23x","7x","35x"]
[4,"Connector","Wire-to-board connector, 2-pin",57,100,null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,6.8199999999999994,null,null,"AGC-L, EXC-L, AUDIO-L, EXP-L","AGC-L, EXC-L, AUDIO-L, EXP-L, AGC-R, EXC-R, AUDIO-R, EXP-R, INT-R, INT-L, MONO-SW","VUV-NSE, AGC, EXC-OUT, MIX-IN1, MIX-IN2","VUV-NSE, AGC, EXC-OUT, MIX-SW, MIX-OUT1, MIX-OUT2","VOICE, NOISE-L, NOISE-R, EXC-L, EXC-R, MIX-L, MIX-R, NOISE-INH, NOISE-INH, VOICED-LED, UNVOICED-LED","11x","7x","2x"]
[4,"Connector","Wire-to-board connector, 3-pin",19,100,null,"S3B-EH(LF)(SN)","Farnell",2481438,9.8599999999999993E-2,9.86,null,null,"SUPPLY","SUPPLY","SUPPLY, NOISE-SRC","SUPPLY, NOISE-SRC","SUPPLY, FORCED-VUV-SW","1x","1x","9x"]
[4,"Connector","Wire-to-board terminal block, 2 entries",1,null,null,"Weidmuller 1934250000","Farnell",2893169,1.02,1.02,null,null,null,null,null,null,null,null,null,"1x"]
[4,"Misc","8 A, slow blow, 20 x 5 mm",1,10,null,"Schurter 0001.2513","Farnell",1360861,0.29599999999999999,2.96,null,null,null,null,null,null,null,null,null,"FUSE"]
[5,"Misc","12 VDC 5 A 60 W",1,null,null,"GST60A12-P1J","Amazon, Jameco","GST60A12-P1J",14,14,null,null,null,null,null,null,null,null,null,"Power supply"]
[2,"Misc","ELC10D101E (100 µH)",2,null,null,"ELC-10D101E","Mouser","667-ELC-10D101E",0.91,1.82,null,null,null,null,null,null,null,null,null,"L1, L2"]
[4,"Misc","HTC-100M",1,null,null,"HTC-100M","Farnell",2550634,0.51400000000000001,0.51400000000000001,null,null,null,null,null,null,null,null,null,"FUSEHOLDER"]
[5,"Misc","Isolated 2.1x5.5mm power jack",1,null,null,null,"JDS Labs","JDS Labs",2.58,2.58,null,null,null,null,null,null,null,null,null,"Power jack"]
[5,"Misc","Solder pins,  ⌀ 1 mm",109,200,null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,5.18,"CHOP, CV, SYNTH, FLT",null,"LEFT, GND","LEFT, RIGHT, GND","AGCO, GND, PNK, SAW, WHT, SQR","AGCO, GND, PNK, SAW, WHT, SQR","GND, MIX-L, MIX-R","ENV, PWMR, PWML, BR, SBSW, GND, TRI, FLTR, VC-R, VC-L","GND, LOG, OSC, SLEW","GND, +12V, -12V"]
[2,"Misc","TRACO TEN 40-1222N",1,null,"Module","TRACO TEN 40-1222N","Mouser","495-TEN40-1222N",65.430000000000007,65.430000000000007,null,null,null,null,null,null,null,null,null,"TEN 40-1222N"]
[5,"Misc-2","1.6 mm shrink tubing",1,null,null,null,"Farnell",1210349,8.2799999999999999E-2,8.2799999999999999E-2,null,null,null,null,null,null,null,null,null,null,"1x"]
[5,"Misc-2","3 mm screws with nut, 12 mm length",6,null,null,null,null,"screws 1",null,0,null,null,null,null,null,null,null,null,null,null,"6x"]
[5,"Misc-2","3 mm screws with nut, 25 mm length",4,null,null,null,null,"screws 2",null,0,null,null,null,null,null,null,null,null,null,null,"4x"]
[5,"Misc-2","3.2 mm shrink tubing",1,null,null,null,"Farnell",1210352,1.63,1.63,null,null,null,null,null,null,null,null,null,null,"1x"]
[3,"Misc-2","10 Ω, 17 W resistor for testing purposes",2,null,null,"SQP20AJB-10R","Mouser","603-SQP20AJB-10R",1.06,2.12,null,null,null,null,null,null,null,null,null,"2x"]
[5,"Misc-2","16-wire ribbon cable, 28 AWG",1,null,null,"3M 3365-16","Farnell",297318,2.34,2.34,null,null,null,null,null,null,null,null,null,null,"1x"]
[4,"Misc-2","19 inch 3U enclosure",1,null,null,"Slim Line 03/230 3U 400 SILVER","Modushop","enclosure",53.9,53.9,null,null,null,null,null,null,null,null,null,null,"1x"]
[4,"Misc-2","Coax cable, 1.9 mm overall diameter",3,null,null,"Lapp 2170002","Farnell",1491534,4.6500000000000004,13.950000000000001,null,null,null,null,null,null,null,null,null,null,"1x"]
[5,"Misc-2","Knobs",50,null,"6.35 mm round shaft","Davies clone 1900h with brass insert","Thonk","knobs",0.73,36.5,null,null,null,null,null,null,null,null,null,null,"50x"]
[5,"Misc-2","Round nylon spacer",6,null,null,"D01475","Farnell",1733405,3.1699999999999999E-2,0.19019999999999998,null,null,null,null,null,null,null,null,null,null,"6x"]
[4,"Misc-2","Single-pole dual-throw switch, ON-OFF-ON",1,null,null,"H8620VBAAA","Farnell",733878,3.8,3.8,null,null,null,null,null,null,null,null,null,null,"1x"]
[4,"Misc-2","Single-pole dual-throw switch, ON-ON",6,null,null,"H8610VBAAA","Farnell",151134,2.36,14.16,null,null,null,null,null,null,null,null,null,null,"5x"]
[4,"Misc-2","Single-pole single-throw switch, momentary ON",1,null,null,"H8601VBAAA","Farnell",480393,3.8,3.8,null,null,null,null,null,null,null,null,null,null,"1x"]
[""]
["","totals:",null,{"$f":"SUM(D21:D261)","v":4056},null,null,null,null,null,null,{"$f":"SUM(K21:K261)","v":953.23799999999983}]
[""]
[""]
["","Color legend for left-most column:"]
[1,"See Mouser project \"18-channel stereo vocoder (excl. supply)\""]
[2,"See Mouser project \"Vocoder DC/DC supply\""]
[3,"See Mouser project \"Vocoder LDO supply\""]
[4,"See bundle request form"]
[5,"Your own responsibility"]

{"sheet":"Channel (common)","index":2,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
[" Below list of components is required 18 times"]
[" "]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Diode","D1, D2","1N4148",{"$f":"IF(B5<>\"\",LEN(B5)-LEN(SUBSTITUTE(B5,\",\",\"\"))+1,\"\")","v":2},"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,{"$f":"I5*D5","v":3.5999999999999997E-2}]
["LED","LED","LED red, 2.4 V, 2 mA",{"$f":"IF(B6<>\"\",LEN(B6)-LEN(SUBSTITUTE(B6,\",\",\"\"))+1,\"\")","v":1},"3 mm LED","TLLR4401","Mouser","78-TLLR4401",0.3,{"$f":"I6*D6","v":0.3}]
["Transistor","T1, T2","2N3904",2,"TO-92","2N3904BU","Mouser","512-2N3904BU",5.0999999999999997E-2,0.10199999999999999]
["IC","IC3, IC4","TL074",2,"DIL14","TL074CN","Mouser","595-TL074CN",0.46800000000000003,0.93600000000000005]
["IC","IC1, IC2","MC33079",2,"DIL14","MC33079PG","Rochester","MC33079",0.62,1.24]
["IC","IC5","CD4053",1,"DIL16","CD4053BE","Mouser","595-CD4053BE",0.372,0.372]
["Ceramic","C18, C19, C20, C21, C23, C24, C25, C26, C27, C28, C29, C30, C31, C32, C33, C34","100 nF",16,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,0.38400000000000001]
["Film","C17, C22","220 nF",{"$f":"IF(B12<>\"\",LEN(B12)-LEN(SUBSTITUTE(B12,\",\",\"\"))+1,\"\")","v":2},"RM2.5/RM5.0","R82DC3220Z360K","Mouser","80-82DC3220Z360K",0.10299999999999999,0.20599999999999999]
["Electrolytic","C35, C36, C37, C38, C39, C40","47 µF/35 V, max. ⌀ 5 mm",6,"RM2.0","Würth 860010572005","Mouser","710-860010572005",7.0999999999999994E-2,0.42599999999999993]
["Resistor","R59, R60, R61, R62, R63, R64, R65","47 Ω, 250 mW",7,"0204/0207","LR0204F47R","Farnell",2329945,4.0800000000000003E-2,0.28560000000000002]
["Resistor","R46","100 Ω",{"$f":"IF(B15<>\"\",LEN(B15)-LEN(SUBSTITUTE(B15,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F100R","Farnell",2329854,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R26","750 Ω",1,"0204/0207","LR0204F750R","Farnell",2329971,3.5299999999999998E-2,{"$f":"I16*D16","v":3.5299999999999998E-2}]
["Resistor","R43","1 kΩ",1,"0204/0207","LR0204F1K0","Farnell",2329885,7.7100000000000002E-2,7.7100000000000002E-2]
["Resistor","R58","2.2 kΩ",1,"0204/0207","LR0204F2K2","Farnell",2329912,7.7100000000000002E-2,7.7100000000000002E-2]
["Resistor","R52, R53","3.3 kΩ",{"$f":"IF(B19<>\"\",LEN(B19)-LEN(SUBSTITUTE(B19,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F3K3","Farnell",2329934,3.5999999999999997E-2,{"$f":"I19*D19","v":7.1999999999999995E-2}]
["Resistor","R42","4.7 kΩ",1,"0204/0207","LR0204F4K7","Farnell",2329947,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R49","5.1 kΩ",1,"0204/0207","LR0204F5K1","Farnell",2329957,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R40, R50","8.2 kΩ",2,"0204/0207","LR0204F8K2","Farnell",2329981,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R27, R28, R29, R30, R31, R32, R33, R34, R41, R51, R54","10 kΩ",11,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,0.374]
["Resistor","R47, R48","15 kΩ",2,"0204/0207","LR0204F15K","Farnell",2329873,3.5299999999999998E-2,7.0599999999999996E-2]
["Resistor","R55","20 kΩ",{"$f":"IF(B25<>\"\",LEN(B25)-LEN(SUBSTITUTE(B25,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,{"$f":"I25*D25","v":3.5299999999999998E-2}]
["Resistor","R57","22 kΩ",1,"0204/0207","LR0204F22K","Farnell",2329901,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R44","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R25","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,{"$f":"I28*D28","v":3.5299999999999998E-2}]
["Resistor","R35, R45","47 kΩ",2,"0204/0207","LR0204F47K","Farnell",2329944,2.7E-2,5.3999999999999999E-2]
["Resistor","R56, R66","100 kΩ",2,"0204/0207","LR0204F100K","Farnell",2329853,2.6499999999999999E-2,5.2999999999999999E-2]
["Resistor","R36","4.7 MΩ, 5%",{"$f":"IF(B31<>\"\",LEN(B31)-LEN(SUBSTITUTE(B31,\",\",\"\"))+1,\"\")","v":1},"0204/0207","CFR16J4M7","Farnell",2329535,5.2900000000000003E-2,5.2900000000000003E-2]
["Trimmer, multi-turn","TR4, TR5","100 kΩ",2,null,"T93XA104KT20","Mouser","72-T93XA-100K",1.23,2.46]
["Trimmer","TR1, TR2, TR3","25 kΩ",3,null,"PT 10 LH 25K","Mouser","531-PT10H-25K",0.48699999999999999,1.4609999999999999]
["Potentiometer","P1, P2","100 kΩ log, Alpha 9 mm, right angled (side adjust)",2,null,"RD901F-20-15R1-A100K","Small Bear (US) or Thonk (EU)","100k-log-single",1.17,2.34]
["Jack","CV-IN, CV-OUT","3.5 mm jack",2,null,"CL13845G","Farnell",2766196,1.26,2.52,"alternative: CL1384"]
["Connector","2x","2x2 board-to-board connector, angled, RM2.54 mm",2,null,"Würth 61300421021","Mouser","710-61300421021",0.39,0.78]
["Connector","1x","2x8 board-to-board connector, angled, RM2.54 mm",1,null,"Würth 61301621021","Mouser","710-61301621021",0.871,0.871]
["Connector","1x","2x8 wire-to-board connector, RM2.54 mm",1,null,"Würth 61201623021","Mouser","710-61201623021",0.65,0.65]
["Connector","2x","Jumper",2,null,"M7582-05","Mouser","855-M7582-05",9.7000000000000003E-2,0.19400000000000001]
["IC Socket","IC1, IC2, IC3, IC4","14 pins",{"$f":"IF(B40<>\"\",LEN(B40)-LEN(SUBSTITUTE(B40,\",\",\"\"))+1,\"\")","v":4},null,"110-99-314-41-001000","Mouser","575-199314",0.49299999999999999,{"$f":"I40*D40","v":1.972}]
["IC Socket","IC5","16 pins",{"$f":"IF(B41<>\"\",LEN(B41)-LEN(SUBSTITUTE(B41,\",\",\"\"))+1,\"\")","v":1},null,"110-99-316-41-001000","Mouser","575-199316",0.42799999999999999,{"$f":"I41*D41","v":0.42799999999999999}]
["Misc","CHOP, CV, SYNTH, FLT","Solder pins,  ⌀ 1 mm",{"$f":"IF(B42<>\"\",LEN(B42)-LEN(SUBSTITUTE(B42,\",\",\"\"))+1,\"\")","v":4},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,{"$f":"I42*D42","v":0.1036}]
[]
[null,null,null,null,null,null,null,null,"Sub Total:",{"$f":"SUM(J5:J42)","v":19.255099999999999}]
[]
[null,null,null,null,null,null,null,null,"+ Capacitors:",{"$f":"SUM('Channel (frequency)'!O30:O32)/18","v":3.9500000000000006}]
[null,null,null,null,null,null,null,null,"+ Resistors:",{"$f":"'Channel (frequency)'!Q122/18","v":3.7661555555555566}]
[]
[null,null,null,null,null,null,null,null,"Grand total:",{"$f":"SUM(J44:J47)","v":26.971255555555555}]

{"sheet":"Channel (frequency)","index":3,"n_rows":124,"n_cols":20,"rows_kept":124,"cut":false,"hidden":false,"merged":[[123,16,124,18],[5,1,22,1],[3,4,3,18],[1,1,1,19],[29,9,29,11],[30,9,30,11],[31,9,31,11],[28,9,28,11]]}
[]
[null,"Channel-dependent components"]
[]
[null,null,null,null,"Resistors (many from the E48 series), 1% tolerance, 125 mW or higher, throughhole, RM7.5 or smaller",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"SMD (1206 or 0805), ±5% tolerance or better, C0G/NP0 for temperature stability."]
[null,null,null,null,"R1, R13","R2, R14","R3, R15","R4, R16","R5, R17","R6, R18","R7, R19","R8, R20","R9, R21","R10, R22","R11, R23","R12, R24","R37","R38","R39","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16"]
[null,"Frequency",1,"7000 Hz","301 Ω","9.09 kΩ","18.7 kΩ","287 Ω","8.66 kΩ","17.8 kΩ","237 Ω","8.66 kΩ","28.7 kΩ","196 Ω","6.81 kΩ","22.6 kΩ","24 kΩ","20 kΩ","6.8 kΩ","10 nF"]
[null,null,{"$f":"1+C6","v":2},"5500 Hz","383 Ω","11.5 kΩ","23.7 kΩ","365 Ω","11 kΩ","22.6 kΩ","301 Ω","11 kΩ","36.5 kΩ","249 Ω","8.66 kΩ","28.7 kΩ","24 kΩ","20 kΩ","6.8 kΩ","10 nF"]
[null,null,{"$f":"1+C7","v":3},"4330 Hz","487 Ω","14.7 kΩ","30.1 kΩ","464 Ω","14 kΩ","28.7 kΩ","383 Ω","14 kΩ","46.4 kΩ","316 Ω","11 kΩ","36.5 kΩ","24 kΩ","20 kΩ","6.8 kΩ","10 nF"]
[null,null,4,"3410 Hz","619 Ω","18.7 kΩ","38.3 kΩ","590 Ω","17.8 kΩ","36.5 kΩ","487 Ω","17.8 kΩ","59 kΩ","402 Ω","14 kΩ","46.4 kΩ","24 kΩ","20 kΩ","6.8 kΩ","10 nF"]
[null,null,5,"2680 Hz","787 Ω","23.7 kΩ","48.7 kΩ","750 Ω","22.6 kΩ","46.4 kΩ","619 Ω","22.6 kΩ","75 kΩ","511 Ω","17.8 kΩ","59 kΩ","24 kΩ","20 kΩ","6.8 kΩ","10 nF"]
[null,null,6,"2110 Hz","1 kΩ","30.1 kΩ","61.9 kΩ","953 Ω","28.7 kΩ","59 kΩ","787 Ω","28.7 kΩ","95.3 kΩ","649 Ω","22.6 kΩ","75 kΩ","24 kΩ","20 kΩ","6.8 kΩ","10 nF"]
[null,null,7,"1660 Hz","383 Ω","11.5 kΩ","23.7 kΩ","365 Ω","11 kΩ","22.6 kΩ","301 Ω","11 kΩ","36.5 kΩ","249 Ω","8.66 kΩ","28.7 kΩ","24 kΩ","20 kΩ","6.8 kΩ","33 nF"]
[null,null,8,"1310 Hz","487 Ω","14.7 kΩ","30.1 kΩ","464 Ω","14 kΩ","28.7 kΩ","383 Ω","14 kΩ","46.4 kΩ","316 Ω","11 kΩ","36.5 kΩ","24 kΩ","20 kΩ","6.8 kΩ","33 nF"]
[null,null,9,"1030 Hz","619 Ω","18.7 kΩ","38.3 kΩ","590 Ω","17.8 kΩ","36.5 kΩ","487 Ω","17.8 kΩ","59 kΩ","402 Ω","14 kΩ","46.4 kΩ","24 kΩ","20 kΩ","6.8 kΩ","33 nF"]
[null,null,10,"810 Hz","787 Ω","23.7 kΩ","48.7 kΩ","750 Ω","22.6 kΩ","46.4 kΩ","619 Ω","22.6 kΩ","75 kΩ","511 Ω","17.8 kΩ","59 kΩ","24 kΩ","20 kΩ","6.8 kΩ","33 nF"]
[null,null,11,"640 Hz","1 kΩ","30.1 kΩ","61.9 kΩ","953 Ω","28.7 kΩ","59 kΩ","787 Ω","28.7 kΩ","95.3 kΩ","649 Ω","22.6 kΩ","75 kΩ","24 kΩ","20 kΩ","6.8 kΩ","33 nF"]
[null,null,12,"500 Hz","1.27 kΩ","38.3 kΩ","78.7 kΩ","1.21 kΩ","36.5 kΩ","75 kΩ","1 kΩ","36.5 kΩ","121 kΩ","825 Ω","28.7 kΩ","95.3 kΩ","24 kΩ","20 kΩ","6.8 kΩ","33 nF"]
[null,null,13,"390 Hz","536 Ω","16.2 kΩ","33.2 kΩ","511 Ω","15.4 kΩ","31.6 kΩ","422 Ω","15.4 kΩ","51.1 kΩ","348 Ω","12.1 kΩ","40.2 kΩ","33 kΩ","27 kΩ","10 kΩ","100 nF"]
[null,null,14,"310 Hz","681 Ω","20.5 kΩ","42.2 kΩ","649 Ω","19.6 kΩ","40.2 kΩ","536 Ω","19.6 kΩ","64.9 kΩ","442 Ω","15.4 kΩ","51.1 kΩ","33 kΩ","27 kΩ","10 kΩ","100 nF"]
[null,null,15,"240 Hz","866 Ω","26.1 kΩ","53.6 kΩ","825 Ω","24.9 kΩ","51.1 kΩ","681 Ω","24.9 kΩ","82.5 kΩ","562 Ω","19.6 kΩ","64.9 kΩ","33 kΩ","27 kΩ","10 kΩ","100 nF"]
[null,null,16,"190 Hz","1.1 kΩ","33.2 kΩ","68.1 kΩ","1.05 kΩ","31.6 kΩ","64.9 kΩ","866 Ω","31.6 kΩ","105 kΩ","715 Ω","24.9 kΩ","82.5 kΩ","33 kΩ","27 kΩ","10 kΩ","100 nF"]
[null,null,17,"150 Hz","1.4 kΩ","42.2 kΩ","86.6 kΩ","1.33 kΩ","40.2 kΩ","82.5 kΩ","1.1 kΩ","40.2 kΩ","133 kΩ","909 Ω","31.6 kΩ","105 kΩ","33 kΩ","27 kΩ","10 kΩ","100 nF"]
[null,null,18,"120 Hz","1.78 kΩ","53.6 kΩ","110 kΩ","1.69 kΩ","51.1 kΩ","105 kΩ","1.4 kΩ","51.1 kΩ","169 kΩ","1.15 kΩ","40.2 kΩ","133 kΩ","33 kΩ","27 kΩ","10 kΩ","100 nF"]
[]
[]
[]
[null,null,null,"Suggested products:"]
[]
[null,null,null,null,"Value",null,"Count",null,"Distr","Product",null,null,"Order #","Price [€]","Total [€]"]
[null,null,null,null,"10 nF",null,100,null,"Mouser","08055A103JAT2A",null,null,"581-08055A103JAT2A",0.224,{"$f":"N30*G30","v":22.400000000000002}]
[null,null,null,null,"33 nF",null,100,null,"Mouser","CGA5F2C0G1H333J085AA",null,null,"810-CGA5F2C0G1H333J",0.16,{"$f":"N31*G31","v":16}]
[null,null,null,null,"100 nF",null,100,null,"Mouser","GRM31C5C1H104JA01L",null,null,"81-GRM31C5C1H104JA1L",0.32700000000000001,{"$f":"N32*G32","v":32.700000000000003}]
[null,null,null,null,"6.8 kΩ",null,12,null,"Farnell","LR0204F6K8",null,null,2329969,3.5299999999999998E-2,{"$f":"N33*G33","v":0.42359999999999998},null,{"$f":"O33","v":0.42359999999999998}]
[null,null,null,null,"10 kΩ",null,6,null,"Farnell","LR0204F10K",null,null,2329855,3.4000000000000002E-2,{"$f":"N34*G34","v":0.20400000000000001},null,0.20400000000000001]
[null,null,null,null,"20 kΩ",null,12,null,"Farnell","LR0204F20K",null,null,2329897,3.5299999999999998E-2,0.42359999999999998,null,0.42359999999999998]
[null,null,null,null,"24 kΩ",null,12,null,"Farnell","LR0204F24K",null,null,2329904,3.5999999999999997E-2,0.43199999999999994,null,0.43199999999999994]
[null,null,null,null,"27 kΩ",null,6,null,"Farnell","LR0204F27K",null,null,2329909,3.5299999999999998E-2,0.21179999999999999,null,0.21179999999999999]
[null,null,null,null,"33 kΩ",null,6,null,"Farnell","LR0204F33K",null,null,2329922,3.5299999999999998E-2,0.21179999999999999,null,0.21179999999999999]
[null,null,null,null,"196 Ω",1,{"$f":"F39*2","v":2},{"$f":"IF(MID(E39,FIND(\"Ω\",E39)-1,1)=\"k\",LEFT(E39,FIND(\"k\",E39)-1)*1000,LEFT(E39,FIND(\"Ω\",E39)-1)*1)","v":196},"Farnell",{"$f":"IF(H39<1000,CONCATENATE(\"MRS25000C\",H39,\"0FCT00\"),IF(H39<10000,CONCATENATE(\"MRS25000C\",LEFT(H39,3),\"1FCT00\"),IF(H39<100000,CONCATENATE(\"MRS25000C\",LEFT(H39,3),\"2FCT00\"),IF(H39<1000000,CONCATENATE(\"MRS25000C\",LEFT(H39,3),\"3FCT00\")))))","v":"MRS25000C1960FCT00"},null,null,9465120,5.0999999999999997E-2,{"$f":"IF(N39<>0,IF(G39<10,N39*10,G39*N39),\"\")","v":0.51},null,{"$f":"IF(G39<10,N39*10,G39*N39)","v":0.51}]
[null,null,null,null,"237 Ω",1,{"$f":"F40*2","v":2},{"$f":"IF(MID(E40,FIND(\"Ω\",E40)-1,1)=\"k\",LEFT(E40,FIND(\"k\",E40)-1)*1000,LEFT(E40,FIND(\"Ω\",E40)-1)*1)","v":237},"Farnell",{"$f":"IF(H40<1000,CONCATENATE(\"MRS25000C\",H40,\"0FCT00\"),IF(H40<10000,CONCATENATE(\"MRS25000C\",LEFT(H40,3),\"1FCT00\"),IF(H40<100000,CONCATENATE(\"MRS25000C\",LEFT(H40,3),\"2FCT00\"),IF(H40<1000000,CONCATENATE(\"MRS25000C\",LEFT(H40,3),\"3FCT00\")))))","v":"MRS25000C2370FCT00"},null,null,9466185,8.3000000000000004E-2,{"$f":"IF(N40<>0,IF(G40<10,N40*10,G40*N40),\"\")","v":0.83000000000000007},null,0.83000000000000007]
[null,null,null,null,"249 Ω",2,4,249,"Farnell","MRS25000C2490FCT00",null,null,9466282,8.5999999999999993E-2,0.85999999999999988,null,0.85999999999999988]
[null,null,null,null,"287 Ω",1,2,287,"Farnell","MRS25000C2870FCT00",null,null,9466584,5.0999999999999997E-2,0.51,null,0.51]
[null,null,null,null,"301 Ω",3,6,301,"Farnell","MRS25000C3010FCT00",null,null,9467149,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"316 Ω",2,4,316,"Farnell","MRS25000C3160FCT00",null,null,9467246,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"348 Ω",1,2,348,"Farnell","MRS25000C3480FCT00",null,null,9467424,7.2999999999999995E-2,0.73,null,0.73]
[null,null,null,null,"365 Ω",2,4,365,"Farnell","MRS25000C3650FCT00",null,null,9467548,5.0999999999999997E-2,0.51,null,0.51]
[null,null,null,null,"383 Ω",4,8,383,"Farnell","MRS25000C3830FCT00",null,null,9467645,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"402 Ω",2,4,402,"Farnell","MRS25000C4020FCT00",null,null,9468145,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"422 Ω",1,2,422,"Farnell","MRS25000C4220FCT00",null,null,9468226,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"442 Ω",1,2,442,"Farnell","MRS25000C4420FCT00",null,null,9468340,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"464 Ω",2,4,464,"Farnell","MRS25000C4640FCT00",null,null,9468420,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"487 Ω",4,8,487,"Farnell","MRS25000C4870FCT00",null,null,9468544,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"511 Ω",3,6,511,"Farnell","MRS25000C5110FCT00",null,null,9468854,7.2999999999999995E-2,0.73,null,0.73]
[null,null,null,null,"536 Ω",2,4,536,"Farnell","MRS25000C5360FCT00",null,null,9468951,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"562 Ω",1,2,562,"Farnell","MRS25000C5620FCT00",null,null,9469052,6.5000000000000002E-2,0.65,null,0.65]
[null,null,null,null,"590 Ω",2,4,590,"Farnell","MRS25000C5900FCT00",null,null,9469150,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"619 Ω",4,8,619,"Farnell","MRS25000C6190FCT00",null,null,9469435,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"649 Ω",3,6,649,"Farnell","MRS25000C6490FCT00",null,null,9469559,0.05,0.5,null,0.5]
[null,null,null,null,"681 Ω",2,4,681,"Farnell","MRS25000C6810FCT00",null,null,9469656,8.4000000000000005E-2,0.84000000000000008,null,0.84000000000000008]
[null,null,null,null,"715 Ω",1,2,715,"Farnell","MRS25000C7150FCT00",null,null,9469907,8.7999999999999995E-2,0.87999999999999989,null,0.87999999999999989]
[null,null,null,null,"750 Ω",2,4,750,"Farnell","MRS25000C7500FCT00",null,null,9469982,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"787 Ω",4,8,787,"Farnell","MRS25000C7870FCT00",null,null,9470069,7.2999999999999995E-2,0.73,null,0.73]
[null,null,null,null,"825 Ω",2,4,825,"Farnell","MRS25000C8250FCT00",null,null,9470263,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"866 Ω",2,4,866,"Farnell","MRS25000C8660FCT00",null,null,9470360,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"909 Ω",1,2,909,"Farnell","MRS25000C9090FCT00",null,null,9470549,5.0999999999999997E-2,0.51,null,0.51]
[null,null,null,null,"953 Ω",2,4,953,"Farnell","MRS25000C9530FCT00",null,null,9470670,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"1 kΩ",3,6,1000,"Farnell","MRS25000C1001FCT00",null,null,9465170,0.05,0.5,null,0.5]
[null,null,null,null,"1.05 kΩ",1,2,1050,"Farnell","MRS25000C1051FCT00",null,null,9465197,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"1.1 kΩ",2,4,1100,"Farnell","MRS25000C1101FCT00",null,null,9465219,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"1.15 kΩ",1,2,1150,"Farnell","MRS25000C1151FCT00",null,null,9465235,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"1.21 kΩ",1,2,1210,"Farnell","MRS25000C1211FCT00",null,null,9465260,5.0999999999999997E-2,0.51,null,{"$f":"IF(G71<10,N71*10,G71*N71)","v":0.51}]
[null,null,null,null,"1.27 kΩ",1,2,1270,"Farnell","MRS25000C1271FCT00",null,null,9465286,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"1.33 kΩ",1,2,1330,"Farnell","MRS25000C1331FCT00",null,null,9465308,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"1.4 kΩ",2,4,1400,"Farnell","MRS25000C1401FCT00",null,null,9465324,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"1.69 kΩ",1,2,1690,"Farnell","MRS25000C1691FCT00",null,null,9465413,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"1.78 kΩ",1,2,1780,"Farnell","MRS25000C1781FCT00",null,null,9465430,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"6.81 kΩ",1,2,6810,"Farnell","MRS25000C6811FCT00",null,null,9469818,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"8.66 kΩ",4,8,8660,"Farnell","MRS25000C8661FCT00",null,null,9470476,8.8999999999999996E-2,0.8899999999999999,null,0.8899999999999999]
[null,null,null,null,"9.09 kΩ",1,2,9090,"Farnell","MRS25000C9091FCT00",null,null,9470743,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"11 kΩ",6,12,11000,"Farnell","MRS25000C1102FCT00",null,null,9464140,5.0999999999999997E-2,0.61199999999999999,null,0.61199999999999999]
[null,null,null,null,"11.5 kΩ",2,4,11500,"Farnell","MRS25000C1152FCT00",null,null,9464166,5.0999999999999997E-2,0.51,null,0.51]
[null,null,null,null,"12.1 kΩ",1,2,12100,"Farnell","MRS25000C1212FCT00",null,null,9464310,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"14 kΩ",6,12,14000,"Farnell","MRS25000C1402FCT00",null,null,9464565,8.6999999999999994E-2,1.044,null,1.044]
[null,null,null,null,"14.7 kΩ",2,4,14700,"Farnell","MRS25000C1472FCT00",null,null,9464581,8.5000000000000006E-2,0.85000000000000009,null,0.85000000000000009]
[null,null,null,null,"15.4 kΩ",3,6,15400,"Farnell","MRS25000C1542FCT00",null,null,9464697,8.4000000000000005E-2,0.84000000000000008,null,0.84000000000000008]
[null,null,null,null,"16.2 kΩ",1,2,16200,"Farnell","MRS25000C1622FCT00",null,null,9464832,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"17.8 kΩ",7,14,17800,"Farnell","MRS25000C1782FCT00",null,null,9464956,0.06,0.84,null,0.84]
[null,null,null,null,"18.7 kΩ",3,6,18700,"Farnell","MRS25000C1872FCT00",null,null,9465057,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"19.6 kΩ",3,6,19600,"Farnell","MRS25000C1962FCT00",null,null,9465146,8.4000000000000005E-2,0.84000000000000008,null,0.84000000000000008]
[null,null,null,null,"20.5 kΩ",1,2,20500,"Farnell","MRS25000C2052FCT00",null,null,9465928,8.1000000000000003E-2,0.81,null,0.81]
[null,null,null,null,"22.6 kΩ",9,18,22600,"Farnell","MRS25000C2262FCT00",null,null,9466118,8.5000000000000006E-2,1.53,null,1.53]
[null,null,null,null,"23.7 kΩ",4,8,23700,"Farnell","MRS25000C2372FCT00",null,null,9466207,5.0999999999999997E-2,0.51,null,0.51]
[null,null,null,null,"24.9 kΩ",3,6,24900,"Farnell","MRS25000C2492FCT00",null,null,9466312,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"26.1 kΩ",1,2,26100,"Farnell","MRS25000C2612FCT00",null,null,9466436,8.7999999999999995E-2,0.87999999999999989,null,0.87999999999999989]
[null,null,null,null,"28.7 kΩ",10,20,28700,"Farnell","MRS25000C2872FCT00",null,null,9466606,8.6999999999999994E-2,1.7399999999999998,null,1.7399999999999998]
[null,null,null,null,"30.1 kΩ",4,8,30100,"Farnell","MRS25000C3012FCT00",null,null,9467181,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"31.6 kΩ",4,8,31600,"Farnell","MRS25000C3162FCT00",null,null,9467254,5.0999999999999997E-2,0.51,null,0.51]
[null,null,null,null,"33.2 kΩ",2,4,33200,"Farnell","MRS25000C3322FCT00",null,null,9467360,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"36.5 kΩ",8,16,36500,"Farnell","MRS25000C3652FCT00",null,null,9467564,8.5000000000000006E-2,1.36,null,1.36]
[null,null,null,null,"38.3 kΩ",3,6,38300,"Farnell","MRS25000C3832FCT00",null,null,9467653,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"40.2 kΩ",5,10,40200,"Farnell","MRS25000C4022FCT00",null,null,9468153,8.4000000000000005E-2,0.84000000000000008,null,0.84000000000000008]
[null,null,null,null,"42.2 kΩ",2,4,42200,"Farnell","MRS25000C4222FCT00",null,null,9468234,5.0999999999999997E-2,0.51,null,0.51]
[null,null,null,null,"46.4 kΩ",6,12,46400,"Farnell","MRS25000C4642FCT00",null,null,9468439,8.6999999999999994E-2,1.044,null,{"$f":"IF(G103<10,N103*10,G103*N103)","v":1.044}]
[null,null,null,null,"48.7 kΩ",2,{"$f":"F104*2","v":4},{"$f":"IF(MID(E104,FIND(\"Ω\",E104)-1,1)=\"k\",LEFT(E104,FIND(\"k\",E104)-1)*1000,LEFT(E104,FIND(\"Ω\",E104)-1)*1)","v":48700},"Farnell",{"$f":"IF(H104<1000,CONCATENATE(\"MRS25000C\",H104,\"0FCT00\"),IF(H104<10000,CONCATENATE(\"MRS25000C\",LEFT(H104,3),\"1FCT00\"),IF(H104<100000,CONCATENATE(\"MRS25000C\",LEFT(H104,3),\"2FCT00\"),IF(H104<1000000,CONCATENATE(\"MRS25000C\",LEFT(H104,3),\"3FCT00\")))))","v":"MRS25000C4872FCT00"},null,null,9468552,8.6999999999999994E-2,{"$f":"IF(N104<>0,IF(G104<10,N104*10,G104*N104),\"\")","v":0.86999999999999988},null,0.86999999999999988]
[null,null,null,null,"51.1 kΩ",5,10,51100,"Farnell","MRS25000C5112FCT00",null,null,9468870,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"53.6 kΩ",2,4,53600,"Farnell","MRS25000C5362FCT00",null,null,9468960,5.0999999999999997E-2,0.51,null,0.51]
[null,null,null,null,"59 kΩ",6,12,59000,"Farnell","MRS25000C5902FCT00",null,null,9469168,8.6999999999999994E-2,1.044,null,1.044]
[null,null,null,null,"61.9 kΩ",2,4,61900,"Farnell","MRS25000C6192FCT00",null,null,9469443,8.5999999999999993E-2,0.85999999999999988,null,0.85999999999999988]
[null,null,null,null,"64.9 kΩ",3,6,64900.000000000007,"Farnell","MRS25000C6492FCT00",null,null,9469567,0.06,0.6,null,0.6]
[null,null,null,null,"68.1 kΩ",1,2,68100,"Farnell","MRS25000C6812FCT00",null,null,9469672,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"75 kΩ",5,10,75000,"Farnell","MRS25000C7502FCT00",null,null,9469990,8.4000000000000005E-2,0.84000000000000008,null,0.84000000000000008]
[null,null,null,null,"78.7 kΩ",1,2,78700,"Farnell","MRS25000C7872FCT00",null,null,9470077,0.06,0.6,null,0.6]
[null,null,null,null,"82.5 kΩ",3,6,82500,"Farnell","MRS25000C8252FCT00",null,null,9470280,0.06,0.6,null,0.6]
[null,null,null,null,"86.6 kΩ",1,2,86600,"Farnell","MRS25000C8662FCT00",null,null,9470379,0.06,0.6,null,0.6]
[null,null,null,null,"95.3 kΩ",3,6,95300,"Farnell","MRS25000C9532FCT00",null,null,9470689,0.05,0.5,null,0.5]
[null,null,null,null,"105 kΩ",3,6,105000,"Farnell","MRS25000C1053FCT00",null,null,9463933,4.9000000000000002E-2,0.49,null,0.49]
[null,null,null,null,"110 kΩ",1,2,110000,"Farnell","MRS25000C1103FCT00",null,null,9464069,5.0999999999999997E-2,0.51,null,0.51]
[null,null,null,null,"121 kΩ",1,2,121000,"Farnell","MRS25000C1213FCT00",null,null,9464247,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[null,null,null,null,"133 kΩ",2,4,133000,"Farnell","MRS25000C1333FCT00",null,null,9464409,8.4000000000000005E-2,0.84000000000000008,null,0.84000000000000008]
[null,null,null,null,"169 kΩ",1,2,169000,"Farnell","MRS25000C1693FCT00",null,null,9464808,8.6999999999999994E-2,0.86999999999999988,null,0.86999999999999988]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Total:",{"$f":"SUM(O30:O120)","v":138.89080000000007},"€",{"$f":"SUM(Q33:Q120)","v":67.790800000000019},"€"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Total price resistors, all boards combined."]

{"sheet":"Voice preamp","index":4,"n_rows":47,"n_cols":11,"rows_kept":47,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Diode","D1, D2, D3, D4","1N4148",{"$f":"IF(B5<>\"\",LEN(B5)-LEN(SUBSTITUTE(B5,\",\",\"\"))+1,\"\")","v":4},"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,{"$f":"I5*D5","v":7.1999999999999995E-2}]
[]
["LED","LED8, LED9, LED10","LED red, 2.4 V, 2 mA",3,"3 mm LED","TLLR4401","Mouser","78-TLLR4401",0.3,{"$f":"I7*D7","v":0.89999999999999991}]
["LED","LED7","LED yellow, 2.4 V, 2 mA",1,"3 mm LED","TLLY4401","Mouser","78-TLLY4401",0.36699999999999999,0.36699999999999999]
["LED","LED1, LED2, LED3, LED4, LED5, LED6","LED green, 2.4 V, 2 mA",6,"3 mm LED","TLLG4401","Mouser","78-TLLG4401",0.3,1.7999999999999998]
["IC","IC1, IC2, IC3","NE5532",3,"DIL8","NE5532AP","Mouser","595-NE5532AP",0.81399999999999995,2.4419999999999997]
["IC","IC4","TL072",1,"DIL8","TL072IP","Mouser","595-TL072IP",0.59399999999999997,0.59399999999999997]
["IC","IC5","LM3916",1,"DIL18",{"$f":"C12","v":"LM3916"},null,"LM3916",1.98,1.98]
["Ceramic","C5, C6","22 pF",2,"RM2.5","K220J15C0GF53L2","Mouser","594-K220J15C0GF53L2",0.27100000000000002,0.54200000000000004]
["Ceramic","C22, C23, C24, C25, C26, C27, C28, C29, C30","100 nF",9,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,0.216]
[]
["Film","C1, C11","100 nF",2,"RM2.5/RM5.0","R82EC3100AA70J","Mouser","80-R82EC3100AA70J",0.14099999999999999,0.28199999999999997]
["Film","C7","220 nF",1,"RM2.5/RM5.0","R82DC3220Z360K","Mouser","80-82DC3220Z360K",0.10299999999999999,0.10299999999999999]
["Film","C3, C4, C13, C14","1 µF",4,"RM2.5/RM5.0","R82DC4100Z360K","Mouser","80-R82DC4100Z360K",0.27900000000000003,1.1160000000000001]
["Electrolytic","C8","3.3 µF/50 V, max. ⌀ 5 mm",1,"RM2.0","Würth 860020672007","Mouser","710-860020672007",0.1,0.1]
["Electrolytic","C2, C12","10 µF/50 V, max. ⌀ 5 mm",2,"RM2.0","Würth 860020672010","Mouser","710-860020672010",0.1,0.2]
["Electrolytic","C20, C21, C31, C32","100 µF/25 V, max. ⌀ 7 mm",4,"RM2.5","Würth 860010473007","Mouser","710-860010473007",0.111,0.44400000000000001]
["Resistor","R23, R24","47 Ω, 250 mW",2,"0204/0207","LR0204F47R","Farnell",2329945,4.0800000000000003E-2,8.1600000000000006E-2]
["Resistor","R20","510 Ω",1,"0204/0207","LR0204F510R","Farnell",2329949,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R3, R33","1 kΩ",2,"0204/0207","LR0204F1K0","Farnell",2329885,7.7100000000000002E-2,0.1542]
["Resistor","R21","7.5 kΩ",1,"0204/0207","LR0204F7K5","Farnell",2329974,8.1199999999999994E-2,8.1199999999999994E-2]
["Resistor","R11","10 kΩ",1,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,3.4000000000000002E-2]
["Resistor","R22","15 kΩ",1,"0204/0207","LR0204F15K","Farnell",2329873,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R12","22 kΩ",1,"0204/0207","LR0204F22K","Farnell",2329901,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R7","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R13","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,{"$f":"I30*D30","v":3.5299999999999998E-2}]
["Resistor","R1, R5, R6, R8, R9, R31, R35, R36","47 kΩ",8,"0204/0207","LR0204F47K","Farnell",2329944,2.7E-2,0.216]
["Resistor","R10, R14, R15, R16, R17","100 kΩ",5,"0204/0207","LR0204F100K","Farnell",2329853,2.6499999999999999E-2,0.13250000000000001]
["Resistor","R4, R18, R19, R34","200 kΩ",4,"0204/0207","LR0204F200K","Farnell",2329895,3.4700000000000002E-2,0.13880000000000001]
["Resistor","R2, R32","1 MΩ",2,"0204/0207","LR0204F1M0","Farnell",2329894,3.5299999999999998E-2,7.0599999999999996E-2]
["Potentiometer","P1","100 kΩ log, Alpha 9 mm, right angled (side adjust)",1,null,"RD901F-20-15R1-A100K","Small Bear (US) or Thonk (EU)","100k-log-single",1.17,1.17]
["Trimmer","TR1","100 kΩ",{"$f":"IF(B36<>\"\",LEN(B36)-LEN(SUBSTITUTE(B36,\",\",\"\"))+1,\"\")","v":1},null,"PT 10 LH 100K","Mouser","531-PT10H-100K",0.50800000000000001,{"$f":"I36*D36","v":0.50800000000000001}]
["Jack","LINE-IN, MIC","6.35 mm jack",2,null,"ACJS-MHDR","Mouser","523-ACJS-MHDR",1.1599999999999999,{"$f":"I37*D37","v":2.3199999999999998}]
["Connector","AGC-L, EXC-L, AUDIO-L, EXP-L","Wire-to-board connector, 2-pin",4,null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,{"$f":"I38*D38","v":0.27279999999999999}]
["Connector","SUPPLY","Wire-to-board connector, 3-pin",1,null,"S3B-EH(LF)(SN)","Farnell",2481438,9.8599999999999993E-2,9.8599999999999993E-2]
["Connector",{"$f":"CONCATENATE(D40,\"x\")","v":"4x"},"EHR-2",{"$f":"D38","v":4},null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,0.12479999999999999]
["Connector",{"$f":"CONCATENATE(D41,\"x\")","v":"1x"},"EHR-3",{"$f":"D39","v":1},null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,3.4500000000000003E-2]
["Connector",{"$f":"CONCATENATE(D42,\"x\")","v":"11x"},"SEH-001T-P0.6",{"$f":"D40*2+D41*3","v":11},null,"SEH-001T-P0.6","Farnell",1863249,2.4400000000000002E-2,0.26840000000000003]
["IC Socket","IC1, IC2, IC3, IC5","8 pins",{"$f":"IF(B43<>\"\",LEN(B43)-LEN(SUBSTITUTE(B43,\",\",\"\"))+1,\"\")","v":4},null,"110-99-308-41-001000","Mouser","575-199308",0.38,{"$f":"I43*D43","v":1.52}]
["IC Socket","IC4","18 pins",{"$f":"IF(B44<>\"\",LEN(B44)-LEN(SUBSTITUTE(B44,\",\",\"\"))+1,\"\")","v":1},null,"110-44-318-41-001000","Mouser","575-11044318",0.79500000000000004,{"$f":"I44*D44","v":0.79500000000000004}]
["Misc","LEFT, GND","Solder pins,  ⌀ 1 mm",{"$f":"IF(B45<>\"\",LEN(B45)-LEN(SUBSTITUTE(B45,\",\",\"\"))+1,\"\")","v":2},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,{"$f":"I45*D45","v":5.1799999999999999E-2}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J45)","v":19.4087},"total"]

{"sheet":"Carrier preamp","index":5,"n_rows":47,"n_cols":11,"rows_kept":47,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Diode","D1, D2, D3, D4, D5, D6, D7, D8","1N4148",{"$f":"IF(B5<>\"\",LEN(B5)-LEN(SUBSTITUTE(B5,\",\",\"\"))+1,\"\")","v":8},"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,{"$f":"I5*D5","v":0.14399999999999999}]
["JFET","J1","J113",1,"TO-92","J113","Mouser","512-J113",0.249,0.249]
["LED","LED8, LED9, LED10, LED18, LED19, LED20","LED red, 2.4 V, 2 mA",6,"3 mm LED","TLLR4401","Mouser","78-TLLR4401",0.3,1.7999999999999998]
["LED","LED7, LED17","LED yellow, 2.4 V, 2 mA",2,"3 mm LED","TLLY4401","Mouser","78-TLLY4401",0.36699999999999999,0.73399999999999999]
["LED","LED1, LED2, LED3, LED4, LED5, LED6, LED11, LED12, LED13, LED14, LED15, LED16","LED green, 2.4 V, 2 mA",12,"3 mm LED","TLLG4401","Mouser","78-TLLG4401",0.3,3.5999999999999996]
["IC","IC1, IC2, IC3, IC6, IC7","NE5532",5,"DIL8","NE5532AP","Mouser","595-NE5532AP",0.81399999999999995,4.0699999999999994]
["IC","IC4, IC8","TL072",2,"DIL8","TL072IP","Mouser","595-TL072IP",0.59399999999999997,1.1879999999999999]
["IC","IC5, IC9","LM3916",2,"DIL18",{"$f":"C12","v":"LM3916"},null,"LM3916",1.98,3.96]
["Ceramic","C5, C6, C15, C16","22 pF",4,"RM2.5","K220J15C0GF53L2","Mouser","594-K220J15C0GF53L2",0.27100000000000002,1.0840000000000001]
["Ceramic","C22, C23, C24, C25, C26, C27, C28, C29, C30, C34, C35, C36, C37, C38, C39, C40","100 nF",16,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,0.38400000000000001]
["Ceramic","C19","10 nF",1,"RM2.5","K103K15X7RF53L2","Mouser","594-K103K15X7RF53L2",0.314,0.314]
["Film","C1, C11","100 nF",2,"RM2.5/RM5.0","R82EC3100AA70J","Mouser","80-R82EC3100AA70J",0.14099999999999999,0.28199999999999997]
["Film","C7, C17","220 nF",{"$f":"IF(B17<>\"\",LEN(B17)-LEN(SUBSTITUTE(B17,\",\",\"\"))+1,\"\")","v":2},"RM2.5/RM5.0","R82DC3220Z360K","Mouser","80-82DC3220Z360K",0.10299999999999999,0.20599999999999999]
["Film","C3, C4, C13, C14","1 µF",4,"RM2.5/RM5.0","R82DC4100Z360K","Mouser","80-R82DC4100Z360K",0.27900000000000003,1.1160000000000001]
["Electrolytic","C8, C18","3.3 µF/50 V, max. ⌀ 5 mm",2,"RM2.0","Würth 860020672007","Mouser","710-860020672007",0.1,0.2]
["Electrolytic","C2, C12","10 µF/50 V, max. ⌀ 5 mm",2,"RM2.0","Würth 860020672010","Mouser","710-860020672010",0.1,0.2]
["Electrolytic","C20, C21, C31, C32","100 µF/25 V, max. ⌀ 7 mm",4,"RM2.5","Würth 860010473007","Mouser","710-860010473007",0.111,0.44400000000000001]
["Resistor","R23, R24","47 Ω, 250 mW",2,"0204/0207","LR0204F47R","Farnell",2329945,4.0800000000000003E-2,8.1600000000000006E-2]
["Resistor","R20, R50","510 Ω",2,"0204/0207","LR0204F510R","Farnell",2329949,3.5299999999999998E-2,7.0599999999999996E-2]
["Resistor","R3, R33","1 kΩ",2,"0204/0207","LR0204F1K0","Farnell",2329885,7.7100000000000002E-2,0.1542]
["Resistor","R21, R51","7.5 kΩ",2,"0204/0207","LR0204F7K5","Farnell",2329974,8.1199999999999994E-2,0.16239999999999999]
["Resistor","R11, R41","10 kΩ",2,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,6.8000000000000005E-2]
["Resistor","R22, R52","15 kΩ",2,"0204/0207","LR0204F15K","Farnell",2329873,3.5299999999999998E-2,7.0599999999999996E-2]
["Resistor","R12, R42","22 kΩ",2,"0204/0207","LR0204F22K","Farnell",2329901,3.5999999999999997E-2,7.1999999999999995E-2]
[]
["Resistor","R13, R43","33 kΩ",{"$f":"IF(B30<>\"\",LEN(B30)-LEN(SUBSTITUTE(B30,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,{"$f":"I30*D30","v":7.0599999999999996E-2}]
["Resistor","R1, R5, R6, R7, R8, R9, R31, R35, R36, R37, R38, R39","47 kΩ",12,"0204/0207","LR0204F47K","Farnell",2329944,2.7E-2,0.32400000000000001]
["Resistor","R10, R14, R15, R16, R17, R25, R26, R40, R44, R45, R46, R47","100 kΩ",12,"0204/0207","LR0204F100K","Farnell",2329853,2.6499999999999999E-2,0.318]
["Resistor","R4, R18, R19, R34, R48, R49","200 kΩ",6,"0204/0207","LR0204F200K","Farnell",2329895,3.4700000000000002E-2,0.2082]
["Resistor","R2, R32","1 MΩ",2,"0204/0207","LR0204F1M0","Farnell",2329894,3.5299999999999998E-2,7.0599999999999996E-2]
["Potentiometer","P1","100 kΩ log, Alpha 9 mm, right angled (side adjust), stereo",1,null,"Alpha 9-PC-STE-100k log, RD902F-20-15R1-A100K","Small Bear (US) or banzaimusic.com (EU)","100k-log-dual",2.8,2.8]
["Trimmer","TR1, TR2","100 kΩ",2,null,"PT 10 LH 100K","Mouser","531-PT10H-100K",0.50800000000000001,{"$f":"I36*D36","v":1.016}]
["Jack","LINE-IN, MIC","6.35 mm jack",2,null,"ACJS-MHDR","Mouser","523-ACJS-MHDR",1.1599999999999999,{"$f":"I37*D37","v":2.3199999999999998}]
["Connector","AGC-L, EXC-L, AUDIO-L, EXP-L, AGC-R, EXC-R, AUDIO-R, EXP-R, INT-R, INT-L, MONO-SW","Wire-to-board connector, 2-pin",11,null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,{"$f":"I38*D38","v":0.75019999999999998}]
["Connector","SUPPLY","Wire-to-board connector, 3-pin",1,null,"S3B-EH(LF)(SN)","Farnell",2481438,9.8599999999999993E-2,{"$f":"I39*D39","v":9.8599999999999993E-2}]
["Connector",{"$f":"CONCATENATE(D40,\"x\")","v":"11x"},"EHR-2",{"$f":"D38","v":11},null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,0.34320000000000001]
["Connector",{"$f":"CONCATENATE(D41,\"x\")","v":"1x"},"EHR-3",{"$f":"D39","v":1},null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,3.4500000000000003E-2]
["Connector",{"$f":"CONCATENATE(D42,\"x\")","v":"25x"},"SEH-001T-P0.6",{"$f":"D40*2+D41*3","v":25},null,"SEH-001T-P0.6","Farnell",1863249,2.4400000000000002E-2,0.61]
["IC Socket","IC1, IC2, IC3, IC5, IC6, IC7","8 pins",{"$f":"IF(B43<>\"\",LEN(B43)-LEN(SUBSTITUTE(B43,\",\",\"\"))+1,\"\")","v":6},null,"110-99-308-41-001000","Mouser","575-199308",0.38,{"$f":"I43*D43","v":2.2800000000000002}]
["IC Socket","IC4, IC8","18 pins",{"$f":"IF(B44<>\"\",LEN(B44)-LEN(SUBSTITUTE(B44,\",\",\"\"))+1,\"\")","v":2},null,"110-44-318-41-001000","Mouser","575-11044318",0.79500000000000004,{"$f":"I44*D44","v":1.59}]
["Misc","LEFT, RIGHT, GND","Solder pins,  ⌀ 1 mm",{"$f":"IF(B45<>\"\",LEN(B45)-LEN(SUBSTITUTE(B45,\",\",\"\"))+1,\"\")","v":3},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,{"$f":"I45*D45","v":7.7699999999999991E-2}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J45)","v":33.566000000000003},"total"]

{"sheet":"Internal exc. (left)","index":6,"n_rows":84,"n_cols":11,"rows_kept":84,"cut":false,"hidden":false,"merged":[[0,0,1,3]]}
["Fewer components than \"internal exc. (right)\":  J4, J5, C18, R66, R67, R68, MIX-SW. Also notice the difference in MIX-IN1, MIX-IN2."]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Diode","D1, D2","1N4148",{"$f":"IF(B5<>\"\",LEN(B5)-LEN(SUBSTITUTE(B5,\",\",\"\"))+1,\"\")","v":2},"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,{"$f":"I5*D5","v":3.5999999999999997E-2}]
["JFET","J1","J105",1,"TO-92","J105","Mouser","512-J105",0.55300000000000005,0.55300000000000005]
["JFET","J2, J3","J113",2,"TO-92","J113","Mouser","512-J113",0.249,0.498]
["Transistor","T1, T2","2N3904",2,"TO-92","2N3904BU","Mouser","512-2N3904BU",5.0999999999999997E-2,0.10199999999999999]
["Transistor","T3","2N3906",1,"TO-92","2N3906BU","Mouser","512-2N3906BU",0.23599999999999999,0.23599999999999999]
["IC","IC1","TL072",1,"DIL8","TL072IP","Mouser","595-TL072IP",0.59399999999999997,0.59399999999999997]
["IC","IC3, IC5, IC7","TL074",3,"DIL14","TL074CN","Mouser","595-TL074CN",0.46800000000000003,1.4040000000000001]
["IC","IC2","THAT300",1,"DIL14","THAT300P14-U","Mouser","887-300P14-U",7.95,7.95]
["IC","IC6","LM13700",1,"DIL16","LM13700N","Mouser","926-LM13700N/NOPB",1.82,1.82]
["IC","IC4","LM319",1,"DIL14","LM319N","Mouser","512-LM319N",0.498,0.498]
["IC","IC8","NE5532",1,"DIL8","NE5532AP","Mouser","595-NE5532AP",0.81399999999999995,0.81399999999999995]
["Ceramic","C9","22 pF",1,"RM2.5","K220J15C0GF53L2","Mouser","594-K220J15C0GF53L2",0.27100000000000002,0.27100000000000002]
["Ceramic","C1, C6, C17","100 pF",3,"RM2.5","K101J15C0GF53L2","Mouser","594-K101J15C0GF53L2",8.6999999999999994E-2,0.26100000000000001]
["Ceramic","C16","220 pF",1,"RM2.5/RM5.0","C315C221M5R5TA","Mouser","80-C315C221M5R",0.27900000000000003,0.27900000000000003]
["Ceramic","C15","470 pF",1,"RM2.5/RM5.0","K471J15C0GF53L2","Mouser","594-K471J15C0GF53L2",0.105,0.105]
["Film","C14","1 nF",1,"RM2.5/RM5.0","R82EC1100AA50K","Mouser","80-R82EC1100AA50K",0.21,0.21]
["Film","C13","2.2 nF",1,"RM2.5/RM5.0","R82EC1220DQ50J","Mouser","80-R82EC1220DQ50J",0.26200000000000001,0.26200000000000001]
["Film","C12","4.7 nF",1,"RM2.5/RM5.0","R82EC1470CK50J","Mouser","80-R82EC1470CK50J",0.253,0.253]
[]
["Film","C11","10 nF",{"$f":"IF(B24<>\"\",LEN(B24)-LEN(SUBSTITUTE(B24,\",\",\"\"))+1,\"\")","v":1},"RM2.5/RM5.0","R82EC2100AA50J","Mouser","80-R82EC2100AA50J",0.218,{"$f":"I24*D24","v":0.218}]
["Film","C10","22 nF",{"$f":"IF(B25<>\"\",LEN(B25)-LEN(SUBSTITUTE(B25,\",\",\"\"))+1,\"\")","v":1},"RM2.5/RM5.0","R82EC2220AA50J","Mouser","80-R82EC2220AA50J",0.218,0.218]
["Film","C5","47 nF",{"$f":"IF(B26<>\"\",LEN(B26)-LEN(SUBSTITUTE(B26,\",\",\"\"))+1,\"\")","v":1},"RM2.5/RM5.0","R82EC2470AA60J","Mouser","80-R82EC2470AA60J",0.218,0.218]
["Film","C3, C8","100 nF",{"$f":"IF(B27<>\"\",LEN(B27)-LEN(SUBSTITUTE(B27,\",\",\"\"))+1,\"\")","v":2},"RM2.5/RM5.0","R82EC3100AA70J","Mouser","80-R82EC3100AA70J",0.14099999999999999,0.28199999999999997]
["Ceramic","C2, C22, C23, C26, C27, C28, C29, C32, C33, C34, C35, C38, C39, C42, C43","100 nF",15,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,0.36]
["Film","C4","1 µF",1,"RM2.5/RM5.0","R82DC4100Z360K","Mouser","80-R82DC4100Z360K",0.27900000000000003,0.27900000000000003]
["Electrolytic","C7","2.2 µF/25 V, max. ⌀ 5 mm",1,"RM2.0","Würth 860020672006","Mouser","710-860020672006",0.1,{"$f":"I30*D30","v":0.1}]
["Electrolytic","C20, C21, C24, C25, C30, C31, C36, C37, C40, C41","47 µF/35 V, max. ⌀ 5 mm",10,"RM2.0","Würth 860010572005","Mouser","710-860010572005",7.0999999999999994E-2,0.71]
["Tempco","R7","2 kΩ, 3300 ppm/°C",{"$f":"IF(B32<>\"\",LEN(B32)-LEN(SUBSTITUTE(B32,\",\",\"\"))+1,\"\")","v":1},null,null,"Thonk","tempco",1.61,{"$f":"I32*D32","v":1.61},"Akaneohm"]
["Resistor","R8, R69, R70, R71, R72, R73, R74, R75, R76, R77, R78, R82, R83","47 Ω, 250 mW",13,"0204/0207","LR0204F47R","Farnell",2329945,4.0800000000000003E-2,0.53039999999999998]
["Resistor","R41","430 Ω",1,"0204/0207","LR0204F430R","Farnell",2329938,3.7199999999999997E-2,3.7199999999999997E-2]
["Resistor","R40","470 Ω",1,"0204/0207","LR0204F470R","Farnell",2329942,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R9","820 Ω",1,"0204/0207","LR0204F820R","Farnell",2329976,7.7100000000000002E-2,7.7100000000000002E-2]
["Resistor","R34","1 kΩ",1,"0204/0207","LR0204F1K0","Farnell",2329885,7.7100000000000002E-2,7.7100000000000002E-2]
["Resistor","R6, R11","2.2 kΩ",{"$f":"IF(B38<>\"\",LEN(B38)-LEN(SUBSTITUTE(B38,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F2K2","Farnell",2329912,7.7100000000000002E-2,0.1542]
["Resistor","R60, R81","3.3 kΩ",{"$f":"IF(B39<>\"\",LEN(B39)-LEN(SUBSTITUTE(B39,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F3K3","Farnell",2329934,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R33, R44, R46, R59","4.7 kΩ",4,"0204/0207","LR0204F4K7","Farnell",2329947,3.5999999999999997E-2,0.14399999999999999]
["Resistor","R36, R37","5.6 kΩ",2,"0204/0207","LR0204F5K6","Farnell",2329958,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R58","10 kΩ",1,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,3.4000000000000002E-2]
["Resistor","R42","12 kΩ",{"$f":"IF(B43<>\"\",LEN(B43)-LEN(SUBSTITUTE(B43,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F12K","Farnell",2329863,3.5999999999999997E-2,{"$f":"I43*D43","v":3.5999999999999997E-2}]
["Resistor","R35, R43","15 kΩ",2,"0204/0207","LR0204F15K","Farnell",2329873,3.5299999999999998E-2,7.0599999999999996E-2]
["Resistor","R27, R28, R29","18 kΩ",3,"0204/0207","LR0204F18K","Farnell",2329882,3.5999999999999997E-2,0.10799999999999998]
["Resistor","R57","22 kΩ",1,"0204/0207","LR0204F22K","Farnell",2329901,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R50","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R17","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R30","36 kΩ",1,"0204/0207","LR0204F36K","Farnell",2329927,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R19, R47,  R56","47 kΩ",3,"0204/0207","LR0204F47K","Farnell",2329944,2.7E-2,8.1000000000000003E-2]
["Resistor","R14","56 kΩ",1,"0204/0207","LR0204F56K","Farnell",2329954,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R65","62 kΩ",{"$f":"IF(B52<>\"\",LEN(B52)-LEN(SUBSTITUTE(B52,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F62K","Farnell",2329961,7.7100000000000002E-2,{"$f":"I52*D52","v":7.7100000000000002E-2}]
["Resistor","R1, R2, R5, R16, R18, R21, R22, R23, R55, R61, R62, R63, R64, R80","100 kΩ",14,"0204/0207","LR0204F100K","Farnell",2329853,2.6499999999999999E-2,0.371]
["Resistor","R4, R20, R31","150 kΩ",3,"0204/0207","LR0204F150K","Farnell",2329871,3.5999999999999997E-2,{"$f":"I54*D54","v":0.10799999999999998}]
["Resistor","R12, R32, R54","220 kΩ",{"$f":"IF(B55<>\"\",LEN(B55)-LEN(SUBSTITUTE(B55,\",\",\"\"))+1,\"\")","v":3},"0204/0207","LR0204F220K","Farnell",2329899,3.5999999999999997E-2,0.10799999999999998]
["Resistor","R15","330 kΩ",1,"0204/0207","MFR3-330KFC","Farnell",1565303,4.2500000000000003E-2,4.2500000000000003E-2]
["Resistor","R13","390 kΩ",{"$f":"IF(B57<>\"\",LEN(B57)-LEN(SUBSTITUTE(B57,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F390K","Farnell",2329929,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R53","470 kΩ",{"$f":"IF(B58<>\"\",LEN(B58)-LEN(SUBSTITUTE(B58,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F470K","Farnell",2329941,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R24","820 kΩ",{"$f":"IF(B59<>\"\",LEN(B59)-LEN(SUBSTITUTE(B59,\",\",\"\"))+1,\"\")","v":1},"0204/0207","MRS25000C8203FCT00","Farnell",9470239,9.0999999999999998E-2,9.0999999999999998E-2]
["Resistor","R25, R26, R38, R39, R45, R48, R49, R51, R52","1 MΩ",9,"0204/0207","LR0204F1M0","Farnell",2329894,3.5299999999999998E-2,0.31769999999999998]
["Resistor","R10, R79","1.5 MΩ",{"$f":"IF(B61<>\"\",LEN(B61)-LEN(SUBSTITUTE(B61,\",\",\"\"))+1,\"\")","v":2},"0204/0207","MRS25000C1504FCT00","Farnell",9465537,5.2400000000000002E-2,0.1048]
["Resistor","R3","6.8 MΩ",1,"0204/0207","MRS25000C6804FCT00","Farnell",9469842,5.2900000000000003E-2,5.2900000000000003E-2]
["Potentiometer","P1, P2","100 kΩ lin, Alpha 9 mm, right angled (side adjust)",{"$f":"IF(B63<>\"\",LEN(B63)-LEN(SUBSTITUTE(B63,\",\",\"\"))+1,\"\")","v":2},null,"RD901F-20-15R1-B100K","Small Bear (US) or Thonk (EU)","100k-lin-single",1.38,{"$f":"I63*D63","v":2.76}]
["Potentiometer","P3, P4","100 kΩ log, Alpha 9 mm, right angled (side adjust)",{"$f":"IF(B64<>\"\",LEN(B64)-LEN(SUBSTITUTE(B64,\",\",\"\"))+1,\"\")","v":2},null,"RD901F-20-15R1-A100K","Small Bear (US) or Thonk (EU)","100k-log-single",1.17,{"$f":"I64*D64","v":2.34}]
["Trimmer, multi-turn","TR1, TR3","100 Ω",2,null,"T93XA101KT20","Mouser","72-T93XA-100",1.56,3.12]
["Trimmer, multi-turn","TR2","2.2 kΩ",1,null,"T93XA202KT20","Mouser","72-T93XA-2K",1.48,1.48]
["Trimmer, multi-turn","TR4","100 kΩ",1,null,"T93XA104KT20","Mouser","72-T93XA-100K",1.23,1.23]
["Trimmer","TR5","10 kΩ",1,null,"PT 10 LH 10K","Mouser","531-PT10H-10K",0.51800000000000002,0.51800000000000002]
["Trimmer","TR6, TR7, TR8, TR9","100 kΩ",4,null,"PT 10 LH 100K","Mouser","531-PT10H-100K",0.50800000000000001,2.032]
["Trimmer","TR10","250 kΩ",1,null,"PT 10 LH 250K","Mouser","531-PT10H-250K",0.50800000000000001,0.50800000000000001]
["Jack","CV-IN","3.5 mm jack",{"$f":"IF(B71<>\"\",LEN(B71)-LEN(SUBSTITUTE(B71,\",\",\"\"))+1,\"\")","v":1},null,"CL13845G","Farnell",2766196,1.26,2.2000000000000002]
["Connector","2x","2x2 board-to-board connector, angled, RM2.54 mm",2,null,"Würth 61300421021","Mouser","710-61300421021",0.39,{"$f":"I72*D72","v":0.78}]
["Connector","VUV-NSE, AGC, EXC-OUT, MIX-IN1, MIX-IN2","Wire-to-board connector, 2-pin",{"$f":"IF(B73<>\"\",LEN(B73)-LEN(SUBSTITUTE(B73,\",\",\"\"))+1,\"\")","v":5},null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,0.34099999999999997]
["Connector","SUPPLY, NOISE-SRC","Wire-to-board connector, 3-pin",2,null,"S3B-EH(LF)(SN)","Farnell",2481438,9.8599999999999993E-2,0.19719999999999999]
["Connector",{"$f":"CONCATENATE(D75, \"x\")","v":"5x"},"EHR-2",{"$f":"D73","v":5},null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,0.156]
["Connector",{"$f":"CONCATENATE(D76, \"x\")","v":"2x"},"EHR-3",{"$f":"D74","v":2},null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,6.9000000000000006E-2]
["Connector",{"$f":"CONCATENATE(D77, \"x\")","v":"16x"},"SEH-001T-P0.6",{"$f":"D75*2+D76*3","v":16},null,"SEH-001T-P0.6","Farnell",1863249,2.4400000000000002E-2,0.39040000000000002]
["Connector","2x","Jumper",2,null,"M7582-05","Mouser","855-M7582-05",9.7000000000000003E-2,0.19400000000000001]
["IC Socket","IC1, IC8","8 pins",{"$f":"IF(B79<>\"\",LEN(B79)-LEN(SUBSTITUTE(B79,\",\",\"\"))+1,\"\")","v":2},null,"110-99-308-41-001000","Mouser","575-199308",0.38,{"$f":"I79*D79","v":0.76}]
["IC Socket","IC2, IC3, IC4, IC5, IC7","14 pins",{"$f":"IF(B80<>\"\",LEN(B80)-LEN(SUBSTITUTE(B80,\",\",\"\"))+1,\"\")","v":5},null,"110-99-314-41-001000","Mouser","575-199314",0.49299999999999999,2.4649999999999999]
["IC Socket","IC6","16 pins",{"$f":"IF(B81<>\"\",LEN(B81)-LEN(SUBSTITUTE(B81,\",\",\"\"))+1,\"\")","v":1},null,"110-99-316-41-001000","Mouser","575-199316",0.42799999999999999,0.42799999999999999]
["Misc","AGCO, GND, PNK, SAW, WHT, SQR","Solder pins,  ⌀ 1 mm",{"$f":"IF(B82<>\"\",LEN(B82)-LEN(SUBSTITUTE(B82,\",\",\"\"))+1,\"\")","v":6},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,{"$f":"I82*D82","v":0.15539999999999998}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J82)","v":45.31750000000001},"total"]

{"sheet":"Internal exc. (right)","index":7,"n_rows":84,"n_cols":11,"rows_kept":84,"cut":false,"hidden":false,"merged":[[0,0,1,2]]}
["Note: this board is populated with the mixing circuitry, so it's different from its sibling \"Internal exc. (left)\""]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Diode","D1, D2","1N4148",{"$f":"IF(B5<>\"\",LEN(B5)-LEN(SUBSTITUTE(B5,\",\",\"\"))+1,\"\")","v":2},"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,{"$f":"I5*D5","v":3.5999999999999997E-2}]
["JFET","J1","J105",{"$f":"IF(B6<>\"\",LEN(B6)-LEN(SUBSTITUTE(B6,\",\",\"\"))+1,\"\")","v":1},"TO-92","J105","Mouser","512-J105",0.55300000000000005,{"$f":"I6*D6","v":0.55300000000000005}]
["JFET","J2, J3, J4, J5","J113",{"$f":"IF(B7<>\"\",LEN(B7)-LEN(SUBSTITUTE(B7,\",\",\"\"))+1,\"\")","v":4},"TO-92","J113","Mouser","512-J113",0.249,{"$f":"I7*D7","v":0.996}]
["Transistor","T1, T2","2N3904",{"$f":"IF(B8<>\"\",LEN(B8)-LEN(SUBSTITUTE(B8,\",\",\"\"))+1,\"\")","v":2},"TO-92","2N3904BU","Mouser","512-2N3904BU",5.0999999999999997E-2,0.10199999999999999]
["Transistor","T3","2N3906",1,"TO-92","2N3906BU","Mouser","512-2N3906BU",0.23599999999999999,0.23599999999999999]
["IC","IC1","TL072",{"$f":"IF(B10<>\"\",LEN(B10)-LEN(SUBSTITUTE(B10,\",\",\"\"))+1,\"\")","v":1},"DIL8","TL072IP","Mouser","595-TL072IP",0.59399999999999997,{"$f":"I10*D10","v":0.59399999999999997}]
["IC","IC3, IC5, IC7","TL074",3,"DIL14","TL074CN","Mouser","595-TL074CN",0.46800000000000003,1.4040000000000001]
["IC","IC2","THAT300",1,"DIL14","THAT300P14-U","Mouser","887-300P14-U",7.95,7.95]
["IC","IC6","LM13700",1,"DIL16","LM13700N","Mouser","926-LM13700N/NOPB",1.82,1.82]
["IC","IC4","LM319",1,"DIL14","LM319N","Mouser","512-LM319N",0.498,0.498]
["IC","IC8","NE5532",1,"DIL8","NE5532AP","Mouser","595-NE5532AP",0.81399999999999995,0.81399999999999995]
["Ceramic","C9","22 pF",1,"RM2.5","K220J15C0GF53L2","Mouser","594-K220J15C0GF53L2",0.27100000000000002,0.27100000000000002]
["Ceramic","C1, C6, C17","100 pF",3,"RM2.5","K101J15C0GF53L2","Mouser","594-K101J15C0GF53L2",8.6999999999999994E-2,0.26100000000000001]
["Ceramic","C16","220 pF",1,"RM2.5/RM5.0","C315C221M5R5TA","Mouser","80-C315C221M5R",0.27900000000000003,0.27900000000000003]
["Ceramic","C15","470 pF",1,"RM2.5/RM5.0","K471J15C0GF53L2","Mouser","594-K471J15C0GF53L2",0.105,0.105]
["Film","C14","1 nF",1,"RM2.5/RM5.0","R82EC1100AA50K","Mouser","80-R82EC1100AA50K",0.21,0.21]
["Film","C13","2.2 nF",1,"RM2.5/RM5.0","R82EC1220DQ50J","Mouser","80-R82EC1220DQ50J",0.26200000000000001,0.26200000000000001]
["Film","C12","4.7 nF",1,"RM2.5/RM5.0","R82EC1470CK50J","Mouser","80-R82EC1470CK50J",0.253,0.253]
["Ceramic","C18","10 nF",{"$f":"IF(B23<>\"\",LEN(B23)-LEN(SUBSTITUTE(B23,\",\",\"\"))+1,\"\")","v":1},"RM2.5","K103K15X7RF53L2","Mouser","594-K103K15X7RF53L2",0.314,{"$f":"I23*D23","v":0.314}]
["Film","C11","10 nF",1,"RM2.5/RM5.0","R82EC2100AA50J","Mouser","80-R82EC2100AA50J",0.218,0.218]
["Film","C10","22 nF",1,"RM2.5/RM5.0","R82EC2220AA50J","Mouser","80-R82EC2220AA50J",0.218,0.218]
["Film","C5","47 nF",1,"RM2.5/RM5.0","R82EC2470AA60J","Mouser","80-R82EC2470AA60J",0.218,0.218]
["Film","C3, C8","100 nF",2,"RM2.5/RM5.0","R82EC3100AA70J","Mouser","80-R82EC3100AA70J",0.14099999999999999,0.28199999999999997]
["Ceramic","C2, C22, C23, C26, C27, C28, C29, C32, C33, C34, C35, C38, C39, C42, C43","100 nF",15,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,0.36]
["Film","C4","1 µF",1,"RM2.5/RM5.0","R82DC4100Z360K","Mouser","80-R82DC4100Z360K",0.27900000000000003,0.27900000000000003]
["Electrolytic","C7","2.2 µF/25 V, max. ⌀ 5 mm",1,"RM2.0","Würth 860020672006","Mouser","710-860020672006",0.1,0.1]
["Electrolytic","C20, C21, C24, C25, C30, C31, C36, C37, C40, C41","47 µF/35 V, max. ⌀ 5 mm",10,"RM2.0","Würth 860010572005","Mouser","710-860010572005",7.0999999999999994E-2,0.71]
["Tempco","R7","2 kΩ, 3300 ppm/°C",{"$f":"IF(B32<>\"\",LEN(B32)-LEN(SUBSTITUTE(B32,\",\",\"\"))+1,\"\")","v":1},null,null,"Thonk","tempco",1.61,1.61,"Akaneohm"]
["Resistor","R8, R69, R70, R71, R72, R73, R74, R75, R76, R77, R78, R82, R83","47 Ω, 250 mW",13,"0204/0207","LR0204F47R","Farnell",2329945,4.0800000000000003E-2,0.53039999999999998]
["Resistor","R41","430 Ω",1,"0204/0207","LR0204F430R","Farnell",2329938,3.7199999999999997E-2,3.7199999999999997E-2]
["Resistor","R40","470 Ω",1,"0204/0207","LR0204F470R","Farnell",2329942,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R9","820 Ω",1,"0204/0207","LR0204F820R","Farnell",2329976,7.7100000000000002E-2,7.7100000000000002E-2]
["Resistor","R34","1 kΩ",1,"0204/0207","LR0204F1K0","Farnell",2329885,7.7100000000000002E-2,7.7100000000000002E-2]
["Resistor","R6, R11","2.2 kΩ",{"$f":"IF(B38<>\"\",LEN(B38)-LEN(SUBSTITUTE(B38,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F2K2","Farnell",2329912,7.7100000000000002E-2,0.1542]
["Resistor","R60, R81","3.3 kΩ",{"$f":"IF(B39<>\"\",LEN(B39)-LEN(SUBSTITUTE(B39,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F3K3","Farnell",2329934,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R33, R44, R46, R59","4.7 kΩ",4,"0204/0207","LR0204F4K7","Farnell",2329947,3.5999999999999997E-2,0.14399999999999999]
["Resistor","R36, R37","5.6 kΩ",2,"0204/0207","LR0204F5K6","Farnell",2329958,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R58","10 kΩ",1,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,3.4000000000000002E-2]
["Resistor","R42","12 kΩ",{"$f":"IF(B43<>\"\",LEN(B43)-LEN(SUBSTITUTE(B43,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F12K","Farnell",2329863,3.5999999999999997E-2,{"$f":"I43*D43","v":3.5999999999999997E-2}]
["Resistor","R35, R43","15 kΩ",2,"0204/0207","LR0204F15K","Farnell",2329873,3.5299999999999998E-2,7.0599999999999996E-2]
["Resistor","R27, R28, R29","18 kΩ",3,"0204/0207","LR0204F18K","Farnell",2329882,3.5999999999999997E-2,0.10799999999999998]
["Resistor","R57","22 kΩ",1,"0204/0207","LR0204F22K","Farnell",2329901,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R50","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R17","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R30","36 kΩ",1,"0204/0207","LR0204F36K","Farnell",2329927,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R19, R47,  R56","47 kΩ",3,"0204/0207","LR0204F47K","Farnell",2329944,2.7E-2,8.1000000000000003E-2]
["Resistor","R14","56 kΩ",1,"0204/0207","LR0204F56K","Farnell",2329954,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R65","62 kΩ",{"$f":"IF(B52<>\"\",LEN(B52)-LEN(SUBSTITUTE(B52,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F62K","Farnell",2329961,7.7100000000000002E-2,{"$f":"I52*D52","v":7.7100000000000002E-2}]
["Resistor","R1, R2, R5, R16, R18, R21, R22, R23, R55, R61, R62, R63, R64, R80","100 kΩ",14,"0204/0207","LR0204F100K","Farnell",2329853,2.6499999999999999E-2,0.371]
["Resistor","R4, R20, R31","150 kΩ",3,"0204/0207","LR0204F150K","Farnell",2329871,3.5999999999999997E-2,0.10799999999999998]
["Resistor","R12, R32, R54, R66, R67, R68","220 kΩ",{"$f":"IF(B55<>\"\",LEN(B55)-LEN(SUBSTITUTE(B55,\",\",\"\"))+1,\"\")","v":6},"0204/0207","LR0204F220K","Farnell",2329899,3.5999999999999997E-2,0.21599999999999997]
["Resistor","R15","330 kΩ",1,"0204/0207","MFR3-330KFC","Farnell",1565303,4.2500000000000003E-2,4.2500000000000003E-2]
["Resistor","R13","390 kΩ",{"$f":"IF(B57<>\"\",LEN(B57)-LEN(SUBSTITUTE(B57,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F390K","Farnell",2329929,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R53","470 kΩ",{"$f":"IF(B58<>\"\",LEN(B58)-LEN(SUBSTITUTE(B58,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F470K","Farnell",2329941,3.5999999999999997E-2,{"$f":"I58*D58","v":3.5999999999999997E-2}]
["Resistor","R24","820 kΩ",{"$f":"IF(B59<>\"\",LEN(B59)-LEN(SUBSTITUTE(B59,\",\",\"\"))+1,\"\")","v":1},"0204/0207","MRS25000C8203FCT00","Farnell",9470239,9.0999999999999998E-2,9.0999999999999998E-2]
["Resistor","R25, R26, R38, R39, R45, R48, R49, R51, R52","1 MΩ",9,"0204/0207","LR0204F1M0","Farnell",2329894,3.5299999999999998E-2,0.31769999999999998]
["Resistor","R10, R79","1.5 MΩ",2,"0204/0207","MRS25000C1504FCT00","Farnell",9465537,5.2400000000000002E-2,0.1048]
["Resistor","R3","6.8 MΩ",1,"0204/0207","MRS25000C6804FCT00","Farnell",9469842,5.2900000000000003E-2,5.2900000000000003E-2]
["Potentiometer","P1, P2","100 kΩ lin, Alpha 9 mm, right angled (side adjust)",{"$f":"IF(B63<>\"\",LEN(B63)-LEN(SUBSTITUTE(B63,\",\",\"\"))+1,\"\")","v":2},null,"RD901F-20-15R1-B100K","Small Bear (US) or Thonk (EU)","100k-lin-single",1.38,{"$f":"I63*D63","v":2.76}]
["Potentiometer","P3, P4","100 kΩ log, Alpha 9 mm, right angled (side adjust)",{"$f":"IF(B64<>\"\",LEN(B64)-LEN(SUBSTITUTE(B64,\",\",\"\"))+1,\"\")","v":2},null,"RD901F-20-15R1-A100K","Small Bear (US) or Thonk (EU)","100k-log-single",1.17,{"$f":"I64*D64","v":2.34}]
["Trimmer, multi-turn","TR1, TR3","100 Ω",2,null,"T93XA101KT20","Mouser","72-T93XA-100",1.56,3.12]
["Trimmer, multi-turn","TR2","2.2 kΩ",1,null,"T93XA202KT20","Mouser","72-T93XA-2K",1.48,1.48]
["Trimmer, multi-turn","TR4","100 kΩ",1,null,"T93XA104KT20","Mouser","72-T93XA-100K",1.23,1.23]
["Trimmer","TR5","10 kΩ",1,null,"PT 10 LH 10K","Mouser","531-PT10H-10K",0.51800000000000002,0.51800000000000002]
["Trimmer","TR6, TR7, TR8, TR9","100 kΩ",4,null,"PT 10 LH 100K","Mouser","531-PT10H-100K",0.50800000000000001,2.032]
["Trimmer","TR10","250 kΩ",1,null,"PT 10 LH 250K","Mouser","531-PT10H-250K",0.50800000000000001,0.50800000000000001]
["Jack","CV-IN","3.5 mm jack",{"$f":"IF(B71<>\"\",LEN(B71)-LEN(SUBSTITUTE(B71,\",\",\"\"))+1,\"\")","v":1},null,"CL13845G","Farnell",2766196,1.26,1.26]
["Connector","2x","2x2 board-to-board connector, angled, RM2.54 mm",2,null,"Würth 61300421021","Mouser","710-61300421021",0.39,{"$f":"I72*D72","v":0.78}]
["Connector","VUV-NSE, AGC, EXC-OUT, MIX-SW, MIX-OUT1, MIX-OUT2","Wire-to-board connector, 2-pin",{"$f":"IF(B73<>\"\",LEN(B73)-LEN(SUBSTITUTE(B73,\",\",\"\"))+1,\"\")","v":6},null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,0.40920000000000001]
["Connector","SUPPLY, NOISE-SRC","Wire-to-board connector, 3-pin",2,null,"S3B-EH(LF)(SN)","Farnell",2481438,9.8599999999999993E-2,0.19719999999999999]
["Connector",{"$f":"CONCATENATE(D75, \"x\")","v":"6x"},"EHR-2",{"$f":"D73","v":6},null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,0.18719999999999998]
["Connector",{"$f":"CONCATENATE(D76, \"x\")","v":"2x"},"EHR-3",{"$f":"IF(B74<>\"\",LEN(B74)-LEN(SUBSTITUTE(B74,\",\",\"\"))+1,\"\")","v":2},null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,6.9000000000000006E-2]
["Connector",{"$f":"CONCATENATE(D77, \"x\")","v":"18x"},"SEH-001T-P0.6",{"$f":"D75*2+D76*3","v":18},null,"SEH-001T-P0.6","Farnell",1863249,2.4400000000000002E-2,0.43920000000000003]
["Connector","2x","Jumper",2,null,"M7582-05","Mouser","855-M7582-05",9.7000000000000003E-2,0.19400000000000001]
["IC Socket","IC1, IC8","8 pins",2,null,"110-99-308-41-001000","Mouser","575-199308",0.38,0.76]
["IC Socket","IC2, IC3, IC4, IC5, IC7","14 pins",5,null,"110-99-314-41-001000","Mouser","575-199314",0.49299999999999999,2.4649999999999999]
["IC Socket","IC6","16 pins",1,null,"110-99-316-41-001000","Mouser","575-199316",0.42799999999999999,0.42799999999999999]
["Misc","AGCO, GND, PNK, SAW, WHT, SQR","Solder pins,  ⌀ 1 mm",{"$f":"IF(B82<>\"\",LEN(B82)-LEN(SUBSTITUTE(B82,\",\",\"\"))+1,\"\")","v":6},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,{"$f":"I82*D82","v":0.15539999999999998}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J82)","v":45.445700000000002},"total"]

{"sheet":"VUV detector","index":8,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Diode","D1, D2, D3, D4, D5, D6, D7, D8, D9, D10, D11, D12","1N4148",{"$f":"IF(B5<>\"\",LEN(B5)-LEN(SUBSTITUTE(B5,\",\",\"\"))+1,\"\")","v":12},"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,{"$f":"I5*D5","v":0.21599999999999997}]
["JFET","J1, J2, J3, J4","J113",{"$f":"IF(B6<>\"\",LEN(B6)-LEN(SUBSTITUTE(B6,\",\",\"\"))+1,\"\")","v":4},"TO-92","J113","Mouser","512-J113",0.249,{"$f":"I6*D6","v":0.996}]
["Transistor","T1, T2","2N3904",{"$f":"IF(B7<>\"\",LEN(B7)-LEN(SUBSTITUTE(B7,\",\",\"\"))+1,\"\")","v":2},"TO-92","2N3904BU","Mouser","512-2N3904BU",5.0999999999999997E-2,0.10199999999999999]
["IC","IC1","TL072",{"$f":"IF(B8<>\"\",LEN(B8)-LEN(SUBSTITUTE(B8,\",\",\"\"))+1,\"\")","v":1},"DIL8","TL072IP","Mouser","595-TL072IP",0.59399999999999997,{"$f":"I8*D8","v":0.59399999999999997}]
["IC","IC2, IC3, IC4, IC5","TL074",{"$f":"IF(B9<>\"\",LEN(B9)-LEN(SUBSTITUTE(B9,\",\",\"\"))+1,\"\")","v":4},"DIL14","TL074CN","Mouser","595-TL074CN",0.46800000000000003,{"$f":"I9*D9","v":1.8720000000000001}]
["IC","IC6","NE5532",{"$f":"IF(B10<>\"\",LEN(B10)-LEN(SUBSTITUTE(B10,\",\",\"\"))+1,\"\")","v":1},"DIL8","NE5532AP","Mouser","595-NE5532AP",0.81399999999999995,0.81399999999999995]
["IC","IC7","CD4093",1,"DIL14","CD4093BE","Mouser","595-CD4093BE",0.42799999999999999,0.42799999999999999]
["IC","IC8","CD40106",{"$f":"IF(B12<>\"\",LEN(B12)-LEN(SUBSTITUTE(B12,\",\",\"\"))+1,\"\")","v":1},"DIL14","CD40106BE","Mouser","595-CD40106BE",0.44500000000000001,{"$f":"I12*D12","v":0.44500000000000001}]
["Ceramic","C26, C27","100 pF",{"$f":"IF(B13<>\"\",LEN(B13)-LEN(SUBSTITUTE(B13,\",\",\"\"))+1,\"\")","v":2},"RM2.5","K101J15C0GF53L2","Mouser","594-K101J15C0GF53L2",8.6999999999999994E-2,{"$f":"I13*D13","v":0.17399999999999999}]
["Ceramic","C22, C23, C24, C25","1.5 nF",4,"RM2.5","C315C152K1R5TA","Mouser","80-C315C152K1R",0.30599999999999999,1.224]
["Film","C1, C2, C3","10 nF",3,"RM2.5/RM5.0","R82EC2100AA50J","Mouser","80-R82EC2100AA50J",0.218,0.65400000000000003]
["Ceramic","C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16, C17, C18, C19, C20, C21, C30, C31, C34, C35, C38, C39, C40, C41, C42, C43, C44, C45, C47, C48","100 nF",32,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,0.76800000000000002]
["Electrolytic","C46","22 µF/25 V, max. ⌀ 5 mm",{"$f":"IF(B17<>\"\",LEN(B17)-LEN(SUBSTITUTE(B17,\",\",\"\"))+1,\"\")","v":1},"RM2.0","Würth 860010572003","Mouser","710-860010572003",8.8999999999999996E-2,8.8999999999999996E-2]
["Electrolytic","C28, C29, C32, C33","47 µF/35 V, max. ⌀ 5 mm",4,"RM2.0","Würth 860010572005","Mouser","710-860010572005",7.0999999999999994E-2,0.28399999999999997]
["Electrolytic","C36, C37","100 µF/25 V, max. ⌀ 7 mm",{"$f":"IF(B19<>\"\",LEN(B19)-LEN(SUBSTITUTE(B19,\",\",\"\"))+1,\"\")","v":2},"RM2.5","Würth 860010473007","Mouser","710-860010473007",0.111,{"$f":"I19*D19","v":0.222}]
["Resistor","R76, R77, R78, R79, R80, R81, R82","47 Ω, 250 mW",{"$f":"IF(B20<>\"\",LEN(B20)-LEN(SUBSTITUTE(B20,\",\",\"\"))+1,\"\")","v":7},"0204/0207","LR0204F47R","Farnell",2329945,4.0800000000000003E-2,0.28560000000000002]
["Resistor","R49","100 Ω",{"$f":"IF(B21<>\"\",LEN(B21)-LEN(SUBSTITUTE(B21,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F100R","Farnell",2329854,3.5999999999999997E-2,{"$f":"I21*D21","v":3.5999999999999997E-2}]
["Resistor","R5, R23","1.5 kΩ",{"$f":"IF(B22<>\"\",LEN(B22)-LEN(SUBSTITUTE(B22,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F1K5","Farnell",2329891,7.5700000000000003E-2,{"$f":"I22*D22","v":0.15140000000000001}]
["Resistor","R73, R75","2.2 kΩ",{"$f":"IF(B23<>\"\",LEN(B23)-LEN(SUBSTITUTE(B23,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F2K2","Farnell",2329912,7.7100000000000002E-2,0.1542]
["Resistor","R3","3.9 kΩ",{"$f":"IF(B24<>\"\",LEN(B24)-LEN(SUBSTITUTE(B24,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F3K9","Farnell",2329936,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R13, R36, R46","4.7 kΩ",{"$f":"IF(B25<>\"\",LEN(B25)-LEN(SUBSTITUTE(B25,\",\",\"\"))+1,\"\")","v":3},"0204/0207","LR0204F4K7","Farnell",2329947,3.5999999999999997E-2,0.10799999999999998]
["Resistor","R21, R22","5.6 kΩ",{"$f":"IF(B26<>\"\",LEN(B26)-LEN(SUBSTITUTE(B26,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F5K6","Farnell",2329958,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R19","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R14, R34, R47","8.2 kΩ",3,"0204/0207","LR0204F8K2","Farnell",2329981,3.5999999999999997E-2,0.10799999999999998]
["Resistor","R1, R15, R16, R24, R25, R35, R48, R58, R59, R60, R61, R62, R63, R64, R65, R71","10 kΩ",{"$f":"IF(B29<>\"\",LEN(B29)-LEN(SUBSTITUTE(B29,\",\",\"\"))+1,\"\")","v":16},"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,0.54400000000000004]
["Resistor","R33","12 kΩ",{"$f":"IF(B30<>\"\",LEN(B30)-LEN(SUBSTITUTE(B30,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F12K","Farnell",2329863,3.5999999999999997E-2,{"$f":"I30*D30","v":3.5999999999999997E-2}]
["Resistor","R11, R12, R18, R44, R45","15 kΩ",5,"0204/0207","LR0204F15K","Farnell",2329873,3.5299999999999998E-2,0.17649999999999999]
["Resistor","R66, R67","20 kΩ",{"$f":"IF(B32<>\"\",LEN(B32)-LEN(SUBSTITUTE(B32,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,7.0599999999999996E-2]
["Resistor","R2, R17","22 kΩ",{"$f":"IF(B33<>\"\",LEN(B33)-LEN(SUBSTITUTE(B33,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F22K","Farnell",2329901,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R4, R50","27 kΩ",{"$f":"IF(B34<>\"\",LEN(B34)-LEN(SUBSTITUTE(B34,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F27K","Farnell",2329909,3.5299999999999998E-2,7.0599999999999996E-2]
["Resistor","R31, R32","36 kΩ",{"$f":"IF(B35<>\"\",LEN(B35)-LEN(SUBSTITUTE(B35,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F36K","Farnell",2329927,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R72, R74","47 kΩ",2,"0204/0207","LR0204F47K","Farnell",2329944,2.7E-2,5.3999999999999999E-2]
["Resistor","R6, R7, R8, R9, R10, R20, R26, R27, R28, R29, R30, R38, R39, R40, R41, R42, R43, R52, R53, R68, R69, R70","100 kΩ",{"$f":"IF(B37<>\"\",LEN(B37)-LEN(SUBSTITUTE(B37,\",\",\"\"))+1,\"\")","v":22},"0204/0207","LR0204F100K","Farnell",2329853,2.6499999999999999E-2,0.58299999999999996]
["Resistor","R51","330 kΩ",{"$f":"IF(B38<>\"\",LEN(B38)-LEN(SUBSTITUTE(B38,\",\",\"\"))+1,\"\")","v":1},"0204/0207","MFR3-330KFC","Farnell",1565303,4.2500000000000003E-2,4.2500000000000003E-2]
["Resistor","R54, R55, R56, R57","1 MΩ",{"$f":"IF(B39<>\"\",LEN(B39)-LEN(SUBSTITUTE(B39,\",\",\"\"))+1,\"\")","v":4},"0204/0207","LR0204F1M0","Farnell",2329894,3.5299999999999998E-2,0.14119999999999999]
["Resistor","R37","2.2 MΩ, 5%",{"$f":"IF(B40<>\"\",LEN(B40)-LEN(SUBSTITUTE(B40,\",\",\"\"))+1,\"\")","v":1},"0204/0207","CFR16J2M2","Farnell",2329510,2.46E-2,2.46E-2]
["Trimmer","TR2","10 kΩ",{"$f":"IF(B41<>\"\",LEN(B41)-LEN(SUBSTITUTE(B41,\",\",\"\"))+1,\"\")","v":1},null,"PT 10 LV 10K","Mouser","531-PT10V-10K",0.52900000000000003,{"$f":"I41*D41","v":0.52900000000000003}]
["Trimmer","TR1","100 kΩ",{"$f":"IF(B42<>\"\",LEN(B42)-LEN(SUBSTITUTE(B42,\",\",\"\"))+1,\"\")","v":1},null,"PT 10 LV 100K","Mouser","531-PT10V-100K",0.51800000000000002,{"$f":"I42*D42","v":0.51800000000000002}]
["Connector","VOICE, NOISE-L, NOISE-R, EXC-L, EXC-R, MIX-L, MIX-R, NOISE-INH, NOISE-INH, VOICED-LED, UNVOICED-LED","Wire-to-board connector, 2-pin",11,null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,0.75019999999999998]
["Connector","SUPPLY, FORCED-VUV-SW","Wire-to-board connector, 3-pin",{"$f":"IF(B44<>\"\",LEN(B44)-LEN(SUBSTITUTE(B44,\",\",\"\"))+1,\"\")","v":2},null,"S3B-EH(LF)(SN)","Farnell",2481438,9.8599999999999993E-2,0.19719999999999999]
["Connector",{"$f":"CONCATENATE(D45, \"x\")","v":"11x"},"EHR-2",{"$f":"D43","v":11},null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,0.34320000000000001]
["Connector",{"$f":"CONCATENATE(D46, \"x\")","v":"2x"},"EHR-3",{"$f":"D44","v":2},null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,6.9000000000000006E-2]
["Connector",{"$f":"CONCATENATE(D47, \"x\")","v":"28x"},"SEH-001T-P0.6",{"$f":"D45*2+D46*3","v":28},null,"SEH-001T-P0.6","Farnell",1863249,2.4400000000000002E-2,0.68320000000000003]
["IC Socket","IC1, IC6","8 pins",{"$f":"IF(B48<>\"\",LEN(B48)-LEN(SUBSTITUTE(B48,\",\",\"\"))+1,\"\")","v":2},null,"110-99-308-41-001000","Mouser","575-199308",0.38,0.76]
["IC Socket","IC2, IC3, IC4, IC5, IC7, IC8","14 pins",{"$f":"IF(B49<>\"\",LEN(B49)-LEN(SUBSTITUTE(B49,\",\",\"\"))+1,\"\")","v":6},null,"110-99-314-41-001000","Mouser","575-199314",0.49299999999999999,2.9580000000000002]
["Misc","GND, MIX-L, MIX-R","Solder pins,  ⌀ 1 mm",{"$f":"IF(B50<>\"\",LEN(B50)-LEN(SUBSTITUTE(B50,\",\",\"\"))+1,\"\")","v":3},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,{"$f":"I50*D50","v":7.7699999999999991E-2}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J51)","v":18.641000000000002},"total"]

{"sheet":"Output, PWM, bridging","index":9,"n_rows":69,"n_cols":11,"rows_kept":69,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Diode","D1, D2, D3, D4","1N4148",{"$f":"IF(B5<>\"\",LEN(B5)-LEN(SUBSTITUTE(B5,\",\",\"\"))+1,\"\")","v":4},"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,{"$f":"I5*D5","v":7.1999999999999995E-2}]
["Diode","D5","1N4001",1,"DO-41","1N4001RLG","Mouser","863-1N4001RLG",0.183,0.183]
["LED","LED1","LED red, 2.4 V, 2 mA",{"$f":"IF(B7<>\"\",LEN(B7)-LEN(SUBSTITUTE(B7,\",\",\"\"))+1,\"\")","v":1},"3 mm LED","TLLR4401","Mouser","78-TLLR4401",0.3,{"$f":"I7*D7","v":0.3}]
["JFET","J1, J2, J3, J4","J113",{"$f":"IF(B8<>\"\",LEN(B8)-LEN(SUBSTITUTE(B8,\",\",\"\"))+1,\"\")","v":4},"TO-92","J113","Mouser","512-J113",0.249,0.996]
["IC","IC8, IC10","LM319",2,"DIL14","LM319N","Mouser","512-LM319N",0.498,0.996]
["IC","IC1, IC2, IC3, IC4, IC5, IC6","NE5532",6,"DIL8","NE5532AP","Mouser","595-NE5532AP",0.81399999999999995,4.8839999999999995]
["IC","IC7, IC16","TL072",2,"DIL8","TL072IP","Mouser","595-TL072IP",0.59399999999999997,1.1879999999999999]
["IC","IC14, IC15","TL074",2,"DIL14","TL074CN","Mouser","595-TL074CN",0.46800000000000003,0.93600000000000005]
["IC","IC11","CD40106",{"$f":"IF(B13<>\"\",LEN(B13)-LEN(SUBSTITUTE(B13,\",\",\"\"))+1,\"\")","v":1},"DIL14","CD40106BE","Mouser","595-CD40106BE",0.44500000000000001,{"$f":"I13*D13","v":0.44500000000000001}]
["IC","IC9","CD4050",{"$f":"IF(B14<>\"\",LEN(B14)-LEN(SUBSTITUTE(B14,\",\",\"\"))+1,\"\")","v":1},"DIL16","CD4050BE","Mouser","595-CD4050BE",0.46300000000000002,{"$f":"I14*D14","v":0.46300000000000002}]
["IC","IC12","78L05",{"$f":"IF(B15<>\"\",LEN(B15)-LEN(SUBSTITUTE(B15,\",\",\"\"))+1,\"\")","v":1},"TO-92","LM78L05ACZXA","Mouser","511-L78L05ACZ",0.33200000000000002,{"$f":"I15*D15","v":0.33200000000000002}]
["IC","IC13","79L05",1,"TO-92","LM79L05ACZ","Mouser","511-L79L05ACZ",0.35799999999999998,{"$f":"I16*D16","v":0.35799999999999998}]
["Ceramic","C1, C2, C3, C4, C5, C6, C11, C12, C14","22 pF",9,"RM2.5","K220J15C0GF53L2","Mouser","594-K220J15C0GF53L2",0.27100000000000002,{"$f":"I17*D17","v":2.4390000000000001}]
["Ceramic","C19","100 pF",{"$f":"IF(B18<>\"\",LEN(B18)-LEN(SUBSTITUTE(B18,\",\",\"\"))+1,\"\")","v":1},"RM2.5","K101J15C0GF53L2","Mouser","594-K101J15C0GF53L2",8.6999999999999994E-2,8.6999999999999994E-2]
["Ceramic","C26, C27, C29","1 nF",{"$f":"IF(B19<>\"\",LEN(B19)-LEN(SUBSTITUTE(B19,\",\",\"\"))+1,\"\")","v":3},"RM2.5","R82EC1100AA50K","Mouser","80-R82EC1100AA50K",0.21,0.63]
["Film","C13, C30","10 nF",2,"RM2.5/RM5.0","R82EC2100AA50J","Mouser","80-R82EC2100AA50J",0.218,0.436]
["Ceramic","C20, C25, C31, C32, C33, C34, C35, C36, C37, C38, C39, C40, C41, C42, C46, C48, C49, C51, C54, C55, C56, C57, C58, C59, C60, C63, C64","100 nF",27,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,0.64800000000000002]
["Film","C22, C23, C24, C28","220 nF",{"$f":"IF(B22<>\"\",LEN(B22)-LEN(SUBSTITUTE(B22,\",\",\"\"))+1,\"\")","v":4},"RM2.5/RM5.0","R82DC3220Z360K","Mouser","80-82DC3220Z360K",0.10299999999999999,0.41199999999999998]
["Film","C52, C53","330 nF",{"$f":"IF(B23<>\"\",LEN(B23)-LEN(SUBSTITUTE(B23,\",\",\"\"))+1,\"\")","v":2},"RM2.5/RM5.0","R82DC3330AA60K","Mouser","80-R82DC3330AA60K",0.26200000000000001,0.52400000000000002]
["Film","C21","1 µF",{"$f":"IF(B24<>\"\",LEN(B24)-LEN(SUBSTITUTE(B24,\",\",\"\"))+1,\"\")","v":1},"RM2.5/RM5.0","R82DC4100Z360K","Mouser","80-R82DC4100Z360K",0.27900000000000003,0.27900000000000003]
["Electrolytic","C7, C8, C9, C10, C15, C16, C17, C18, C47","22 µF/25 V, max. ⌀ 5 mm",9,"RM2.0","Würth 860010572003","Mouser","710-860010572003",8.8999999999999996E-2,0.80099999999999993]
["Electrolytic","C45, C61, C62","47 µF/35 V, max. ⌀ 5 mm",3,"RM2.0","Würth 860010572005","Mouser","710-860010572005",7.0999999999999994E-2,0.21299999999999997]
["Electrolytic","C43, C44, C50","100 µF/25 V, max. ⌀ 7 mm",{"$f":"IF(B27<>\"\",LEN(B27)-LEN(SUBSTITUTE(B27,\",\",\"\"))+1,\"\")","v":3},"RM2.5","Würth 860010473007","Mouser","710-860010473007",0.111,{"$f":"I27*D27","v":0.33300000000000002}]
["Resistor","R73, R85, R86, R87, R88, R89, R90, R91, R92, R93","47 Ω, 250 mW",{"$f":"IF(B28<>\"\",LEN(B28)-LEN(SUBSTITUTE(B28,\",\",\"\"))+1,\"\")","v":10},"0204/0207","LR0204F47R","Farnell",2329945,4.0800000000000003E-2,{"$f":"I28*D28","v":0.40800000000000003}]
["Resistor","R95","220 Ω",1,"0204/0207","LR0204F220R","Farnell",2329900,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R45, R46, R75","470 Ω",3,"0204/0207","LR0204F470R","Farnell",2329942,3.5299999999999998E-2,0.10589999999999999]
["Resistor","R21, R22, R33, R34","560 Ω",4,"0204/0207","LR0204F560R","Farnell",2329953,3.5299999999999998E-2,0.14119999999999999]
["Resistor","R84","2.2 kΩ",{"$f":"IF(B32<>\"\",LEN(B32)-LEN(SUBSTITUTE(B32,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F2K2","Farnell",2329912,7.7100000000000002E-2,7.7100000000000002E-2]
["Resistor","R50","3.3 kΩ",{"$f":"IF(B33<>\"\",LEN(B33)-LEN(SUBSTITUTE(B33,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F3K3","Farnell",2329934,3.5999999999999997E-2,{"$f":"I33*D33","v":3.5999999999999997E-2}]
["Resistor","R39, R81","4.7 kΩ",{"$f":"IF(B34<>\"\",LEN(B34)-LEN(SUBSTITUTE(B34,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F4K7","Farnell",2329947,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R47, R48, R59","6.8 kΩ",3,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,0.10589999999999999]
["Resistor","R60","8.2 kΩ",1,"0204/0207","LR0204F8K2","Farnell",2329981,3.5999999999999997E-2,{"$f":"I36*D36","v":3.5999999999999997E-2}]
["Resistor","R29, R30, R31, R32, R49, R52, R53, R54, R55, R56, R61, R64, R67, R77","10 kΩ",{"$f":"IF(B37<>\"\",LEN(B37)-LEN(SUBSTITUTE(B37,\",\",\"\"))+1,\"\")","v":14},"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,0.47600000000000003]
["Resistor","R1, R2","15 kΩ",{"$f":"IF(B38<>\"\",LEN(B38)-LEN(SUBSTITUTE(B38,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F15K","Farnell",2329873,3.5299999999999998E-2,{"$f":"I38*D38","v":7.0599999999999996E-2}]
["Resistor","R37","18 kΩ",{"$f":"IF(B39<>\"\",LEN(B39)-LEN(SUBSTITUTE(B39,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F18K","Farnell",2329882,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R58, R62, R63, R76","20 kΩ",{"$f":"IF(B40<>\"\",LEN(B40)-LEN(SUBSTITUTE(B40,\",\",\"\"))+1,\"\")","v":4},"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,0.14119999999999999]
["Resistor","R51, R57, R94","24 kΩ",{"$f":"IF(B41<>\"\",LEN(B41)-LEN(SUBSTITUTE(B41,\",\",\"\"))+1,\"\")","v":3},"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,0.10799999999999998]
["Resistor","R9, R10","27 kΩ",{"$f":"IF(B42<>\"\",LEN(B42)-LEN(SUBSTITUTE(B42,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F27K","Farnell",2329909,3.5299999999999998E-2,7.0599999999999996E-2]
["Resistor","R65","39 kΩ",{"$f":"IF(B43<>\"\",LEN(B43)-LEN(SUBSTITUTE(B43,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F39K","Farnell",2329932,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R3, R4, R5, R6, R7, R8, R82","47 kΩ",7,"0204/0207","LR0204F47K","Farnell",2329944,2.7E-2,0.189]
["Resistor","R40","75 kΩ",1,"0204/0207","LR0204F75K","Farnell",2329972,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R11, R12, R13, R14, R15, R16, R23, R24, R25, R26, R27, R35, R36, R38, R41, R42, R66, R68, R69, R70, R79, R80","100 kΩ",{"$f":"IF(B46<>\"\",LEN(B46)-LEN(SUBSTITUTE(B46,\",\",\"\"))+1,\"\")","v":22},"0204/0207","LR0204F100K","Farnell",2329853,2.6499999999999999E-2,0.58299999999999996]
["Resistor","R19, R20","180 kΩ",{"$f":"IF(B47<>\"\",LEN(B47)-LEN(SUBSTITUTE(B47,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F180K","Farnell",2329880,4.4699999999999997E-2,8.9399999999999993E-2]
["Resistor","R17, R18","200 kΩ",{"$f":"IF(B48<>\"\",LEN(B48)-LEN(SUBSTITUTE(B48,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F200K","Farnell",2329895,3.4700000000000002E-2,6.9400000000000003E-2]
["Resistor","R74","220 kΩ",1,"0204/0207","LR0204F220K","Farnell",2329899,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R43, R44, R71, R72, R78, R83","1 MΩ",{"$f":"IF(B50<>\"\",LEN(B50)-LEN(SUBSTITUTE(B50,\",\",\"\"))+1,\"\")","v":6},"0204/0207","LR0204F1M0","Farnell",2329894,3.5299999999999998E-2,0.21179999999999999]
["Potentiometer","P2","100 kΩ log, Alpha 9 mm, right angled (side adjust), stereo",1,null,"Alpha 9-PC-STE-100k log, RD902F-20-15R1-A100K","Small Bear (US) or banzaimusic.com (EU)","100k-log-dual",2.8,{"$f":"I51*D51","v":2.8}]
["Potentiometer","P1, P3","100 kΩ log, Alpha 9 mm, right angled (side adjust)",{"$f":"IF(B52<>\"\",LEN(B52)-LEN(SUBSTITUTE(B52,\",\",\"\"))+1,\"\")","v":2},null,"RD901F-20-15R1-A100K","Small Bear (US) or Thonk (EU)","100k-log-single",1.17,2.34]
["Trimmer, multi-turn","TR8, TR9, TR10","100 kΩ",{"$f":"IF(B53<>\"\",LEN(B53)-LEN(SUBSTITUTE(B53,\",\",\"\"))+1,\"\")","v":3},null,"T93XA104KT20","Mouser","72-T93XA-100K",1.23,3.69]
["Trimmer","TR1, TR2, TR3, TR5","10 kΩ",4,null,"PT 10 LH 10K","Mouser","531-PT10H-10K",0.51800000000000002,2.0720000000000001]
["Trimmer","TR4, TR6, TR7","25 kΩ",3,null,"PT 10 LH 25K","Mouser","531-PT10H-25K",0.48699999999999999,1.4609999999999999]
["Jack","FLTR-OUT, VOCODER-OUT","6.35 mm jack",{"$f":"IF(B56<>\"\",LEN(B56)-LEN(SUBSTITUTE(B56,\",\",\"\"))+1,\"\")","v":2},null,"ACJS-MHDR","Mouser","523-ACJS-MHDR",1.1599999999999999,2.3199999999999998]
["Connector","11x","Wire-to-board connector, 2-pin",11,null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,0.75019999999999998]
["Connector","1x","Wire-to-board connector, 3-pin",1,null,"S3B-EH(LF)(SN)","Farnell",2481438,9.8599999999999993E-2,9.8599999999999993E-2]
["Connector","11x","EHR-2",{"$f":"D57","v":11},null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,0.34320000000000001]
["Connector","1x","EHR-3",{"$f":"D58","v":1},null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,3.4500000000000003E-2]
["Connector","23x","SEH-001T-P0.6",{"$f":"D59*2+D60*3","v":25},null,"SEH-001T-P0.6","Farnell",1863249,2.4400000000000002E-2,0.61]
["Connector","1x","2x8 board-to-board connector, angled, RM2.54 mm",1,null,"Würth 61301621021","Mouser","710-61301621021",0.871,0.871]
["Connector","1x","2x8 wire-to-board connector, RM2.54 mm",1,null,"Würth 61201623021","Mouser","710-61201623021",0.65,0.65]
["IC Socket","IC1, IC2, IC3, IC4, IC5, IC6, IC16","8 pins",7,null,"110-99-308-41-001000","Mouser","575-199308",0.38,2.66]
["IC Socket","IC8, IC10, IC11, IC14, IC15","14 pins",5,null,"110-99-314-41-001000","Mouser","575-199314",0.49299999999999999,2.4649999999999999]
["IC Socket","IC9","16 pins",1,null,"110-99-316-41-001000","Mouser","575-199316",0.42799999999999999,0.42799999999999999]
["Misc","ENV, PWMR, PWML, BR, SBSW, GND, TRI, FLTR, VC-R, VC-L","Solder pins,  ⌀ 1 mm",{"$f":"IF(B67<>\"\",LEN(B67)-LEN(SUBSTITUTE(B67,\",\",\"\"))+1,\"\")","v":10},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,0.25900000000000001]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J67)","v":44.977200000000011},"total"]

{"sheet":"Slew-freeze","index":10,"n_rows":54,"n_cols":11,"rows_kept":54,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Diode","D1, D2, D3, D4, D5, D6, D7, D8","1N4148",{"$f":"IF(B5<>\"\",LEN(B5)-LEN(SUBSTITUTE(B5,\",\",\"\"))+1,\"\")","v":8},"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,{"$f":"I5*D5","v":0.14399999999999999}]
["JFET","J1, J2","J113",2,"TO-92","J113","Mouser","512-J113",0.249,0.498]
["Transistor","T1, T2, T3","2N3904",3,"TO-92","2N3904BU","Mouser","512-2N3904BU",5.0999999999999997E-2,0.153]
["IC","IC1, IC2, IC3","TL074",3,"DIL14","TL074CN","Mouser","595-TL074CN",0.46800000000000003,1.4040000000000001]
["IC","IC4","LM319",1,"DIL14","LM319N","Mouser","512-LM319N",0.498,0.498]
["IC","IC5","CD4093",1,"DIL14","CD4093BE","Mouser","595-CD4093BE",0.42799999999999999,0.42799999999999999]
["Film","C6","1 nF",1,"RM2.5/RM5.0","R82EC1100AA50K","Mouser","80-R82EC1100AA50K",0.21,0.21]
["Film","C7","4.7 nF",1,"RM2.5/RM5.0","R82EC1470CK50J","Mouser","80-R82EC1470CK50J",0.253,0.253]
["Film","C5","10 nF",1,"RM2.5/RM5.0","R82EC2100AA50J","Mouser","80-R82EC2100AA50J",0.218,0.218]
["Film","C3, C4, C10","100 nF",3,"RM2.5/RM5.0","R82EC3100AA70J","Mouser","80-R82EC3100AA70J",0.14099999999999999,0.42299999999999993]
["Ceramic","C8, C9, C11, C12, C15, C16, C19, C20, C21, C22, C25","100 nF",11,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,0.26400000000000001]
["Film","C1","220 nF",1,"RM2.5/RM5.0","R82DC3220Z360K","Mouser","80-82DC3220Z360K",0.10299999999999999,4.3999999999999997E-2]
["Electrolytic","C2","2.2 µF/25 V, max. ⌀ 5 mm",1,"RM2.0","Würth 860020672006","Mouser","710-860020672006",0.1,{"$f":"I17*D17","v":0.1}]
["Electrolytic","C13, C14, C17, C18, C23, C24, C26","22 µF/25 V, max. ⌀ 5 mm",7,"RM2.0","Würth 860010572003","Mouser","710-860010572003",8.8999999999999996E-2,0.623]
["Tempco","R20","2 kΩ, 3300 ppm/°C",1,null,null,"Thonk","tempco",1.61,1.61,"Akaneohm"]
["Resistor","R34","10 Ω",{"$f":"IF(B20<>\"\",LEN(B20)-LEN(SUBSTITUTE(B20,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F10R","Farnell",2329856,3.5999999999999997E-2,{"$f":"I20*D20","v":3.5999999999999997E-2}]
["Resistor","R54, R55, R56, R57, R58, R59, R60, R61","47 Ω, 250 mW",8,"0204/0207","LR0204F47R","Farnell",2329945,4.0800000000000003E-2,0.32640000000000002]
["Resistor","R23, R38, R39, R46, R50, R53","2.2 kΩ",6,"0204/0207","LR0204F2K2","Farnell",2329912,7.7100000000000002E-2,0.46260000000000001]
["Resistor","R9, R25","4.7 kΩ",2,"0204/0207","LR0204F4K7","Farnell",2329947,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R15, R49","7.5 kΩ",2,"0204/0207","LR0204F7K5","Farnell",2329974,8.1199999999999994E-2,0.16239999999999999]
["Resistor","R21, R22","10 kΩ",2,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,6.8000000000000005E-2]
["Resistor","R41","30 kΩ",1,"0204/0207","LR0204F30K","Farnell",2329917,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R13","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,3.5299999999999998E-2]
["Resistor","R10, R31, R32, R33, R37, R45, R51, R52","47 kΩ",8,"0204/0207","LR0204F47K","Farnell",2329944,2.7E-2,0.216]
["Resistor","R12, R17","56 kΩ",2,"0204/0207","LR0204F56K","Farnell",2329954,3.5299999999999998E-2,7.0599999999999996E-2]
["Resistor","R16, R27","91 kΩ",2,"0204/0207","LR0204F91K","Farnell",2329984,3.4700000000000002E-2,6.9400000000000003E-2]
["Resistor","R1, R2, R3, R8, R19, R26, R28, R29, R30, R36, R44, R48","100 kΩ",12,"0204/0207","LR0204F100K","Farnell",2329853,2.6499999999999999E-2,0.318]
["Resistor","R18","120 kΩ",1,"0204/0207","LR0204F120K","Farnell",2329861,8.5699999999999998E-2,8.5699999999999998E-2]
["Resistor","R14","150 kΩ",1,"0204/0207","LR0204F150K","Farnell",2329871,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R4","200 kΩ",1,"0204/0207","LR0204F200K","Farnell",2329895,3.4700000000000002E-2,3.4700000000000002E-2]
["Resistor","R6, R47","220 kΩ",2,"0204/0207","LR0204F220K","Farnell",2329899,3.5999999999999997E-2,7.1999999999999995E-2]
["Resistor","R24","470 kΩ",1,"0204/0207","LR0204F470K","Farnell",2329941,3.5999999999999997E-2,3.5999999999999997E-2]
["Resistor","R5, R7, R11","1 MΩ",3,"0204/0207","LR0204F1M0","Farnell",2329894,3.5299999999999998E-2,0.10589999999999999]
["Resistor","R40","2.2 MΩ, 5%",1,"0204/0207","CFR16J2M2","Farnell",2329510,2.46E-2,2.46E-2]
["Resistor","R35","3.3 MΩ, 5%",1,"0204/0207","CFR16J3M3","Farnell",2329524,5.2900000000000003E-2,5.2900000000000003E-2]
["Potentiometer","P1","100 kΩ lin, Alpha 9 mm, right angled (side adjust)",{"$f":"IF(B40<>\"\",LEN(B40)-LEN(SUBSTITUTE(B40,\",\",\"\"))+1,\"\")","v":1},null,"RD901F-20-15R1-B100K","Small Bear (US) or Thonk (EU)","100k-lin-single",1.38,1.38]
["Trimmer","TR3","1k Ω",{"$f":"IF(B41<>\"\",LEN(B41)-LEN(SUBSTITUTE(B41,\",\",\"\"))+1,\"\")","v":1},null,"PT 10 LV 1K","Mouser","531-PT10V-1K",0.50800000000000001,{"$f":"I41*D41","v":0.50800000000000001}]
["Trimmer","TR1, TR2","10 kΩ",{"$f":"IF(B42<>\"\",LEN(B42)-LEN(SUBSTITUTE(B42,\",\",\"\"))+1,\"\")","v":2},null,"PT 10 LV 10K","Mouser","531-PT10V-10K",0.52900000000000003,{"$f":"I42*D42","v":1.0580000000000001}]
["Trimmer","TR4","20 kΩ",1,null,"PT 10 LV 20K","Mouser","531-PT10V-20K",0.50800000000000001,{"$f":"I43*D43","v":0.50800000000000001}]
["Jack","CV-IN","3.5 mm jack",{"$f":"IF(B44<>\"\",LEN(B44)-LEN(SUBSTITUTE(B44,\",\",\"\"))+1,\"\")","v":1},null,"CL13845G","Farnell",2766196,1.26,{"$f":"I44*D44","v":1.26},"alternative: CL1384"]
["Jack","FOOT-SW","6.35 mm jack",{"$f":"IF(B45<>\"\",LEN(B45)-LEN(SUBSTITUTE(B45,\",\",\"\"))+1,\"\")","v":1},null,"ACJS-MHDR","Mouser","523-ACJS-MHDR",1.1599999999999999,1.1599999999999999]
["Connector","7x","Wire-to-board connector, 2-pin",7,null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,0.47739999999999999]
["Connector","1x","Wire-to-board connector, 3-pin",1,null,"S3B-EH(LF)(SN)","Farnell",2481438,9.8599999999999993E-2,9.8599999999999993E-2]
["Connector",{"$f":"B46","v":"7x"},"EHR-2",{"$f":"D46","v":7},null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,0.21839999999999998]
["Connector",{"$f":"B47","v":"1x"},"EHR-3",{"$f":"D47","v":1},null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,3.4500000000000003E-2]
["Connector","7x","SEH-001T-P0.6",{"$f":"D48*2+D49*3","v":17},null,"SEH-001T-P0.6","Farnell",1863249,2.4400000000000002E-2,0.4148]
["IC Socket","IC1, IC2, IC3, IC4, IC5","14 pins",{"$f":"IF(B51<>\"\",LEN(B51)-LEN(SUBSTITUTE(B51,\",\",\"\"))+1,\"\")","v":5},null,"110-99-314-41-001000","Mouser","575-199314",0.49299999999999999,{"$f":"I51*D51","v":2.4649999999999999}]
["Misc","GND, LOG, OSC, SLEW","Solder pins,  ⌀ 1 mm",{"$f":"IF(B52<>\"\",LEN(B52)-LEN(SUBSTITUTE(B52,\",\",\"\"))+1,\"\")","v":4},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,0.1036]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J52)","v":18.876799999999992},"total"]

{"sheet":"DC-DC supply","index":11,"n_rows":30,"n_cols":11,"rows_kept":30,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Misc","TEN 40-1222N","TRACO TEN 40-1222N",1,"Module","TRACO TEN 40-1222N","Mouser","495-TEN40-1222N",65.430000000000007,{"$f":"I5*D5","v":65.430000000000007}]
["Diode","D1","SB540",{"$f":"IF(B6<>\"\",LEN(B6)-LEN(SUBSTITUTE(B6,\",\",\"\"))+1,\"\")","v":1},"DO-201AD",{"$f":"C6","v":"SB540"},"Mouser","512-SB540",0.46,0.46]
["IC","IC1","IRF7319",1,"SO-8","IRF7319TRPBF","Mouser","942-IRF7319TRPBF",0.79500000000000004,0.79500000000000004]
["Transistor","T2, T3","2N3904",{"$f":"IF(B8<>\"\",LEN(B8)-LEN(SUBSTITUTE(B8,\",\",\"\"))+1,\"\")","v":2},"TO-92","2N3904BU","Mouser","512-2N3904BU",5.0999999999999997E-2,0.10199999999999999]
["Transistor","T1, T4","2N3906",2,"TO-92","2N3906BU","Mouser","512-2N3906BU",0.23599999999999999,0.47199999999999998]
["Ceramic","C8, C9","100 nF",{"$f":"IF(B10<>\"\",LEN(B10)-LEN(SUBSTITUTE(B10,\",\",\"\"))+1,\"\")","v":2},"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,4.8000000000000001E-2]
["Ceramic","C1, C4, C5, C6, C7","10 µF, 25 V",5,"SMD 1812","C4532X7R1E106M250KA","Mouser","810-C4532X7R1E106M",1.18,5.8999999999999995]
["Ceramic","C2, C3","1 nF, 2 kV",2,"SMD 1808","C1808C102MGRACAUTO","Mouser","80-C1808C102MGRAUTO",1.51,3.02]
["Resistor","R1, R4, R8","2.2 kΩ",{"$f":"IF(B13<>\"\",LEN(B13)-LEN(SUBSTITUTE(B13,\",\",\"\"))+1,\"\")","v":3},"0204/0207","LR0204F2K2","Farnell",2329912,7.7100000000000002E-2,0.23130000000000001]
["Resistor","R2, R3, R6, R7, R10","10 kΩ",5,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,0.17]
["Resistor","R5, R9","75 kΩ",2,"0204/0207","LR0204F75K","Farnell",2329972,3.5299999999999998E-2,7.0599999999999996E-2]
["Connector",{"$f":"CONCATENATE(D16, \"x\")","v":"2x"},"Wire-to-board connector, 2-pin",2,null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,{"$f":"I16*D16","v":0.13639999999999999},"For power LED"]
["Connector",{"$f":"CONCATENATE(D17, \"x\")","v":"9x"},"Wire-to-board connector, 3-pin",9,null,"S3B-EH(LF)(SN)","Farnell",2481438,9.8599999999999993E-2,0.88739999999999997]
["Connector",{"$f":"CONCATENATE(D18, \"x\")","v":"2x"},"EHR-2",2,null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,6.2399999999999997E-2,"For power LED and switch"]
["Connector",{"$f":"CONCATENATE(D19, \"x\")","v":"11x"},"EHR-3",11,null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,{"$f":"I19*D19","v":0.37950000000000006},"2 needed for supply testing"]
["Connector",{"$f":"CONCATENATE(D20, \"x\")","v":"35x"},"SEH-001T-P0.6",{"$f":"D18*2+D19*3-2","v":35},null,"SEH-001T-P0.6","Farnell",1863249,2.4400000000000002E-2,0.85400000000000009,"4 needed for supply testing"]
["Connector","1x","Wire-to-board terminal block, 2 entries",1,null,"Weidmuller 1934250000","Farnell",2893169,1.02,1.02]
["Misc","L1, L2","ELC10D101E (100 µH)",{"$f":"IF(B22<>\"\",LEN(B22)-LEN(SUBSTITUTE(B22,\",\",\"\"))+1,\"\")","v":2},null,"ELC-10D101E","Mouser","667-ELC-10D101E",0.91,1.82]
["Misc","FUSEHOLDER","HTC-100M",1,null,"HTC-100M","Farnell",2550634,0.51400000000000001,0.51400000000000001]
["Misc","FUSE","8 A, slow blow, 20 x 5 mm",1,null,"Schurter 0001.2513","Farnell",1360861,0.29599999999999999,0.29599999999999999,"As per TRACO datasheet"]
["Misc","Power supply","12 VDC 5 A 60 W",1,null,"GST60A12-P1J","Amazon, Jameco","GST60A12-P1J",14,14,"Works for US and Europe (90-264 V). Power cord extra."]
["Misc","Power jack","Isolated 2.1x5.5mm power jack",1,null,null,"JDS Labs","JDS Labs",2.58,{"$f":"I26*D26","v":2.58},"link"]
["Misc","GND, +12V, -12V","Solder pins,  ⌀ 1 mm",{"$f":"IF(B27<>\"\",LEN(B27)-LEN(SUBSTITUTE(B27,\",\",\"\"))+1,\"\")","v":3},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,{"$f":"I27*D27","v":7.7699999999999991E-2}]
["Misc-2","2x","10 Ω, 17 W resistor for testing purposes",2,null,"SQP20AJB-10R","Mouser","603-SQP20AJB-10R",1.06,2.12,"For power supply testing"]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J28)","v":101.44629999999998},"total"]

{"sheet":"LDO supply","index":12,"n_rows":32,"n_cols":11,"rows_kept":32,"cut":false,"hidden":false,"merged":[[0,0,1,4]]}
["LDO-based alternative to the DC/DC supply. Only build this supply if you are absolutely confident you can build this without risking your life or the life of others."]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["Diode","D1, D2, D3, D4, D5, D6, D7, D8, D9, D10, D11, D12","SB540",{"$f":"IF(B5<>\"\",LEN(B5)-LEN(SUBSTITUTE(B5,\",\",\"\"))+1,\"\")","v":12},"DO-201AD","SB540-E3/54","Mouser","625-SB540-E3",0.375,{"$f":"I5*D5","v":4.5}]
["IC","IC1, IC2","MIC29301-12WT",{"$f":"IF(B6<>\"\",LEN(B6)-LEN(SUBSTITUTE(B6,\",\",\"\"))+1,\"\")","v":2},"TO-220","MIC29301-12WT","Mouser","998-MIC29301-12WT",3.72,{"$f":"I6*D6","v":7.44}]
["Diode","D13, D14","1N4148",{"$f":"IF(B7<>\"\",LEN(B7)-LEN(SUBSTITUTE(B7,\",\",\"\"))+1,\"\")","v":2},"DO-35","1N4148","Mouser","512-1N4148",1.7999999999999999E-2,{"$f":"I7*D7","v":3.5999999999999997E-2}]
["Transistor","T1","2N3904",{"$f":"IF(B8<>\"\",LEN(B8)-LEN(SUBSTITUTE(B8,\",\",\"\"))+1,\"\")","v":1},"TO-92","2N3904BU","Mouser","512-2N3904BU",5.0999999999999997E-2,{"$f":"I8*D8","v":5.0999999999999997E-2}]
["Ceramic","C4A, C5A, C9A, C10A","100 nF",4,"SMD (1206 or 0805)","C1206C104K5RACTU","Mouser","80-C1206C104K5R",2.4E-2,{"$f":"I9*D9","v":9.6000000000000002E-2}]
["Electrolytic","C3, C8","10 µF/50 V, max. ⌀ 5 mm",2,"RM2.0","Würth 860020672010","Mouser","710-860020672010",0.1,0.2]
["Electrolytic","C1, C2, C6, C7","3900 µF/35 V, max. ⌀ 18 mm",4,"RM7.5","EEUFC1V392","Mouser","667-EEU-FC1V392",2.33,{"$f":"I11*D11","v":9.32}]
["Resistor","R1","2.2 kΩ",{"$f":"IF(B12<>\"\",LEN(B12)-LEN(SUBSTITUTE(B12,\",\",\"\"))+1,\"\")","v":1},"0204/0207","LR0204F2K2","Farnell",2329912,7.7100000000000002E-2,{"$f":"I12*D12","v":7.7100000000000002E-2}]
["Resistor","R2, R3","10 kΩ",{"$f":"IF(B13<>\"\",LEN(B13)-LEN(SUBSTITUTE(B13,\",\",\"\"))+1,\"\")","v":2},"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,6.8000000000000005E-2]
["Resistor","R4","47 kΩ",1,"0204/0207","LR0204F47K","Farnell",2329944,2.7E-2,2.7E-2]
["Resistor","R5","330 kΩ",{"$f":"IF(B15<>\"\",LEN(B15)-LEN(SUBSTITUTE(B15,\",\",\"\"))+1,\"\")","v":1},"0204/0207","MFR3-330KFC","Farnell",1565303,4.2500000000000003E-2,4.2500000000000003E-2]
["Connector","2x","Wire-to-board connector, 2-pin",2,null,"S2B-EH(LF)(SN)","Farnell",2481437,6.8199999999999997E-2,{"$f":"I16*D16","v":0.13639999999999999}]
["Connector","8x","Wire-to-board connector, 3-pin",9,null,"S3B-EH(LF)(SN)","Farnell",2481438,0.10299999999999999,0.92699999999999994]
["Connector","1x","Wire-to-board terminal block, 4 entries",1,null,"Weidmuller  9994130000","Farnell",2884774,1.1599999999999999,1.1599999999999999]
["Connector",{"$f":"CONCATENATE(D19, \"x\")","v":"2x"},"EHR-2",2,null,"EHR-2","Farnell",2481434,3.1199999999999999E-2,6.2399999999999997E-2,"For power LED and switch"]
["Connector","2x","EHR-3",11,null,"EHR-3","Farnell",2399175,3.4500000000000003E-2,0.37950000000000006,"2 needed for supply testing"]
["Connector","4x","SEH-001T-P0.6",{"$f":"D19*2+D20*3-2","v":35},null,"SEH-001T-P0.6","Farnell",1863249,2.5399999999999999E-2,{"$f":"I21*D21","v":0.88900000000000001},"4 needed for supply testing"]
["Misc","GND, +12V, -12V","Solder pins,  ⌀ 1 mm",{"$f":"IF(B22<>\"\",LEN(B22)-LEN(SUBSTITUTE(B22,\",\",\"\"))+1,\"\")","v":3},null,"Vogt 1364A.68","Conrad","736018 - 62",2.5899999999999999E-2,{"$f":"I22*D22","v":7.7699999999999991E-2}]
["Misc","1x","Heat sink",1,null,"OS518-150-B","Farnell",1773365,14.54,14.54]
["Misc","2x","Heat sink clips, TO-220",2,null,"MAX01NG","Farnell",2082840,0.433,0.86599999999999999]
["Misc","1x","Thermally conductive foil",1,null,"WLFT 404 24.5 X 27.7","Farnell",4695525,3.99,3.99]
["Misc","1x","Transformer",1,"Toroidal transformer","Sedlbauer 825014\n1x230 V/2x12 V, 50 VA, 2.08 A, temperature switch","Conrad","607136 - 62",38.99,38.99]
["Misc","FUSE","400 mA, slow blow, \n20 x 5 mm",1,null,"Littelfuse 0239.400MXP ","Farnell",1596634,0.35299999999999998,0.35299999999999998,"As per Sedlbauer datasheet"]
["Misc","1x","Power entry module",1,null,"Schurter 4304.6053","Mouser ","693-4304.6053",12.47,12.47]
["Misc","1x","Aluminum box",1,null,"Multicomp MC001186","Farnell",2545078,18.059999999999999,18.059999999999999,"To cover mains area"]
["Misc-2","2x","10 Ω, 17 W resistor for testing purposes",2,null,"SQP20AJB-10R","Mouser","603-SQP20AJB-10R",1.06,2.12,"For power supply testing"]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J30)","v":116.87860000000001},"total"]

{"sheet":"Misc.","index":13,"n_rows":19,"n_cols":11,"rows_kept":19,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks"]
["LED","5x front panel","LED red, 2.4 V, 2 mA",6,"3 mm LED","TLLR4401","Mouser","78-TLLR4401",0.3,{"$f":"D5*I5","v":1.7999999999999998},"Freeze, silence bridging, attack detect, voiced, unvoiced, power"]
["Misc-2","1x","16-wire ribbon cable, 28 AWG",1,null,"3M 3365-16","Farnell",297318,2.34,{"$f":"D6*I6","v":2.34},"1 meter"]
["Misc-2","5x","Single-pole dual-throw switch, ON-ON",6,null,"H8610VBAAA","Farnell",151134,2.36,{"$f":"D7*I7","v":14.16},"Front panel, various switches"]
["Misc-2","1x","Single-pole dual-throw switch, ON-OFF-ON",1,null,"H8620VBAAA","Farnell",733878,3.8,3.8,"Front panel, VUV function"]
["Misc-2","1x","Single-pole single-throw switch, momentary ON",1,null,"H8601VBAAA","Farnell",480393,3.8,3.8,"Front panel, freeze switch"]
["Misc-2","1x","1.6 mm shrink tubing",1,null,null,"Farnell",1210349,8.2799999999999999E-2,8.2799999999999999E-2,"4 feet"]
["Misc-2","1x","3.2 mm shrink tubing",1,null,null,"Farnell",1210352,1.63,1.63,"4 feet"]
["Misc-2","1x","Coax cable, 1.9 mm overall diameter",3,null,"Lapp 2170002","Farnell",1491534,4.6500000000000004,13.950000000000001,"3 meters (10 feet)"]
["Misc-2","50x","Knobs",50,"6.35 mm round shaft","Davies clone 1900h with brass insert","Thonk","knobs",0.73,36.5]
["Misc-2","1x","19 inch 3U enclosure",1,null,"Slim Line 03/230 3U 400 SILVER","Modushop","enclosure",53.9,53.9]
["Misc-2","6x","Round nylon spacer",6,null,"D01475","Farnell",1733405,3.1699999999999999E-2,0.19019999999999998]
["Misc-2","6x","3 mm screws with nut, 12 mm length",6,null,null,null,"screws 1",null,null,"Used for VUV detector board and slew/freeze board"]
["Misc-2","4x","3 mm screws with nut, 25 mm length",4,null,null,null,"screws 2",null,null,"Used for DC/DC board assembly"]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"SUM(J5:J14)","v":131.96280000000002},"total"]

{"sheet":"Baskets","index":14,"n_rows":256,"n_cols":6,"rows_kept":256,"cut":false,"hidden":false,"merged":[]}
[null,"Mouser basket ","Mouser Basket","Mouser Basket","Bundle Request Form","self procure"]
[null,"See Mouser project \"18-channel stereo vocoder (excl. supply)\"","See Mouser project \"Vocoder DC/DC supply\"","See Mouser project \"Vocoder LDO supply\"","See bundle request form","Your own responsibility"]
[null,1,2,3,4,5]
["511-L78L05ACZ","●"]
["511-L79L05ACZ","●"]
["595-CD40106BE","●"]
["595-CD4050BE","●"]
["595-CD4053BE","●"]
["595-CD4093BE","●"]
["926-LM13700N/NOPB","●"]
["512-LM319N","●"]
["595-NE5532AP","●"]
["887-300P14-U","●"]
["595-TL072IP","●"]
["595-TL074CN","●"]
["512-2N3904BU","●"]
["512-2N3906BU","●"]
["512-J105","●"]
["512-J113","●"]
["512-1N4148","●"]
["863-1N4001RLG","●"]
["603-MFR-12FTF52-10R","●"]
["603-MFR-12FTF52-47R","●"]
["603-MFR-12FTF52-100R","●"]
["603-MFR-12FTF52-220R","●"]
["603-MFR-12FTF52-430R","●"]
["603-MFR-12FTF52-470R","●"]
["603-MFR-12FTF52-510R","●"]
["603-MFR-12FTF52-560R","●"]
["603-MFR-12FTF52-750R","●"]
["603-MFR-12FTF52-820R","●"]
["603-MFR-12FTF52-1K","●"]
["603-MFR-12FTF52-1K5","●"]
["603-MFR-12FTF52-2K2","●"]
["603-MFR-12FTF52-3K3","●"]
["603-MFR-12FTF52-3K9","●"]
["603-MFR-12FTF52-4K7","●"]
["603-MFR-12FTF52-5K1","●"]
["603-MFR-12FTF52-5K6","●"]
["603-MFR-12FTF52-6K8","●"]
["603-MFR-12FTF52-7K5","●"]
["603-MFR-12FTF52-8K2","●"]
["603-MFR-12FTF52-10K","●"]
["603-MFR-12FTF52-12K","●"]
["603-MFR-12FTF52-15K","●"]
["603-MFR-12FTF52-18K","●"]
["603-MFR-12FTF52-20K","●"]
["603-MFR-12FTF52-22K","●"]
["603-MFR-12FTF52-24K","●"]
["603-MFR-12FTF52-27K","●"]
["603-MFR-12FTF52-30K","●"]
["603-MFR-12FTF52-33K","●"]
["603-MFR-12FTF52-36K","●"]
["603-MFR-12FTF52-39K","●"]
["603-MFR-12FTF52-47K","●"]
["603-MFR-12FTF52-56K","●"]
["603-MFR-12FTF52-62K","●"]
["603-MFR-12FTF52-75K","●"]
["603-MFR-12FTF52-91K","●"]
["603-MFR-12FTF52-100K","●"]
["603-MFR-12FTF52-120K","●"]
["603-MFR-12FTF52-150K","●"]
["603-MFR-12FTF52-180K","●"]
["603-MFR-12FTF52-200K","●"]
["603-MFR-12FTF52-220K","●"]
["603-MFR-12FTF52-330K","●"]
["603-MFR-12FTF52-390K","●"]
["603-MFR-12FTF52-470K","●"]
["603-MFR-12FTF52-820K","●"]
["603-MFR-12FTF52-1M","●"]
["603-MFR-12FTF52-1M5","●"]
["603-MFR-12FTF52-2M2","●"]
["603-MFR-12FTF52-3M3","●"]
["603-MFR-12FTF52-4M7","●"]
["603-MFR-12FTF52-6M8","●"]
["603-MFR-25FBF52-196R","●"]
["603-MFR-25FBF52-237R","●"]
["603-MFR-25FBF52-249R","●"]
["603-MFR-25FBF52-287R","●"]
["603-MFR-25FBF52-301R","●"]
["603-MFR-25FBF52-316R","●"]
["603-MFR-25FBF52-348R","●"]
["603-MFR-25FBF52-365R","●"]
["603-MFR-25FBF52-383R","●"]
["603-MFR-25FBF52-402R","●"]
["603-MFR-25FBF52-422R","●"]
["603-MFR-25FBF52-442R","●"]
["603-MFR-25FBF52-464R","●"]
["603-MFR-25FBF52-487R","●"]
["603-MFR-25FBF52-511R","●"]
["603-MFR-25FBF52-536R","●"]
["603-MFR-25FBF52-562R","●"]
["603-MFR-25FBF52-590R","●"]
["603-MFR-25FBF52-619R","●"]
["603-MFR-25FBF52-649R","●"]
["603-MFR-25FBF52-681R","●"]
["603-MFR-25FBF52-715R","●"]
["603-MFR-25FBF52-750R","●"]
["603-MFR-25FRF52-787R","●"]
["603-MFR-25FBF52-825R","●"]
["603-MFR-25FBF52-866R","●"]
["603-MFR-25FBF52-909R","●"]
["603-MFR-25FBF52-953R","●"]
["603-MFR-25FBF52-1K","●"]
["603-MFR-25FBF52-1K05","●"]
["603-MFR-25FBF52-1K1","●"]
["603-MFR-25FBF52-1K15","●"]
["603-MFR-25FBF52-1K21","●"]
["603-MFR-25FBF52-1K27","●"]
["603-MFR-25FBF52-1K33","●"]
["603-MFR-25FBF52-1K4","●"]
["603-MFR-25FBF52-1K69","●"]
["603-MFR-25FBF52-1K78","●"]
["603-MFR-25FBF52-6K81","●"]
["603-MFR-25FBF52-8K66","●"]
["603-MFR-25FBF52-9K09","●"]
["603-MFR-25FBF52-11K","●"]
["603-MFR-25FBF52-11K5","●"]
["603-MFR-25FBF52-12K1","●"]
["603-MFR-25FBF52-14K","●"]
["603-MFR-25FBF52-14K7","●"]
["603-MFR-25FBF52-15K4","●"]
["603-MFR-25FBF52-16K2","●"]
["603-MFR-25FBF52-17K8","●"]
["603-MFR-25FBF52-18K7","●"]
["603-MFR-25FBF52-19K6","●"]
["603-MFR-25FBF52-20K5","●"]
["603-MFR-25FBF52-22K6","●"]
["603-MFR-25FBF52-23K7","●"]
["603-MFR-25FBF52-24K9","●"]
["603-MFR-25FBF52-26K1","●"]
["603-MFR-25FBF52-28K7","●"]
["603-MFR-25FBF52-30K1","●"]
["603-MFR-25FBF52-31K6","●"]
["603-MFR-25FBF52-33K2","●"]
["603-MFR-25FBF52-36K5","●"]
["603-MFR-25FBF52-38K3","●"]
["603-MFR-25FBF52-40K2","●"]
["603-MFR-25FBF52-42K2","●"]
["603-MFR-25FBF52-46K4","●"]
["603-MFR-25FBF52-48K7","●"]
["603-MFR-25FBF52-51K1","●"]
["603-MFR-25FTE52-53K6","●"]
["603-MFR-25FBF52-59K","●"]
["603-MFR-25FBF52-61K9","●"]
["603-MFR-25FBF52-64K9","●"]
["603-MFR-25FBF52-68K1","●"]
["603-MFR-25FBF52-75K","●"]
["603-MFR-25FRF52-78K7","●"]
["603-MFR-25FBF52-82K5","●"]
["603-MFR-25FBF52-86K6","●"]
["603-MFR-25FBF52-95K3","●"]
["603-MFR-25FBF52-105K","●"]
["603-MFR-25FBF52-110K","●"]
["603-MFR-25FBF52-121K","●"]
["603-MFR-25FBF52-133K","●"]
["603-MFR-25FBF52-169K","●"]
["594-K220J15C0GF53L2","●"]
["594-K101J15C0GF53L2","●"]
["80-C315C221M5R","●"]
["594-K471J15C0GF53L2","●"]
["80-R82EC1100AA50K","●"]
["80-C315C152K1R","●"]
["581-08055A103JAT2A","●"]
["594-K103K15X7RF53L2","●"]
["810-CGA5F2C0G1H333J","●"]
["80-C1206C104K5R","●"]
["81-GRM31C5C1H104JA1L","●"]
["80-R82EC1100AA50K","●"]
["80-R82EC1220DQ50J","●"]
["80-R82EC1470CK50J","●"]
["80-R82EC2100AA50J","●"]
["80-R82EC2220AA50J","●"]
["80-R82EC2470AA60J","●"]
["80-R82EC3100AA70J","●"]
["80-82DC3220Z360K","●"]
["80-R82DC3330AA60K","●"]
["80-R82DC4100Z360K","●"]
["710-860020672006","●"]
["710-860020672007","●"]
["710-860020672010","●"]
["710-860010572003","●"]
["710-860010572005","●"]
["710-860010473007","●"]
["531-PT10V-1K","●"]
["531-PT10H-10K","●"]
["531-PT10V-10K","●"]
["531-PT10V-20K","●"]
["531-PT10H-25K","●"]
["531-PT10H-100K","●"]
["531-PT10V-100K","●"]
["531-PT10H-250K","●"]
["72-T93XA-100","●"]
["72-T93XA-2K","●"]
["72-T93XA-100K","●"]
["78-TLLG4401","●"]
["78-TLLR4401","●"]
["78-TLLY4401","●"]
["575-199308",null,null,null,null,"●"]
["575-199314",null,null,null,null,"●"]
["575-199316",null,null,null,null,"●"]
["575-11044318",null,null,null,null,"●"]
[2766196,null,null,null,"●"]
["523-ACJS-MHDR","●"]
["710-61201623021","●"]
["710-61300421021","●"]
["710-61301621021","●"]
[2481434,null,null,null,"●"]
[2399175,null,null,null,"●"]
["855-M7582-05","●"]
[1863249,null,null,null,"●"]
[2481437,null,null,null,"●"]
[2481438,null,null,null,"●"]
[2893169,null,null,null,"●"]
[1360861,null,null,null,"●"]
["GST60A12-P1J",null,null,null,null,"●"]
["667-ELC-10D101E",null,"●"]
[2550634,null,null,null,"●"]
["JDS Labs",null,null,null,null,"●"]
["736018 - 62",null,null,null,null,"●"]
["495-TEN40-1222N",null,"●"]
[1210349,null,null,null,null,"●"]
["screws 1",null,null,null,null,"●"]
["screws 2",null,null,null,null,"●"]
[1210352,null,null,null,null,"●"]
["603-SQP20AJB-10R",null,"●","●"]
[297318,null,null,null,null,"●"]
["enclosure",null,null,null,"●"]
[1491534,null,null,null,"●"]
["knobs",null,null,null,null,"●"]
[1733405,null,null,null,null,"●"]
[733878,null,null,null,"●"]
[151134,null,null,null,"●"]
[480393,null,null,null,"●"]
["495-TEN40-1222N",null,"●"]
["942-IRF7319TRPBF",null,"●"]
["512-SB540",null,"●"]
["LM3916",null,null,null,"●"]
["tempco",null,null,null,"●"]
["80-C1808C102MGRAUTO",null,"●"]
["810-C4532X7R1E106M",null,"●"]
["100k-lin-single",null,null,null,"●"]
["100k-log-single",null,null,null,"●"]
["100k-log-dual",null,null,null,"●"]
["MC33079",null,null,null,null,"●"]
[2884774,null,null,null,null,"●"]
[1596634,null,null,null,null,"●"]
["534497 - 62",null,null,null,null,"●"]
[1773365,null,null,null,null,"●"]
[2082840,null,null,null,null,"●"]
["693-4304.6053",null,null,"●"]
[4695525,null,null,null,null,"●"]
["607136 - 62",null,null,null,null,"●"]
["667-EEU-FC1V392",null,null,"●"]
["998-MIC29301-12WT",null,null,"●"]
["625-SB540-E3",null,null,"●"]

{"sheet":"Channel (calc)","index":15,"n_rows":292,"n_cols":12,"rows_kept":292,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["Type","Designator","Identifier","Count","Body type","Suggested product","Distributor","Order #","Individual price","Total price","Remarks","Channel"]
["Resistor-F","R1, R13","1.78 kΩ",2,"0204/0207","MRS25000C1781FCT00","Farnell",9465430,8.5000000000000006E-2,0.17,null,"120 Hz"]
["Resistor-F","R2, R14","53.6 kΩ",2,"0204/0207","MRS25000C5362FCT00","Farnell",9468960,5.0999999999999997E-2,0.10199999999999999,null,"120 Hz"]
["Resistor-F","R3, R15","110 kΩ",2,"0204/0207","MRS25000C1103FCT00","Farnell",9464069,5.0999999999999997E-2,0.10199999999999999,null,"120 Hz"]
["Resistor-F","R4, R16","1.69 kΩ",2,"0204/0207","MRS25000C1691FCT00","Farnell",9465413,8.5000000000000006E-2,0.17,null,"120 Hz"]
["Resistor-F","R5, R17","51.1 kΩ",2,"0204/0207","MRS25000C5112FCT00","Farnell",9468870,8.6999999999999994E-2,0.17399999999999999,null,"120 Hz"]
["Resistor-F","R6, R18","105 kΩ",2,"0204/0207","MRS25000C1053FCT00","Farnell",9463933,4.9000000000000002E-2,9.8000000000000004E-2,null,"120 Hz"]
["Resistor-F","R7, R19","1.4 kΩ",2,"0204/0207","MRS25000C1401FCT00","Farnell",9465324,8.6999999999999994E-2,0.17399999999999999,null,"120 Hz"]
["Resistor-F","R8, R20","51.1 kΩ",2,"0204/0207","MRS25000C5112FCT00","Farnell",9468870,8.6999999999999994E-2,0.17399999999999999,null,"120 Hz"]
["Resistor-F","R9, R21","169 kΩ",2,"0204/0207","MRS25000C1693FCT00","Farnell",9464808,8.6999999999999994E-2,0.17399999999999999,null,"120 Hz"]
["Resistor-F","R10, R22","1.15 kΩ",2,"0204/0207","MRS25000C1151FCT00","Farnell",9465235,8.6999999999999994E-2,0.17399999999999999,null,"120 Hz"]
["Resistor-F","R11, R23","40.2 kΩ",2,"0204/0207","MRS25000C4022FCT00","Farnell",9468153,8.4000000000000005E-2,0.16800000000000001,null,"120 Hz"]
["Resistor-F","R12, R24","133 kΩ",2,"0204/0207","MRS25000C1333FCT00","Farnell",9464409,8.4000000000000005E-2,0.16800000000000001,null,"120 Hz"]
["Resistor-F","R1, R13","1.4 kΩ",2,"0204/0207","MRS25000C1401FCT00","Farnell",9465324,8.6999999999999994E-2,0.17399999999999999,null,"150 Hz"]
["Resistor-F","R2, R14","42.2 kΩ",2,"0204/0207","MRS25000C4222FCT00","Farnell",9468234,5.0999999999999997E-2,0.10199999999999999,null,"150 Hz"]
["Resistor-F","R3, R15","86.6 kΩ",2,"0204/0207","MRS25000C8662FCT00","Farnell",9470379,0.06,0.12,null,"150 Hz"]
["Resistor-F","R4, R16","1.33 kΩ",2,"0204/0207","MRS25000C1331FCT00","Farnell",9465308,8.6999999999999994E-2,0.17399999999999999,null,"150 Hz"]
["Resistor-F","R5, R17","40.2 kΩ",2,"0204/0207","MRS25000C4022FCT00","Farnell",9468153,8.4000000000000005E-2,0.16800000000000001,null,"150 Hz"]
["Resistor-F","R6, R18","82.5 kΩ",2,"0204/0207","MRS25000C8252FCT00","Farnell",9470280,0.06,0.12,null,"150 Hz"]
["Resistor-F","R7, R19","1.1 kΩ",2,"0204/0207","MRS25000C1101FCT00","Farnell",9465219,8.6999999999999994E-2,0.17399999999999999,null,"150 Hz"]
["Resistor-F","R8, R20","40.2 kΩ",2,"0204/0207","MRS25000C4022FCT00","Farnell",9468153,8.4000000000000005E-2,0.16800000000000001,null,"150 Hz"]
["Resistor-F","R9, R21","133 kΩ",2,"0204/0207","MRS25000C1333FCT00","Farnell",9464409,8.4000000000000005E-2,0.16800000000000001,null,"150 Hz"]
["Resistor-F","R10, R22","909 Ω",2,"0204/0207","MRS25000C9090FCT00","Farnell",9470549,5.0999999999999997E-2,0.10199999999999999,null,"150 Hz"]
["Resistor-F","R11, R23","31.6 kΩ",2,"0204/0207","MRS25000C3162FCT00","Farnell",9467254,5.0999999999999997E-2,0.10199999999999999,null,"150 Hz"]
["Resistor-F","R12, R24","105 kΩ",2,"0204/0207","MRS25000C1053FCT00","Farnell",9463933,4.9000000000000002E-2,9.8000000000000004E-2,null,"150 Hz"]
["Resistor-F","R1, R13","1.1 kΩ",2,"0204/0207","MRS25000C1101FCT00","Farnell",9465219,8.6999999999999994E-2,0.17399999999999999,null,"190 Hz"]
["Resistor-F","R2, R14","33.2 kΩ",2,"0204/0207","MRS25000C3322FCT00","Farnell",9467360,8.6999999999999994E-2,0.17399999999999999,null,"190 Hz"]
["Resistor-F","R3, R15","68.1 kΩ",2,"0204/0207","MRS25000C6812FCT00","Farnell",9469672,8.6999999999999994E-2,0.17399999999999999,null,"190 Hz"]
["Resistor-F","R4, R16","1.05 kΩ",2,"0204/0207","MRS25000C1051FCT00","Farnell",9465197,8.6999999999999994E-2,0.17399999999999999,null,"190 Hz"]
["Resistor-F","R5, R17","31.6 kΩ",2,"0204/0207","MRS25000C3162FCT00","Farnell",9467254,5.0999999999999997E-2,0.10199999999999999,null,"190 Hz"]
["Resistor-F","R6, R18","64.9 kΩ",2,"0204/0207","MRS25000C6492FCT00","Farnell",9469567,0.06,0.12,null,"190 Hz"]
["Resistor-F","R7, R19","866 Ω",2,"0204/0207","MRS25000C8660FCT00","Farnell",9470360,8.5000000000000006E-2,0.17,null,"190 Hz"]
["Resistor-F","R8, R20","31.6 kΩ",2,"0204/0207","MRS25000C3162FCT00","Farnell",9467254,5.0999999999999997E-2,0.10199999999999999,null,"190 Hz"]
["Resistor-F","R9, R21","105 kΩ",2,"0204/0207","MRS25000C1053FCT00","Farnell",9463933,4.9000000000000002E-2,9.8000000000000004E-2,null,"190 Hz"]
["Resistor-F","R10, R22","715 Ω",2,"0204/0207","MRS25000C7150FCT00","Farnell",9469907,8.7999999999999995E-2,0.17599999999999999,null,"190 Hz"]
["Resistor-F","R11, R23","24.9 kΩ",2,"0204/0207","MRS25000C2492FCT00","Farnell",9466312,8.6999999999999994E-2,0.17399999999999999,null,"190 Hz"]
["Resistor-F","R12, R24","82.5 kΩ",2,"0204/0207","MRS25000C8252FCT00","Farnell",9470280,0.06,0.12,null,"190 Hz"]
["Resistor-F","R1, R13","866 Ω",2,"0204/0207","MRS25000C8660FCT00","Farnell",9470360,8.5000000000000006E-2,0.17,null,"240 Hz"]
["Resistor-F","R2, R14","26.1 kΩ",2,"0204/0207","MRS25000C2612FCT00","Farnell",9466436,8.7999999999999995E-2,0.17599999999999999,null,"240 Hz"]
["Resistor-F","R3, R15","53.6 kΩ",2,"0204/0207","MRS25000C5362FCT00","Farnell",9468960,5.0999999999999997E-2,0.10199999999999999,null,"240 Hz"]
["Resistor-F","R4, R16","825 Ω",2,"0204/0207","MRS25000C8250FCT00","Farnell",9470263,8.6999999999999994E-2,0.17399999999999999,null,"240 Hz"]
["Resistor-F","R5, R17","24.9 kΩ",2,"0204/0207","MRS25000C2492FCT00","Farnell",9466312,8.6999999999999994E-2,0.17399999999999999,null,"240 Hz"]
["Resistor-F","R6, R18","51.1 kΩ",2,"0204/0207","MRS25000C5112FCT00","Farnell",9468870,8.6999999999999994E-2,0.17399999999999999,null,"240 Hz"]
["Resistor-F","R7, R19","681 Ω",2,"0204/0207","MRS25000C6810FCT00","Farnell",9469656,8.4000000000000005E-2,0.16800000000000001,null,"240 Hz"]
["Resistor-F","R8, R20","24.9 kΩ",2,"0204/0207","MRS25000C2492FCT00","Farnell",9466312,8.6999999999999994E-2,0.17399999999999999,null,"240 Hz"]
["Resistor-F","R9, R21","82.5 kΩ",2,"0204/0207","MRS25000C8252FCT00","Farnell",9470280,0.06,0.12,null,"240 Hz"]
["Resistor-F","R10, R22","562 Ω",2,"0204/0207","MRS25000C5620FCT00","Farnell",9469052,6.5000000000000002E-2,0.13,null,"240 Hz"]
["Resistor-F","R11, R23","19.6 kΩ",2,"0204/0207","MRS25000C1962FCT00","Farnell",9465146,8.4000000000000005E-2,0.16800000000000001,null,"240 Hz"]
["Resistor-F","R12, R24","64.9 kΩ",2,"0204/0207","MRS25000C6492FCT00","Farnell",9469567,0.06,0.12,null,"240 Hz"]
["Resistor-F","R1, R13","681 Ω",2,"0204/0207","MRS25000C6810FCT00","Farnell",9469656,8.4000000000000005E-2,0.16800000000000001,null,"310 Hz"]
["Resistor-F","R2, R14","20.5 kΩ",2,"0204/0207","MRS25000C2052FCT00","Farnell",9465928,8.1000000000000003E-2,0.16200000000000001,null,"310 Hz"]
["Resistor-F","R3, R15","42.2 kΩ",2,"0204/0207","MRS25000C4222FCT00","Farnell",9468234,5.0999999999999997E-2,0.10199999999999999,null,"310 Hz"]
["Resistor-F","R4, R16","649 Ω",2,"0204/0207","MRS25000C6490FCT00","Farnell",9469559,0.05,0.1,null,"310 Hz"]
["Resistor-F","R5, R17","19.6 kΩ",2,"0204/0207","MRS25000C1962FCT00","Farnell",9465146,8.4000000000000005E-2,0.16800000000000001,null,"310 Hz"]
["Resistor-F","R6, R18","40.2 kΩ",2,"0204/0207","MRS25000C4022FCT00","Farnell",9468153,8.4000000000000005E-2,0.16800000000000001,null,"310 Hz"]
["Resistor-F","R7, R19","536 Ω",2,"0204/0207","MRS25000C5360FCT00","Farnell",9468951,8.5000000000000006E-2,0.17,null,"310 Hz"]
["Resistor-F","R8, R20","19.6 kΩ",2,"0204/0207","MRS25000C1962FCT00","Farnell",9465146,8.4000000000000005E-2,0.16800000000000001,null,"310 Hz"]
["Resistor-F","R9, R21","64.9 kΩ",2,"0204/0207","MRS25000C6492FCT00","Farnell",9469567,0.06,0.12,null,"310 Hz"]
["Resistor-F","R10, R22","442 Ω",2,"0204/0207","MRS25000C4420FCT00","Farnell",9468340,8.5000000000000006E-2,0.17,null,"310 Hz"]
["Resistor-F","R11, R23","15.4 kΩ",2,"0204/0207","MRS25000C1542FCT00","Farnell",9464697,8.4000000000000005E-2,0.16800000000000001,null,"310 Hz"]
["Resistor-F","R12, R24","51.1 kΩ",2,"0204/0207","MRS25000C5112FCT00","Farnell",9468870,8.6999999999999994E-2,0.17399999999999999,null,"310 Hz"]
["Resistor-F","R1, R13","536 Ω",2,"0204/0207","MRS25000C5360FCT00","Farnell",9468951,8.5000000000000006E-2,0.17,null,"390 Hz"]
["Resistor-F","R2, R14","16.2 kΩ",2,"0204/0207","MRS25000C1622FCT00","Farnell",9464832,8.6999999999999994E-2,0.17399999999999999,null,"390 Hz"]
["Resistor-F","R3, R15","33.2 kΩ",2,"0204/0207","MRS25000C3322FCT00","Farnell",9467360,8.6999999999999994E-2,0.17399999999999999,null,"390 Hz"]
["Resistor-F","R4, R16","511 Ω",2,"0204/0207","MRS25000C5110FCT00","Farnell",9468854,7.2999999999999995E-2,0.14599999999999999,null,"390 Hz"]
["Resistor-F","R5, R17","15.4 kΩ",2,"0204/0207","MRS25000C1542FCT00","Farnell",9464697,8.4000000000000005E-2,0.16800000000000001,null,"390 Hz"]
["Resistor-F","R6, R18","31.6 kΩ",2,"0204/0207","MRS25000C3162FCT00","Farnell",9467254,5.0999999999999997E-2,0.10199999999999999,null,"390 Hz"]
["Resistor-F","R7, R19","422 Ω",2,"0204/0207","MRS25000C4220FCT00","Farnell",9468226,8.6999999999999994E-2,0.17399999999999999,null,"390 Hz"]
["Resistor-F","R8, R20","15.4 kΩ",2,"0204/0207","MRS25000C1542FCT00","Farnell",9464697,8.4000000000000005E-2,0.16800000000000001,null,"390 Hz"]
["Resistor-F","R9, R21","51.1 kΩ",2,"0204/0207","MRS25000C5112FCT00","Farnell",9468870,8.6999999999999994E-2,0.17399999999999999,null,"390 Hz"]
["Resistor-F","R10, R22","348 Ω",2,"0204/0207","MRS25000C3480FCT00","Farnell",9467424,7.2999999999999995E-2,0.14599999999999999,null,"390 Hz"]
["Resistor-F","R11, R23","12.1 kΩ",2,"0204/0207","MRS25000C1212FCT00","Farnell",9464310,8.6999999999999994E-2,0.17399999999999999,null,"390 Hz"]
["Resistor-F","R12, R24","40.2 kΩ",2,"0204/0207","MRS25000C4022FCT00","Farnell",9468153,8.4000000000000005E-2,0.16800000000000001,null,"390 Hz"]
["Resistor-F","R1, R13","1.27 kΩ",2,"0204/0207","MRS25000C1271FCT00","Farnell",9465286,8.6999999999999994E-2,0.17399999999999999,null,"500 Hz"]
["Resistor-F","R2, R14","38.3 kΩ",2,"0204/0207","MRS25000C3832FCT00","Farnell",9467653,8.6999999999999994E-2,0.17399999999999999,null,"500 Hz"]
["Resistor-F","R3, R15","78.7 kΩ",2,"0204/0207","MRS25000C7872FCT00","Farnell",9470077,0.06,0.12,null,"500 Hz"]
["Resistor-F","R4, R16","1.21 kΩ",2,"0204/0207","MRS25000C1211FCT00","Farnell",9465260,5.0999999999999997E-2,0.10199999999999999,null,"500 Hz"]
["Resistor-F","R5, R17","36.5 kΩ",2,"0204/0207","MRS25000C3652FCT00","Farnell",9467564,8.5000000000000006E-2,0.17,null,"500 Hz"]
["Resistor-F","R6, R18","75 kΩ",2,"0204/0207","MRS25000C7502FCT00","Farnell",9469990,8.4000000000000005E-2,0.16800000000000001,null,"500 Hz"]
["Resistor-F","R7, R19","1 kΩ",2,"0204/0207","MRS25000C1001FCT00","Farnell",9465170,0.05,0.1,null,"500 Hz"]
["Resistor-F","R8, R20","36.5 kΩ",2,"0204/0207","MRS25000C3652FCT00","Farnell",9467564,8.5000000000000006E-2,0.17,null,"500 Hz"]
["Resistor-F","R9, R21","121 kΩ",2,"0204/0207","MRS25000C1213FCT00","Farnell",9464247,8.6999999999999994E-2,0.17399999999999999,null,"500 Hz"]
["Resistor-F","R10, R22","825 Ω",2,"0204/0207","MRS25000C8250FCT00","Farnell",9470263,8.6999999999999994E-2,0.17399999999999999,null,"500 Hz"]
["Resistor-F","R11, R23","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"500 Hz"]
["Resistor-F","R12, R24","95.3 kΩ",2,"0204/0207","MRS25000C9532FCT00","Farnell",9470689,0.05,0.1,null,"500 Hz"]
["Resistor-F","R1, R13","1 kΩ",2,"0204/0207","MRS25000C1001FCT00","Farnell",9465170,0.05,0.1,null,"640 Hz"]
["Resistor-F","R2, R14","30.1 kΩ",2,"0204/0207","MRS25000C3012FCT00","Farnell",9467181,8.6999999999999994E-2,0.17399999999999999,null,"640 Hz"]
["Resistor-F","R3, R15","61.9 kΩ",2,"0204/0207","MRS25000C6192FCT00","Farnell",9469443,8.5999999999999993E-2,0.17199999999999999,null,"640 Hz"]
["Resistor-F","R4, R16","953 Ω",2,"0204/0207","MRS25000C9530FCT00","Farnell",9470670,8.5000000000000006E-2,0.17,null,"640 Hz"]
["Resistor-F","R5, R17","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"640 Hz"]
["Resistor-F","R6, R18","59 kΩ",2,"0204/0207","MRS25000C5902FCT00","Farnell",9469168,8.6999999999999994E-2,0.17399999999999999,null,"640 Hz"]
["Resistor-F","R7, R19","787 Ω",2,"0204/0207","MRS25000C7870FCT00","Farnell",9470069,7.2999999999999995E-2,0.14599999999999999,null,"640 Hz"]
["Resistor-F","R8, R20","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"640 Hz"]
["Resistor-F","R9, R21","95.3 kΩ",2,"0204/0207","MRS25000C9532FCT00","Farnell",9470689,0.05,0.1,null,"640 Hz"]
["Resistor-F","R10, R22","649 Ω",2,"0204/0207","MRS25000C6490FCT00","Farnell",9469559,0.05,0.1,null,"640 Hz"]
["Resistor-F","R11, R23","22.6 kΩ",2,"0204/0207","MRS25000C2262FCT00","Farnell",9466118,8.5000000000000006E-2,0.17,null,"640 Hz"]
["Resistor-F","R12, R24","75 kΩ",2,"0204/0207","MRS25000C7502FCT00","Farnell",9469990,8.4000000000000005E-2,0.16800000000000001,null,"640 Hz"]
["Resistor-F","R1, R13","787 Ω",2,"0204/0207","MRS25000C7870FCT00","Farnell",9470069,7.2999999999999995E-2,0.14599999999999999,null,"810 Hz"]
["Resistor-F","R2, R14","23.7 kΩ",2,"0204/0207","MRS25000C2372FCT00","Farnell",9466207,5.0999999999999997E-2,0.10199999999999999,null,"810 Hz"]
["Resistor-F","R3, R15","48.7 kΩ",2,"0204/0207","MRS25000C4872FCT00","Farnell",9468552,8.6999999999999994E-2,0.17399999999999999,null,"810 Hz"]
["Resistor-F","R4, R16","750 Ω",2,"0204/0207","MRS25000C7500FCT00","Farnell",9469982,8.5000000000000006E-2,0.17,null,"810 Hz"]
["Resistor-F","R5, R17","22.6 kΩ",2,"0204/0207","MRS25000C2262FCT00","Farnell",9466118,8.5000000000000006E-2,0.17,null,"810 Hz"]
["Resistor-F","R6, R18","46.4 kΩ",2,"0204/0207","MRS25000C4642FCT00","Farnell",9468439,8.6999999999999994E-2,0.17399999999999999,null,"810 Hz"]
["Resistor-F","R7, R19","619 Ω",2,"0204/0207","MRS25000C6190FCT00","Farnell",9469435,8.5000000000000006E-2,0.17,null,"810 Hz"]
["Resistor-F","R8, R20","22.6 kΩ",2,"0204/0207","MRS25000C2262FCT00","Farnell",9466118,8.5000000000000006E-2,0.17,null,"810 Hz"]
["Resistor-F","R9, R21","75 kΩ",2,"0204/0207","MRS25000C7502FCT00","Farnell",9469990,8.4000000000000005E-2,0.16800000000000001,null,"810 Hz"]
["Resistor-F","R10, R22","511 Ω",2,"0204/0207","MRS25000C5110FCT00","Farnell",9468854,7.2999999999999995E-2,0.14599999999999999,null,"810 Hz"]
["Resistor-F","R11, R23","17.8 kΩ",2,"0204/0207","MRS25000C1782FCT00","Farnell",9464956,0.06,0.12,null,"810 Hz"]
["Resistor-F","R12, R24","59 kΩ",2,"0204/0207","MRS25000C5902FCT00","Farnell",9469168,8.6999999999999994E-2,0.17399999999999999,null,"810 Hz"]
["Resistor-F","R1, R13","619 Ω",2,"0204/0207","MRS25000C6190FCT00","Farnell",9469435,8.5000000000000006E-2,0.17,null,"1030 Hz"]
["Resistor-F","R2, R14","18.7 kΩ",2,"0204/0207","MRS25000C1872FCT00","Farnell",9465057,8.6999999999999994E-2,0.17399999999999999,null,"1030 Hz"]
["Resistor-F","R3, R15","38.3 kΩ",2,"0204/0207","MRS25000C3832FCT00","Farnell",9467653,8.6999999999999994E-2,0.17399999999999999,null,"1030 Hz"]
["Resistor-F","R4, R16","590 Ω",2,"0204/0207","MRS25000C5900FCT00","Farnell",9469150,8.6999999999999994E-2,0.17399999999999999,null,"1030 Hz"]
["Resistor-F","R5, R17","17.8 kΩ",2,"0204/0207","MRS25000C1782FCT00","Farnell",9464956,0.06,0.12,null,"1030 Hz"]
["Resistor-F","R6, R18","36.5 kΩ",2,"0204/0207","MRS25000C3652FCT00","Farnell",9467564,8.5000000000000006E-2,0.17,null,"1030 Hz"]
["Resistor-F","R7, R19","487 Ω",2,"0204/0207","MRS25000C4870FCT00","Farnell",9468544,8.5000000000000006E-2,0.17,null,"1030 Hz"]
["Resistor-F","R8, R20","17.8 kΩ",2,"0204/0207","MRS25000C1782FCT00","Farnell",9464956,0.06,0.12,null,"1030 Hz"]
["Resistor-F","R9, R21","59 kΩ",2,"0204/0207","MRS25000C5902FCT00","Farnell",9469168,8.6999999999999994E-2,0.17399999999999999,null,"1030 Hz"]
["Resistor-F","R10, R22","402 Ω",2,"0204/0207","MRS25000C4020FCT00","Farnell",9468145,8.5000000000000006E-2,0.17,null,"1030 Hz"]
["Resistor-F","R11, R23","14 kΩ",2,"0204/0207","MRS25000C1402FCT00","Farnell",9464565,8.6999999999999994E-2,0.17399999999999999,null,"1030 Hz"]
["Resistor-F","R12, R24","46.4 kΩ",2,"0204/0207","MRS25000C4642FCT00","Farnell",9468439,8.6999999999999994E-2,0.17399999999999999,null,"1030 Hz"]
["Resistor-F","R1, R13","487 Ω",2,"0204/0207","MRS25000C4870FCT00","Farnell",9468544,8.5000000000000006E-2,0.17,null,"1310 Hz"]
["Resistor-F","R2, R14","14.7 kΩ",2,"0204/0207","MRS25000C1472FCT00","Farnell",9464581,8.5000000000000006E-2,0.17,null,"1310 Hz"]
["Resistor-F","R3, R15","30.1 kΩ",2,"0204/0207","MRS25000C3012FCT00","Farnell",9467181,8.6999999999999994E-2,0.17399999999999999,null,"1310 Hz"]
["Resistor-F","R4, R16","464 Ω",2,"0204/0207","MRS25000C4640FCT00","Farnell",9468420,8.5000000000000006E-2,0.17,null,"1310 Hz"]
["Resistor-F","R5, R17","14 kΩ",2,"0204/0207","MRS25000C1402FCT00","Farnell",9464565,8.6999999999999994E-2,0.17399999999999999,null,"1310 Hz"]
["Resistor-F","R6, R18","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"1310 Hz"]
["Resistor-F","R7, R19","383 Ω",2,"0204/0207","MRS25000C3830FCT00","Farnell",9467645,8.6999999999999994E-2,0.17399999999999999,null,"1310 Hz"]
["Resistor-F","R8, R20","14 kΩ",2,"0204/0207","MRS25000C1402FCT00","Farnell",9464565,8.6999999999999994E-2,0.17399999999999999,null,"1310 Hz"]
["Resistor-F","R9, R21","46.4 kΩ",2,"0204/0207","MRS25000C4642FCT00","Farnell",9468439,8.6999999999999994E-2,0.17399999999999999,null,"1310 Hz"]
["Resistor-F","R10, R22","316 Ω",2,"0204/0207","MRS25000C3160FCT00","Farnell",9467246,8.5000000000000006E-2,0.17,null,"1310 Hz"]
["Resistor-F","R11, R23","11 kΩ",2,"0204/0207","MRS25000C1102FCT00","Farnell",9464140,5.0999999999999997E-2,0.10199999999999999,null,"1310 Hz"]
["Resistor-F","R12, R24","36.5 kΩ",2,"0204/0207","MRS25000C3652FCT00","Farnell",9467564,8.5000000000000006E-2,0.17,null,"1310 Hz"]
["Resistor-F","R1, R13","383 Ω",2,"0204/0207","MRS25000C3830FCT00","Farnell",9467645,8.6999999999999994E-2,0.17399999999999999,null,"1660 Hz"]
["Resistor-F","R2, R14","11.5 kΩ",2,"0204/0207","MRS25000C1152FCT00","Farnell",9464166,5.0999999999999997E-2,0.10199999999999999,null,"1660 Hz"]
["Resistor-F","R3, R15","23.7 kΩ",2,"0204/0207","MRS25000C2372FCT00","Farnell",9466207,5.0999999999999997E-2,0.10199999999999999,null,"1660 Hz"]
["Resistor-F","R4, R16","365 Ω",2,"0204/0207","MRS25000C3650FCT00","Farnell",9467548,5.0999999999999997E-2,0.10199999999999999,null,"1660 Hz"]
["Resistor-F","R5, R17","11 kΩ",2,"0204/0207","MRS25000C1102FCT00","Farnell",9464140,5.0999999999999997E-2,0.10199999999999999,null,"1660 Hz"]
["Resistor-F","R6, R18","22.6 kΩ",2,"0204/0207","MRS25000C2262FCT00","Farnell",9466118,8.5000000000000006E-2,0.17,null,"1660 Hz"]
["Resistor-F","R7, R19","301 Ω",2,"0204/0207","MRS25000C3010FCT00","Farnell",9467149,8.5000000000000006E-2,0.17,null,"1660 Hz"]
["Resistor-F","R8, R20","11 kΩ",2,"0204/0207","MRS25000C1102FCT00","Farnell",9464140,5.0999999999999997E-2,0.10199999999999999,null,"1660 Hz"]
["Resistor-F","R9, R21","36.5 kΩ",2,"0204/0207","MRS25000C3652FCT00","Farnell",9467564,8.5000000000000006E-2,0.17,null,"1660 Hz"]
["Resistor-F","R10, R22","249 Ω",2,"0204/0207","MRS25000C2490FCT00","Farnell",9466282,8.5999999999999993E-2,0.17199999999999999,null,"1660 Hz"]
["Resistor-F","R11, R23","8.66 kΩ",2,"0204/0207","MRS25000C8661FCT00","Farnell",9470476,8.8999999999999996E-2,0.17799999999999999,null,"1660 Hz"]
["Resistor-F","R12, R24","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"1660 Hz"]
["Resistor-F","R1, R13","1 kΩ",2,"0204/0207","MRS25000C1001FCT00","Farnell",9465170,0.05,0.1,null,"2110 Hz"]
["Resistor-F","R2, R14","30.1 kΩ",2,"0204/0207","MRS25000C3012FCT00","Farnell",9467181,8.6999999999999994E-2,0.17399999999999999,null,"2110 Hz"]
["Resistor-F","R3, R15","61.9 kΩ",2,"0204/0207","MRS25000C6192FCT00","Farnell",9469443,8.5999999999999993E-2,0.17199999999999999,null,"2110 Hz"]
["Resistor-F","R4, R16","953 Ω",2,"0204/0207","MRS25000C9530FCT00","Farnell",9470670,8.5000000000000006E-2,0.17,null,"2110 Hz"]
["Resistor-F","R5, R17","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"2110 Hz"]
["Resistor-F","R6, R18","59 kΩ",2,"0204/0207","MRS25000C5902FCT00","Farnell",9469168,8.6999999999999994E-2,0.17399999999999999,null,"2110 Hz"]
["Resistor-F","R7, R19","787 Ω",2,"0204/0207","MRS25000C7870FCT00","Farnell",9470069,7.2999999999999995E-2,0.14599999999999999,null,"2110 Hz"]
["Resistor-F","R8, R20","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"2110 Hz"]
["Resistor-F","R9, R21","95.3 kΩ",2,"0204/0207","MRS25000C9532FCT00","Farnell",9470689,0.05,0.1,null,"2110 Hz"]
["Resistor-F","R10, R22","649 Ω",2,"0204/0207","MRS25000C6490FCT00","Farnell",9469559,0.05,0.1,null,"2110 Hz"]
["Resistor-F","R11, R23","22.6 kΩ",2,"0204/0207","MRS25000C2262FCT00","Farnell",9466118,8.5000000000000006E-2,0.17,null,"2110 Hz"]
["Resistor-F","R12, R24","75 kΩ",2,"0204/0207","MRS25000C7502FCT00","Farnell",9469990,8.4000000000000005E-2,0.16800000000000001,null,"2110 Hz"]
["Resistor-F","R1, R13","787 Ω",2,"0204/0207","MRS25000C7870FCT00","Farnell",9470069,7.2999999999999995E-2,0.14599999999999999,null,"2680 Hz"]
["Resistor-F","R2, R14","23.7 kΩ",2,"0204/0207","MRS25000C2372FCT00","Farnell",9466207,5.0999999999999997E-2,0.10199999999999999,null,"2680 Hz"]
["Resistor-F","R3, R15","48.7 kΩ",2,"0204/0207","MRS25000C4872FCT00","Farnell",9468552,8.6999999999999994E-2,0.17399999999999999,null,"2680 Hz"]
["Resistor-F","R4, R16","750 Ω",2,"0204/0207","MRS25000C7500FCT00","Farnell",9469982,8.5000000000000006E-2,0.17,null,"2680 Hz"]
["Resistor-F","R5, R17","22.6 kΩ",2,"0204/0207","MRS25000C2262FCT00","Farnell",9466118,8.5000000000000006E-2,0.17,null,"2680 Hz"]
["Resistor-F","R6, R18","46.4 kΩ",2,"0204/0207","MRS25000C4642FCT00","Farnell",9468439,8.6999999999999994E-2,0.17399999999999999,null,"2680 Hz"]
["Resistor-F","R7, R19","619 Ω",2,"0204/0207","MRS25000C6190FCT00","Farnell",9469435,8.5000000000000006E-2,0.17,null,"2680 Hz"]
["Resistor-F","R8, R20","22.6 kΩ",2,"0204/0207","MRS25000C2262FCT00","Farnell",9466118,8.5000000000000006E-2,0.17,null,"2680 Hz"]
["Resistor-F","R9, R21","75 kΩ",2,"0204/0207","MRS25000C7502FCT00","Farnell",9469990,8.4000000000000005E-2,0.16800000000000001,null,"2680 Hz"]
["Resistor-F","R10, R22","511 Ω",2,"0204/0207","MRS25000C5110FCT00","Farnell",9468854,7.2999999999999995E-2,0.14599999999999999,null,"2680 Hz"]
["Resistor-F","R11, R23","17.8 kΩ",2,"0204/0207","MRS25000C1782FCT00","Farnell",9464956,0.06,0.12,null,"2680 Hz"]
["Resistor-F","R12, R24","59 kΩ",2,"0204/0207","MRS25000C5902FCT00","Farnell",9469168,8.6999999999999994E-2,0.17399999999999999,null,"2680 Hz"]
["Resistor-F","R1, R13","619 Ω",2,"0204/0207","MRS25000C6190FCT00","Farnell",9469435,8.5000000000000006E-2,0.17,null,"3410 Hz"]
["Resistor-F","R2, R14","18.7 kΩ",2,"0204/0207","MRS25000C1872FCT00","Farnell",9465057,8.6999999999999994E-2,0.17399999999999999,null,"3410 Hz"]
["Resistor-F","R3, R15","38.3 kΩ",2,"0204/0207","MRS25000C3832FCT00","Farnell",9467653,8.6999999999999994E-2,0.17399999999999999,null,"3410 Hz"]
["Resistor-F","R4, R16","590 Ω",2,"0204/0207","MRS25000C5900FCT00","Farnell",9469150,8.6999999999999994E-2,0.17399999999999999,null,"3410 Hz"]
["Resistor-F","R5, R17","17.8 kΩ",2,"0204/0207","MRS25000C1782FCT00","Farnell",9464956,0.06,0.12,null,"3410 Hz"]
["Resistor-F","R6, R18","36.5 kΩ",2,"0204/0207","MRS25000C3652FCT00","Farnell",9467564,8.5000000000000006E-2,0.17,null,"3410 Hz"]
["Resistor-F","R7, R19","487 Ω",2,"0204/0207","MRS25000C4870FCT00","Farnell",9468544,8.5000000000000006E-2,0.17,null,"3410 Hz"]
["Resistor-F","R8, R20","17.8 kΩ",2,"0204/0207","MRS25000C1782FCT00","Farnell",9464956,0.06,0.12,null,"3410 Hz"]
["Resistor-F","R9, R21","59 kΩ",2,"0204/0207","MRS25000C5902FCT00","Farnell",9469168,8.6999999999999994E-2,0.17399999999999999,null,"3410 Hz"]
["Resistor-F","R10, R22","402 Ω",2,"0204/0207","MRS25000C4020FCT00","Farnell",9468145,8.5000000000000006E-2,0.17,null,"3410 Hz"]
["Resistor-F","R11, R23","14 kΩ",2,"0204/0207","MRS25000C1402FCT00","Farnell",9464565,8.6999999999999994E-2,0.17399999999999999,null,"3410 Hz"]
["Resistor-F","R12, R24","46.4 kΩ",2,"0204/0207","MRS25000C4642FCT00","Farnell",9468439,8.6999999999999994E-2,0.17399999999999999,null,"3410 Hz"]
["Resistor-F","R1, R13","487 Ω",2,"0204/0207","MRS25000C4870FCT00","Farnell",9468544,8.5000000000000006E-2,0.17,null,"4330 Hz"]
["Resistor-F","R2, R14","14.7 kΩ",2,"0204/0207","MRS25000C1472FCT00","Farnell",9464581,8.5000000000000006E-2,0.17,null,"4330 Hz"]
["Resistor-F","R3, R15","30.1 kΩ",2,"0204/0207","MRS25000C3012FCT00","Farnell",9467181,8.6999999999999994E-2,0.17399999999999999,null,"4330 Hz"]
["Resistor-F","R4, R16","464 Ω",2,"0204/0207","MRS25000C4640FCT00","Farnell",9468420,8.5000000000000006E-2,0.17,null,"4330 Hz"]
["Resistor-F","R5, R17","14 kΩ",2,"0204/0207","MRS25000C1402FCT00","Farnell",9464565,8.6999999999999994E-2,0.17399999999999999,null,"4330 Hz"]
["Resistor-F","R6, R18","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"4330 Hz"]
["Resistor-F","R7, R19","383 Ω",2,"0204/0207","MRS25000C3830FCT00","Farnell",9467645,8.6999999999999994E-2,0.17399999999999999,null,"4330 Hz"]
["Resistor-F","R8, R20","14 kΩ",2,"0204/0207","MRS25000C1402FCT00","Farnell",9464565,8.6999999999999994E-2,0.17399999999999999,null,"4330 Hz"]
["Resistor-F","R9, R21","46.4 kΩ",2,"0204/0207","MRS25000C4642FCT00","Farnell",9468439,8.6999999999999994E-2,0.17399999999999999,null,"4330 Hz"]
["Resistor-F","R10, R22","316 Ω",2,"0204/0207","MRS25000C3160FCT00","Farnell",9467246,8.5000000000000006E-2,0.17,null,"4330 Hz"]
["Resistor-F","R11, R23","11 kΩ",2,"0204/0207","MRS25000C1102FCT00","Farnell",9464140,5.0999999999999997E-2,0.10199999999999999,null,"4330 Hz"]
["Resistor-F","R12, R24","36.5 kΩ",2,"0204/0207","MRS25000C3652FCT00","Farnell",9467564,8.5000000000000006E-2,0.17,null,"4330 Hz"]
["Resistor-F","R1, R13","383 Ω",2,"0204/0207","MRS25000C3830FCT00","Farnell",9467645,8.6999999999999994E-2,0.17399999999999999,null,"5500 Hz"]
["Resistor-F","R2, R14","11.5 kΩ",2,"0204/0207","MRS25000C1152FCT00","Farnell",9464166,5.0999999999999997E-2,0.10199999999999999,null,"5500 Hz"]
["Resistor-F","R3, R15","23.7 kΩ",2,"0204/0207","MRS25000C2372FCT00","Farnell",9466207,5.0999999999999997E-2,0.10199999999999999,null,"5500 Hz"]
["Resistor-F","R4, R16","365 Ω",2,"0204/0207","MRS25000C3650FCT00","Farnell",9467548,5.0999999999999997E-2,0.10199999999999999,null,"5500 Hz"]
["Resistor-F","R5, R17","11 kΩ",2,"0204/0207","MRS25000C1102FCT00","Farnell",9464140,5.0999999999999997E-2,0.10199999999999999,null,"5500 Hz"]
["Resistor-F","R6, R18","22.6 kΩ",2,"0204/0207","MRS25000C2262FCT00","Farnell",9466118,8.5000000000000006E-2,0.17,null,"5500 Hz"]
["Resistor-F","R7, R19","301 Ω",2,"0204/0207","MRS25000C3010FCT00","Farnell",9467149,8.5000000000000006E-2,0.17,null,"5500 Hz"]
["Resistor-F","R8, R20","11 kΩ",2,"0204/0207","MRS25000C1102FCT00","Farnell",9464140,5.0999999999999997E-2,0.10199999999999999,null,"5500 Hz"]
["Resistor-F","R9, R21","36.5 kΩ",2,"0204/0207","MRS25000C3652FCT00","Farnell",9467564,8.5000000000000006E-2,0.17,null,"5500 Hz"]
["Resistor-F","R10, R22","249 Ω",2,"0204/0207","MRS25000C2490FCT00","Farnell",9466282,8.5999999999999993E-2,0.17199999999999999,null,"5500 Hz"]
["Resistor-F","R11, R23","8.66 kΩ",2,"0204/0207","MRS25000C8661FCT00","Farnell",9470476,8.8999999999999996E-2,0.17799999999999999,null,"5500 Hz"]
["Resistor-F","R12, R24","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"5500 Hz"]
["Resistor-F","R1, R13","301 Ω",2,"0204/0207","MRS25000C3010FCT00","Farnell",9467149,8.5000000000000006E-2,0.17,null,"7000 Hz"]
["Resistor-F","R2, R14","9.09 kΩ",2,"0204/0207","MRS25000C9091FCT00","Farnell",9470743,8.6999999999999994E-2,0.17399999999999999,null,"7000 Hz"]
["Resistor-F","R3, R15","18.7 kΩ",2,"0204/0207","MRS25000C1872FCT00","Farnell",9465057,8.6999999999999994E-2,0.17399999999999999,null,"7000 Hz"]
["Resistor-F","R4, R16","287 Ω",2,"0204/0207","MRS25000C2870FCT00","Farnell",9466584,5.0999999999999997E-2,0.10199999999999999,null,"7000 Hz"]
["Resistor-F","R5, R17","8.66 kΩ",2,"0204/0207","MRS25000C8661FCT00","Farnell",9470476,8.8999999999999996E-2,0.17799999999999999,null,"7000 Hz"]
["Resistor-F","R6, R18","17.8 kΩ",2,"0204/0207","MRS25000C1782FCT00","Farnell",9464956,0.06,0.12,null,"7000 Hz"]
["Resistor-F","R7, R19","237 Ω",2,"0204/0207","MRS25000C2370FCT00","Farnell",9466185,8.3000000000000004E-2,0.16600000000000001,null,"7000 Hz"]
["Resistor-F","R8, R20","8.66 kΩ",2,"0204/0207","MRS25000C8661FCT00","Farnell",9470476,8.8999999999999996E-2,0.17799999999999999,null,"7000 Hz"]
["Resistor-F","R9, R21","28.7 kΩ",2,"0204/0207","MRS25000C2872FCT00","Farnell",9466606,8.6999999999999994E-2,0.17399999999999999,null,"7000 Hz"]
["Resistor-F","R10, R22","196 Ω",2,"0204/0207","MRS25000C1960FCT00","Farnell",9465120,5.0999999999999997E-2,0.10199999999999999,null,"7000 Hz"]
["Resistor-F","R11, R23","6.81 kΩ",2,"0204/0207","MRS25000C6811FCT00","Farnell",9469818,8.6999999999999994E-2,0.17399999999999999,null,"7000 Hz"]
["Resistor-F","R12, R24","22.6 kΩ",2,"0204/0207","MRS25000C2262FCT00","Farnell",9466118,8.5000000000000006E-2,0.17,null,"7000 Hz"]
["Resistor","R37","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,3.5299999999999998E-2,null,"120 Hz"]
["Resistor","R38","27 kΩ",1,"0204/0207","LR0204F27K","Farnell",2329909,3.5299999999999998E-2,3.5299999999999998E-2,null,"120 Hz"]
["Resistor","R39","10 kΩ",1,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,3.4000000000000002E-2,null,"120 Hz"]
["Resistor","R37","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,3.5299999999999998E-2,null,"150 Hz"]
["Resistor","R38","27 kΩ",1,"0204/0207","LR0204F27K","Farnell",2329909,3.5299999999999998E-2,3.5299999999999998E-2,null,"150 Hz"]
["Resistor","R39","10 kΩ",1,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,3.4000000000000002E-2,null,"150 Hz"]
["Resistor","R37","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,3.5299999999999998E-2,null,"190 Hz"]
["Resistor","R38","27 kΩ",1,"0204/0207","LR0204F27K","Farnell",2329909,3.5299999999999998E-2,3.5299999999999998E-2,null,"190 Hz"]
["Resistor","R39","10 kΩ",1,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,3.4000000000000002E-2,null,"190 Hz"]
["Resistor","R37","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,3.5299999999999998E-2,null,"240 Hz"]
["Resistor","R38","27 kΩ",1,"0204/0207","LR0204F27K","Farnell",2329909,3.5299999999999998E-2,3.5299999999999998E-2,null,"240 Hz"]
["Resistor","R39","10 kΩ",1,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,3.4000000000000002E-2,null,"240 Hz"]
["Resistor","R37","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,3.5299999999999998E-2,null,"310 Hz"]
["Resistor","R38","27 kΩ",1,"0204/0207","LR0204F27K","Farnell",2329909,3.5299999999999998E-2,3.5299999999999998E-2,null,"310 Hz"]
["Resistor","R39","10 kΩ",1,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,3.4000000000000002E-2,null,"310 Hz"]
["Resistor","R37","33 kΩ",1,"0204/0207","LR0204F33K","Farnell",2329922,3.5299999999999998E-2,3.5299999999999998E-2,null,"390 Hz"]
["Resistor","R38","27 kΩ",1,"0204/0207","LR0204F27K","Farnell",2329909,3.5299999999999998E-2,3.5299999999999998E-2,null,"390 Hz"]
["Resistor","R39","10 kΩ",1,"0204/0207","LR0204F10K","Farnell",2329855,3.4000000000000002E-2,3.4000000000000002E-2,null,"390 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"500 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"500 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"500 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"640 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"640 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"640 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"810 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"810 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"810 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"1030 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"1030 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"1030 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"1310 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"1310 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"1310 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"1660 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"1660 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"1660 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"2110 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"2110 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"2110 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"2680 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"2680 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"2680 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"3410 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"3410 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"3410 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"4330 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"4330 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"4330 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"5500 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"5500 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"5500 Hz"]
["Resistor","R37","24 kΩ",1,"0204/0207","LR0204F24K","Farnell",2329904,3.5999999999999997E-2,3.5999999999999997E-2,null,"7000 Hz"]
["Resistor","R38","20 kΩ",1,"0204/0207","LR0204F20K","Farnell",2329897,3.5299999999999998E-2,3.5299999999999998E-2,null,"7000 Hz"]
["Resistor","R39","6.8 kΩ",1,"0204/0207","LR0204F6K8","Farnell",2329969,3.5299999999999998E-2,3.5299999999999998E-2,null,"7000 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","100 nF",16,"SMD (1206 or 0805)","GRM31C5C1H104JA01L","Mouser","81-GRM31C5C1H104JA1L",0.32700000000000001,5.2320000000000002,null,"120 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","100 nF",16,"SMD (1206 or 0805)","GRM31C5C1H104JA01L","Mouser","81-GRM31C5C1H104JA1L",0.32700000000000001,5.2320000000000002,null,"150 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","100 nF",16,"SMD (1206 or 0805)","GRM31C5C1H104JA01L","Mouser","81-GRM31C5C1H104JA1L",0.32700000000000001,5.2320000000000002,null,"190 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","100 nF",16,"SMD (1206 or 0805)","GRM31C5C1H104JA01L","Mouser","81-GRM31C5C1H104JA1L",0.32700000000000001,5.2320000000000002,null,"240 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","100 nF",16,"SMD (1206 or 0805)","GRM31C5C1H104JA01L","Mouser","81-GRM31C5C1H104JA1L",0.32700000000000001,5.2320000000000002,null,"310 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","100 nF",16,"SMD (1206 or 0805)","GRM31C5C1H104JA01L","Mouser","81-GRM31C5C1H104JA1L",0.32700000000000001,5.2320000000000002,null,"390 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","33 nF",16,"SMD (1206 or 0805)","CGA5F2C0G1H333J085AA","Mouser","810-CGA5F2C0G1H333J",0.16,2.56,null,"500 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","33 nF",16,"SMD (1206 or 0805)","CGA5F2C0G1H333J085AA","Mouser","810-CGA5F2C0G1H333J",0.16,2.56,null,"640 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","33 nF",16,"SMD (1206 or 0805)","CGA5F2C0G1H333J085AA","Mouser","810-CGA5F2C0G1H333J",0.16,2.56,null,"810 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","33 nF",16,"SMD (1206 or 0805)","CGA5F2C0G1H333J085AA","Mouser","810-CGA5F2C0G1H333J",0.16,2.56,null,"1030 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","33 nF",16,"SMD (1206 or 0805)","CGA5F2C0G1H333J085AA","Mouser","810-CGA5F2C0G1H333J",0.16,2.56,null,"1310 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","33 nF",16,"SMD (1206 or 0805)","CGA5F2C0G1H333J085AA","Mouser","810-CGA5F2C0G1H333J",0.16,2.56,null,"1660 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","10 nF",16,"SMD (1206 or 0805)","08055A103JAT2A","Mouser","581-08055A103JAT2A",0.224,3.5840000000000001,null,"2110 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","10 nF",16,"SMD (1206 or 0805)","08055A103JAT2A","Mouser","581-08055A103JAT2A",0.224,3.5840000000000001,null,"2680 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","10 nF",16,"SMD (1206 or 0805)","08055A103JAT2A","Mouser","581-08055A103JAT2A",0.224,3.5840000000000001,null,"3410 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","10 nF",16,"SMD (1206 or 0805)","08055A103JAT2A","Mouser","581-08055A103JAT2A",0.224,3.5840000000000001,null,"4330 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","10 nF",16,"SMD (1206 or 0805)","08055A103JAT2A","Mouser","581-08055A103JAT2A",0.224,3.5840000000000001,null,"5500 Hz"]
["Ceramic","C1, C2, C3, C4, C5, C6, C7, C8, C9, C10, C11, C12, C13, C14, C15, C16","10 nF",16,"SMD (1206 or 0805)","08055A103JAT2A","Mouser","581-08055A103JAT2A",0.224,3.5840000000000001,null,"7000 Hz"]

{"sheet":"Minimum Order Count","index":16,"n_rows":275,"n_cols":3,"rows_kept":275,"cut":false,"hidden":false,"merged":[]}
["LR0204F10R",10,"Farnell"]
["LR0204F47R",100,"Farnell"]
["LR0204F100R",10,"Farnell"]
["LR0204F220R",10,"Farnell"]
["LR0204F430R",10,"Farnell"]
["LR0204F470R",10,"Farnell"]
["LR0204F510R",10,"Farnell"]
["LR0204F560R",10,"Farnell"]
["LR0204F620R",10,"Farnell"]
["LR0204F750R",10,"Farnell"]
["LR0204F820R",10,"Farnell"]
["LR0204F1K0",10,"Farnell"]
["LR0204F1K5",10,"Farnell"]
["LR0204F1K6",10,"Farnell"]
["LR0204F2K0",10,"Farnell"]
["LR0204F2K2",10,"Farnell"]
["LR0204F2K4",10,"Farnell"]
["LR0204F2K7",10,"Farnell"]
["LR0204F3K3",10,"Farnell"]
["LR0204F3K9",10,"Farnell"]
["LR0204F4K7",10,"Farnell"]
["LR0204F5K1",10,"Farnell"]
["LR0204F5K6",10,"Farnell"]
["LR0204F6K2",10,"Farnell"]
["LR0204F6K8",10,"Farnell"]
["LR0204F7K5",10,"Farnell"]
["LR0204F8K2",10,"Farnell"]
["LR0204F10K",100,"Farnell"]
["LR0204F12K",10,"Farnell"]
["LR0204F13K",10,"Farnell"]
["LR0204F15K",10,"Farnell"]
["LR0204F18K",10,"Farnell"]
["LR0204F20K",10,"Farnell"]
["LR0204F22K",10,"Farnell"]
["LR0204F24K",10,"Farnell"]
["LR0204F27K",10,"Farnell"]
["LR0204F30K",10,"Farnell"]
["LR0204F33K",10,"Farnell"]
["LR0204F36K",10,"Farnell"]
["LR0204F39K",10,"Farnell"]
["LR0204F47K",100,"Farnell"]
["LR0204F51K",10,"Farnell"]
["LR0204F56K",10,"Farnell"]
["LR0204F62K",10,"Farnell"]
["LR0204F75K",10,"Farnell"]
["LR0204F91K",10,"Farnell"]
["LR0204F100K",100,"Farnell"]
["LR0204F120K",10,"Farnell"]
["LR0204F150K",10,"Farnell"]
["LR0204F180K",10,"Farnell"]
["LR0204F200K",10,"Farnell"]
["LR0204F220K",10,"Farnell"]
["MFR3-330KFC",10,"Farnell"]
["LR0204F390K",10,"Farnell"]
["LR0204F430K",10,"Farnell"]
["LR0204F470K",10,"Farnell"]
["MRS25000C8203FCT00",10,"Farnell"]
["LR0204F1M0",10,"Farnell"]
["MRS25000C1504FCT00",10,"Farnell"]
["MRS25000C2004FCT00",10,"Farnell"]
["MRS25000C6804FCT00",10,"Farnell"]
["CFR16J2M2",10,"Farnell"]
["CFR16J3M3",10,"Farnell"]
["CFR16J4M7",10,"Farnell"]
[]
["MRS25000C1960FCT00",10,"Farnell"]
["MRS25000C2370FCT00",10,"Farnell"]
["MRS25000C2490FCT00",10,"Farnell"]
["MRS25000C2870FCT00",10,"Farnell"]
["MRS25000C3010FCT00",10,"Farnell"]
["MRS25000C3160FCT00",10,"Farnell"]
["MRS25000C3480FCT00",10,"Farnell"]
["MRS25000C3650FCT00",10,"Farnell"]
["MRS25000C3830FCT00",10,"Farnell"]
["MRS25000C4020FCT00",10,"Farnell"]
["MRS25000C4220FCT00",10,"Farnell"]
["MRS25000C4420FCT00",10,"Farnell"]
["MRS25000C4640FCT00",10,"Farnell"]
["MRS25000C4870FCT00",10,"Farnell"]
["MRS25000C5110FCT00",10,"Farnell"]
["MRS25000C5360FCT00",10,"Farnell"]
["MRS25000C5620FCT00",10,"Farnell"]
["MRS25000C5900FCT00",10,"Farnell"]
["MRS25000C6190FCT00",10,"Farnell"]
["MRS25000C6490FCT00",10,"Farnell"]
["MRS25000C6810FCT00",10,"Farnell"]
["MRS25000C7150FCT00",10,"Farnell"]
["MRS25000C7500FCT00",10,"Farnell"]
["MRS25000C7870FCT00",10,"Farnell"]
["MRS25000C8250FCT00",10,"Farnell"]
["MRS25000C8660FCT00",10,"Farnell"]
["MRS25000C9090FCT00",10,"Farnell"]
["MRS25000C9530FCT00",10,"Farnell"]
["MRS25000C1001FCT00",10,"Farnell"]
["MRS25000C1051FCT00",10,"Farnell"]
["MRS25000C1101FCT00",10,"Farnell"]
["MRS25000C1151FCT00",10,"Farnell"]
["MRS25000C1211FCT00",10,"Farnell"]
["MRS25000C1271FCT00",10,"Farnell"]
["MRS25000C1331FCT00",10,"Farnell"]
["MRS25000C1401FCT00",10,"Farnell"]
["MRS25000C1691FCT00",10,"Farnell"]
["MRS25000C1781FCT00",10,"Farnell"]
["MRS25000C6811FCT00",10,"Farnell"]
["MRS25000C8661FCT00",10,"Farnell"]
["MRS25000C9091FCT00",10,"Farnell"]
["MRS25000C1102FCT00",10,"Farnell"]
["MRS25000C1152FCT00",10,"Farnell"]
["MRS25000C1212FCT00",10,"Farnell"]
["MRS25000C1402FCT00",10,"Farnell"]
["MRS25000C1472FCT00",10,"Farnell"]
["MRS25000C1542FCT00",10,"Farnell"]
["MRS25000C1622FCT00",10,"Farnell"]
["MRS25000C1782FCT00",10,"Farnell"]
["MRS25000C1872FCT00",10,"Farnell"]
["MRS25000C1962FCT00",10,"Farnell"]
["MRS25000C2052FCT00",10,"Farnell"]
["MRS25000C2262FCT00",10,"Farnell"]
["MRS25000C2372FCT00",10,"Farnell"]
["MRS25000C2492FCT00",10,"Farnell"]
["MRS25000C2612FCT00",10,"Farnell"]
["MRS25000C2872FCT00",10,"Farnell"]
["MRS25000C3012FCT00",10,"Farnell"]
["MRS25000C3162FCT00",10,"Farnell"]
["MRS25000C3322FCT00",10,"Farnell"]
["MRS25000C3652FCT00",10,"Farnell"]
["MRS25000C3832FCT00",10,"Farnell"]
["MRS25000C4022FCT00",10,"Farnell"]
["MRS25000C4222FCT00",10,"Farnell"]
["MRS25000C4642FCT00",10,"Farnell"]
["MRS25000C4872FCT00",10,"Farnell"]
["MRS25000C5112FCT00",10,"Farnell"]
["MRS25000C5362FCT00",10,"Farnell"]
["MRS25000C5902FCT00",10,"Farnell"]
["MRS25000C6192FCT00",10,"Farnell"]
["MRS25000C6492FCT00",10,"Farnell"]
["MRS25000C6812FCT00",10,"Farnell"]
["MRS25000C7502FCT00",10,"Farnell"]
["MRS25000C7872FCT00",10,"Farnell"]
["MRS25000C8252FCT00",10,"Farnell"]
["MRS25000C8662FCT00",10,"Farnell"]
["MRS25000C9532FCT00",10,"Farnell"]
["MRS25000C1053FCT00",10,"Farnell"]
["MRS25000C1103FCT00",10,"Farnell"]
["MRS25000C1213FCT00",10,"Farnell"]
["MRS25000C1333FCT00",10,"Farnell"]
["MRS25000C1693FCT00",10,"Farnell"]
[]
["C1206C104K5RACTU",500,"Farnell"]
[]
["S2B-EH(LF)(SN)",100,"Farnell"]
["S3B-EH(LF)(SN)",100,"Farnell"]
["EHR-2",100,"Farnell"]
["EHR-3",100,"Farnell"]
["SEH-001T-P0.6",10,"Farnell"]
[]
["J113",5,"Farnell"]
[]
["1N4148TR",100,"Farnell"]
["1N4148",100,"Mouser"]
[]
["K220J15C0GF53L2",10,"Farnell"]
["K101J15C0GF53L2",10,"Farnell"]
["K221J15C0GF53L2",10,"Farnell"]
["K471J15C0GF53L2",10,"Farnell"]
["K103K15X7RF53L2",10,"Farnell"]
["K102J15C0GF53L2",10,"Farnell"]
[]
["R82EC1100AA50K",5,"Farnell"]
["R82EC1220DQ50J",5,"Farnell"]
["R82EC1470CK50J",5,"Farnell"]
["R82EC2100AA50J",5,"Farnell"]
["R82EC2220AA50J",5,"Farnell"]
["R82EC2470AA60J",5,"Farnell"]
["R82EC3100AA70J",5,"Farnell"]
["R82DC3220Z360K",50,"RS-Online"]
["R82DC3330AA60K",5,"Farnell"]
[]
["VJ0805Y104KXACW1BC",100,"Farnell"]
["3M 969102-0000-DA",10,"Farnell"]
[]
["Voigt 1364A.61",200,"Bürklin"]
[]
["CD4053BEE4",25,"RS-Online"]
[]
["GRM2195C1H103FA01D",100,"Farnell"]
["GRM3195C1H333JA01D  ",100,"Farnell"]
["GRM31C5C1H104JA01L",100,"Farnell"]
[]
["Würth 860010372004",100,"Farnell"]
[]
["1N4002",10,"Farnell"]
["knobs",25,"Thonk"]
["PT 10 LH 25K",50,"Bürklin"]
["T93XA 100K",10,"Bürklin"]
[]
["TLLR4400",25,"Farnell"]
["TLLG4400",10,"Farnell"]
["TLLR4401",25,"Farnell"]
["TLLG4401",5,"Farnell"]
["TLLY4401",5,"Farnell"]
[]
["2227MC-08-03-18-F1",25,"Farnell"]
["2227MC-16-03-09-F1",25,"Farnell"]
["2227MC-14-03-10-F1",100,"Farnell"]
[]
["AR 08 HZL-TT",30,"RS-Online"]
["AR 14 HZL-TT",100,"RS-Online"]
["AR 16 HZL-TT",30,"RS-Online"]
[]
["MFR3-100RFC",10,"Farnell"]
["MFR3-470RFC",10,"Farnell"]
["MFR3-1K0FC",10,"Farnell"]
["MFR3-2K2FC",10,"Farnell"]
["MFR3-2K7FC",10,"Farnell"]
["MFR3-3K3FC",10,"Farnell"]
["MFR3-3K9FC",10,"Farnell"]
["MFR3-4K7FC",10,"Farnell"]
["MFR3-5K6FC",10,"Farnell"]
["MFR3-6K8FC",10,"Farnell"]
["MFR3-8K2FC",10,"Farnell"]
["MFR3-10KFC",10,"Farnell"]
["MFR3-12KFC",10,"Farnell"]
["MFR3-15KFC",10,"Farnell"]
["MFR3-18KFC",10,"Farnell"]
["MFR3-22KFC",10,"Farnell"]
["MFR3-27KFC",10,"Farnell"]
["MFR3-33KFC",10,"Farnell"]
["MFR3-39KFC",10,"Farnell"]
["MFR3-47KFC",10,"Farnell"]
["MFR3-56KFC",10,"Farnell"]
["MFR3-100KFC",10,"Farnell"]
["MFR3-120KFC",10,"Farnell"]
["MFR3-220KFC",10,"Farnell"]
["MFR3-330KFC",10,"Farnell"]
["MFR3-470KFC",10,"Farnell"]
[]
["CFR16J4M7",10,"Farnell"]
[]
["2N3904BU",100,"Farnell"]
["1N4001G",5,"Farnell"]
[]
["R82DC4100Z360K",10,"Mouser"]
[]
["Würth 860020672006",3,"Farnell"]
["Würth 860020672007",3,"Farnell"]
["Würth 860020672010",5,"Farnell"]
["Würth 860010572003",10,"Farnell"]
["Würth 860010572005",100,"Mouser"]
["Würth 860010473007",10,"Farnell"]
[]
["531-PT10H-25K",50,"Mouser"]
["T93XA104KT20",10,"Mouser"]
[]
["2227MC-18-03-18-F1",5,"Farnell"]
["CL1345G",50,"Farnell"]
[]
["Vogt 1364A.68",200,"Conrad"]
[]
["Würth 61300421021",25,"Mouser"]
["Würth 61301621021",10,"Mouser"]
["MC-2228CG",50,"Mouser"]
[]
["AMP 9-160479-5",10,"Farnell"]
["NE5532AP",10,"Mouser"]
[]
["GCM2195C1H103FA16D",100,"Mouser"]
["C3216C0G1H333J085AA",100,"Mouser"]
["C3216NP01H104J160AA",100,"Mouser"]
[]
["Schurter 0001.2513",10,"Farnell"]
[]
["08055A103JAT2A",100,"Mouser"]
["CGA5F2C0G1H333J085AA",100,"Mouser"]
["GRM31C5C1H104JA01L",100,"Mouser"]

{"sheet":"Resistor pricing","index":17,"n_rows":315,"n_cols":14,"rows_kept":315,"cut":false,"hidden":false,"merged":[]}
["10 Ω","Resistor",2329856,"LR0204F10R","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["47 Ω, 250 mW","Resistor",2329945,"LR0204F47R","Farnell","Farnell",10,7.4999999999999997E-2,100,4.0800000000000003E-2]
["100 Ω","Resistor",2329854,"LR0204F100R","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["220 Ω","Resistor",2329900,"LR0204F220R","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["430 Ω","Resistor",2329938,"LR0204F430R","Farnell","Farnell",10,3.7199999999999997E-2,100,2.7900000000000001E-2]
["470 Ω","Resistor",2329942,"LR0204F470R","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["510 Ω","Resistor",2329949,"LR0204F510R","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["560 Ω","Resistor",2329953,"LR0204F560R","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["620 Ω","Resistor",2329960,"LR0204F620R","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["750 Ω","Resistor",2329971,"LR0204F750R","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["820 Ω","Resistor",2329976,"LR0204F820R","Farnell","Farnell",10,7.7100000000000002E-2,100,4.1500000000000002E-2]
["1 kΩ","Resistor",2329885,"LR0204F1K0","Farnell","Farnell",10,7.7100000000000002E-2,100,4.1500000000000002E-2]
["1.5 kΩ","Resistor",2329891,"LR0204F1K5","Farnell","Farnell",10,7.5700000000000003E-2,100,4.0800000000000003E-2]
["1.6 kΩ","Resistor",2329892,"LR0204F1K6","Farnell","Farnell",10,3.5000000000000003E-2,100,2.5999999999999999E-2]
["2.2 kΩ","Resistor",2329912,"LR0204F2K2","Farnell","Farnell",10,7.7100000000000002E-2,100,4.1500000000000002E-2]
["3.3 kΩ","Resistor",2329934,"LR0204F3K3","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["3.9 kΩ","Resistor",2329936,"LR0204F3K9","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["4.7 kΩ","Resistor",2329947,"LR0204F4K7","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["5.1 kΩ","Resistor",2329957,"LR0204F5K1","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["5.6 kΩ","Resistor",2329958,"LR0204F5K6","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["6.2 kΩ","Resistor",2329968,"LR0204F6K2","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["6.8 kΩ","Resistor",2329969,"LR0204F6K8","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["7.5 kΩ","Resistor",2329974,"LR0204F7K5","Farnell","Farnell",10,8.1199999999999994E-2,100,3.9300000000000002E-2]
["8.2 kΩ","Resistor",2329981,"LR0204F8K2","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["10 kΩ","Resistor",2329855,"LR0204F10K","Farnell","Farnell",10,3.4000000000000002E-2,100,2.5499999999999998E-2]
["12 kΩ","Resistor",2329863,"LR0204F12K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["15 kΩ","Resistor",2329873,"LR0204F15K","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["18 kΩ","Resistor",2329882,"LR0204F18K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["20 kΩ","Resistor",2329897,"LR0204F20K","Farnell","Farnell",10,3.6299999999999999E-2,100,2.6499999999999999E-2]
["22 kΩ","Resistor",2329901,"LR0204F22K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["24 kΩ","Resistor",2329904,"LR0204F24K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["27 kΩ","Resistor",2329909,"LR0204F27K","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["30 kΩ","Resistor",2329917,"LR0204F30K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["33 kΩ","Resistor",2329922,"LR0204F33K","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["36 kΩ","Resistor",2329927,"LR0204F36K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["39 kΩ","Resistor",2329932,"LR0204F39K","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["47 kΩ","Resistor",2329944,"LR0204F47K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["51 kΩ","Resistor",2329950,"LR0204F51K","Farnell","Farnell",10,5.1999999999999998E-2,100,3.4000000000000002E-2]
["56 kΩ","Resistor",2329954,"LR0204F56K","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["62 kΩ","Resistor",2329961,"LR0204F62K","Farnell","Farnell",10,7.7100000000000002E-2,100,4.1500000000000002E-2]
["75 kΩ","Resistor",2329972,"LR0204F75K","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["91 kΩ","Resistor",2329984,"LR0204F91K","Farnell","Farnell",10,3.4700000000000002E-2,100,2.5999999999999999E-2]
["100 kΩ","Resistor",2329853,"LR0204F100K","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["120 kΩ","Resistor",2329861,"LR0204F120K","Farnell","Farnell",10,8.5699999999999998E-2,100,4.6199999999999998E-2]
["150 kΩ","Resistor",2329871,"LR0204F150K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["180 kΩ","Resistor",2329880,"LR0204F180K","Farnell","Farnell",10,4.4699999999999997E-2,100,3.1899999999999998E-2]
["200 kΩ","Resistor",2329895,"LR0204F200K","Farnell","Farnell",10,3.4700000000000002E-2,100,2.5999999999999999E-2]
["220 kΩ","Resistor",2329899,"LR0204F220K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["330 kΩ","Resistor",1565303,"MFR3-330KFC","Farnell","Farnell",10,4.2500000000000003E-2,100,2.58E-2]
["390 kΩ","Resistor",2329929,"LR0204F390K","Farnell","Farnell",10,3.5999999999999997E-2,100,2.7E-2]
["470 kΩ","Resistor",2329941,"LR0204F470K","Farnell","Farnell",10,5.1999999999999998E-2,100,3.4700000000000002E-2]
["820 kΩ","Resistor",9470239,"MRS25000C8203FCT00","Farnell","Farnell",10,9.0999999999999998E-2,100,6.0699999999999997E-2]
["1 MΩ","Resistor",2329894,"LR0204F1M0","Farnell","Farnell",10,3.5299999999999998E-2,100,2.6499999999999999E-2]
["1.5 MΩ","Resistor",9465537,"MRS25000C1504FCT00","Farnell","Farnell",10,5.2400000000000002E-2,100,3.8699999999999998E-2]
["2 MΩ","Resistor",9466878,"MRS25000C2004FCT00","Farnell","Farnell",10,8.8999999999999996E-2,100,5.9299999999999999E-2]
["2.2 MΩ, 5%","Resistor",2329510,"CFR16J2M2","Farnell","Farnell",10,2.46E-2,100,1.84E-2]
["3.3 MΩ, 5%","Resistor",2329524,"CFR16J3M3","Farnell","Farnell",10,5.2900000000000003E-2,100,2.8500000000000001E-2]
["4.7 MΩ, 5%","Resistor",2329535,"CFR16J4M7","Farnell","Farnell",10,5.2900000000000003E-2,100,2.8500000000000001E-2]
["6.8 MΩ","Resistor",9469842,"MRS25000C6804FCT00","Farnell","Farnell",10,5.2900000000000003E-2,100,3.9100000000000003E-2]
["196 Ω","Resistor-F","9465120","MRS25000C1960FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,3.6999999999999998E-2]
["237 Ω","Resistor-F","9466185","MRS25000C2370FCT00","Farnell","Farnell",10,8.3000000000000004E-2,100,5.8000000000000003E-2]
["249 Ω","Resistor-F","9466282","MRS25000C2490FCT00","Farnell","Farnell",10,8.5999999999999993E-2,100,5.7000000000000002E-2]
["287 Ω","Resistor-F","9466584","MRS25000C2870FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,3.6999999999999998E-2]
["301 Ω","Resistor-F","9467149","MRS25000C3010FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["316 Ω","Resistor-F","9467246","MRS25000C3160FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["348 Ω","Resistor-F","9467424","MRS25000C3480FCT00","Farnell","Farnell",10,7.2999999999999995E-2,100,5.8000000000000003E-2]
["365 Ω","Resistor-F","9467548","MRS25000C3650FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,4.5999999999999999E-2]
["383 Ω","Resistor-F","9467645","MRS25000C3830FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["402 Ω","Resistor-F","9468145","MRS25000C4020FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.6000000000000001E-2]
["422 Ω","Resistor-F","9468226","MRS25000C4220FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["442 Ω","Resistor-F","9468340","MRS25000C4420FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.7000000000000002E-2]
["464 Ω","Resistor-F","9468420","MRS25000C4640FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["487 Ω","Resistor-F","9468544","MRS25000C4870FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["511 Ω","Resistor-F","9468854","MRS25000C5110FCT00","Farnell","Farnell",10,7.2999999999999995E-2,100,5.8000000000000003E-2]
["536 Ω","Resistor-F","9468951","MRS25000C5360FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["562 Ω","Resistor-F","9469052","MRS25000C5620FCT00","Farnell","Farnell",10,6.5000000000000002E-2,100,4.7E-2]
["590 Ω","Resistor-F","9469150","MRS25000C5900FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["619 Ω","Resistor-F","9469435","MRS25000C6190FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["649 Ω","Resistor-F","9469559","MRS25000C6490FCT00","Farnell","Farnell",10,0.05,100,3.6999999999999998E-2]
["681 Ω","Resistor-F","9469656","MRS25000C6810FCT00","Farnell","Farnell",10,8.4000000000000005E-2,100,5.8000000000000003E-2]
["715 Ω","Resistor-F","9469907","MRS25000C7150FCT00","Farnell","Farnell",10,8.7999999999999995E-2,100,5.8000000000000003E-2]
["750 Ω","Resistor-F","9469982","MRS25000C7500FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["787 Ω","Resistor-F","9470069","MRS25000C7870FCT00","Farnell","Farnell",10,7.2999999999999995E-2,100,5.8000000000000003E-2]
["825 Ω","Resistor-F","9470263","MRS25000C8250FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["866 Ω","Resistor-F","9470360","MRS25000C8660FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["909 Ω","Resistor-F","9470549","MRS25000C9090FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,3.7999999999999999E-2]
["953 Ω","Resistor-F","9470670","MRS25000C9530FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["1 kΩ","Resistor-F","9465170","MRS25000C1001FCT00","Farnell","Farnell",10,0.05,100,3.6999999999999998E-2]
["1.05 kΩ","Resistor-F","9465197","MRS25000C1051FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["1.1 kΩ","Resistor-F","9465219","MRS25000C1101FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["1.15 kΩ","Resistor-F","9465235","MRS25000C1151FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["1.21 kΩ","Resistor-F","9465260","MRS25000C1211FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,3.6999999999999998E-2]
["1.27 kΩ","Resistor-F","9465286","MRS25000C1271FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["1.33 kΩ","Resistor-F","9465308","MRS25000C1331FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["1.4 kΩ","Resistor-F","9465324","MRS25000C1401FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["1.69 kΩ","Resistor-F","9465413","MRS25000C1691FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["1.78 kΩ","Resistor-F","9465430","MRS25000C1781FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.6000000000000001E-2]
["6.81 kΩ","Resistor-F","9469818","MRS25000C6811FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["8.66 kΩ","Resistor-F","9470476","MRS25000C8661FCT00","Farnell","Farnell",10,8.8999999999999996E-2,100,0.06]
["9.09 kΩ","Resistor-F","9470743","MRS25000C9091FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["11 kΩ","Resistor-F","9464140","MRS25000C1102FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,3.6999999999999998E-2]
["11.5 kΩ","Resistor-F","9464166","MRS25000C1152FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,4.5999999999999999E-2]
["12.1 kΩ","Resistor-F","9464310","MRS25000C1212FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["14 kΩ","Resistor-F","9464565","MRS25000C1402FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["14.7 kΩ","Resistor-F","9464581","MRS25000C1472FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["15.4 kΩ","Resistor-F","9464697","MRS25000C1542FCT00","Farnell","Farnell",10,8.4000000000000005E-2,100,5.8000000000000003E-2]
["16.2 kΩ","Resistor-F","9464832","MRS25000C1622FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["17.8 kΩ","Resistor-F","9464956","MRS25000C1782FCT00","Farnell","Farnell",10,0.06,100,5.8000000000000003E-2]
["18.7 kΩ","Resistor-F","9465057","MRS25000C1872FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["19.6 kΩ","Resistor-F","9465146","MRS25000C1962FCT00","Farnell","Farnell",10,8.4000000000000005E-2,100,5.6000000000000001E-2]
["20.5 kΩ","Resistor-F","9465928","MRS25000C2052FCT00","Farnell","Farnell",10,8.1000000000000003E-2,100,5.8000000000000003E-2]
["22.6 kΩ","Resistor-F","9466118","MRS25000C2262FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.8000000000000003E-2]
["23.7 kΩ","Resistor-F","9466207","MRS25000C2372FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,4.3999999999999997E-2]
["24.9 kΩ","Resistor-F","9466312","MRS25000C2492FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["26.1 kΩ","Resistor-F","9466436","MRS25000C2612FCT00","Farnell","Farnell",10,8.7999999999999995E-2,100,5.8000000000000003E-2]
["28.7 kΩ","Resistor-F","9466606","MRS25000C2872FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["30.1 kΩ","Resistor-F","9467181","MRS25000C3012FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["31.6 kΩ","Resistor-F","9467254","MRS25000C3162FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,3.6999999999999998E-2]
["33.2 kΩ","Resistor-F","9467360","MRS25000C3322FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["36.5 kΩ","Resistor-F","9467564","MRS25000C3652FCT00","Farnell","Farnell",10,8.5000000000000006E-2,100,5.6000000000000001E-2]
["38.3 kΩ","Resistor-F","9467653","MRS25000C3832FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["40.2 kΩ","Resistor-F","9468153","MRS25000C4022FCT00","Farnell","Farnell",10,8.4000000000000005E-2,100,5.6000000000000001E-2]
["42.2 kΩ","Resistor-F","9468234","MRS25000C4222FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,3.7999999999999999E-2]
["46.4 kΩ","Resistor-F","9468439","MRS25000C4642FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["48.7 kΩ","Resistor-F","9468552","MRS25000C4872FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["51.1 kΩ","Resistor-F","9468870","MRS25000C5112FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["53.6 kΩ","Resistor-F","9468960","MRS25000C5362FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,3.6999999999999998E-2]
["59 kΩ","Resistor-F","9469168","MRS25000C5902FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["61.9 kΩ","Resistor-F","9469443","MRS25000C6192FCT00","Farnell","Farnell",10,8.5999999999999993E-2,100,5.7000000000000002E-2]
["64.9 kΩ","Resistor-F","9469567","MRS25000C6492FCT00","Farnell","Farnell",10,0.06,100,0.06]
["68.1 kΩ","Resistor-F","9469672","MRS25000C6812FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["75 kΩ","Resistor-F","9469990","MRS25000C7502FCT00","Farnell","Farnell",10,8.4000000000000005E-2,100,5.8000000000000003E-2]
["78.7 kΩ","Resistor-F","9470077","MRS25000C7872FCT00","Farnell","Farnell",10,0.06,100,5.7000000000000002E-2]
["82.5 kΩ","Resistor-F","9470280","MRS25000C8252FCT00","Farnell","Farnell",10,0.06,100,5.8000000000000003E-2]
["86.6 kΩ","Resistor-F","9470379","MRS25000C8662FCT00","Farnell","Farnell",10,0.06,100,5.8000000000000003E-2]
["95.3 kΩ","Resistor-F","9470689","MRS25000C9532FCT00","Farnell","Farnell",10,0.05,100,3.6999999999999998E-2]
["105 kΩ","Resistor-F","9463933","MRS25000C1053FCT00","Farnell","Farnell",10,4.9000000000000002E-2,100,3.5999999999999997E-2]
["110 kΩ","Resistor-F","9464069","MRS25000C1103FCT00","Farnell","Farnell",10,5.0999999999999997E-2,100,3.6999999999999998E-2]
["121 kΩ","Resistor-F","9464247","MRS25000C1213FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,5.8000000000000003E-2]
["133 kΩ","Resistor-F","9464409","MRS25000C1333FCT00","Farnell","Farnell",10,8.4000000000000005E-2,100,5.8000000000000003E-2]
["169 kΩ","Resistor-F","9464808","MRS25000C1693FCT00","Farnell","Farnell",10,8.6999999999999994E-2,100,0.06]
["10 Ω","Resistor","603-MFR-12FTF52-10R","MFR-12FTF52-10R","Mouser","Mouser",1,0.122,10,6.2E-2,100,2.1999999999999999E-2,null,{"$f":"IF(MID(A142,FIND(\"Ω\",A142)-1,1)=\"k\",LEFT(A142,FIND(\"k\",A142)-1)*1000,LEFT(A142,FIND(\"Ω\",A142)-1)*1)","v":10}]
["47 Ω, 250 mW","Resistor",{"$f":"CONCATENATE(\"603-MFR-12FTF52-\",IF(N143<1000,CONCATENATE(N143,\"R\"),IF(N143<10000,CONCATENATE(TRUNC(N143/1000),\"K\",TRUNC((N143/1000-TRUNC(N143/1000))*10+0.01)),IF(N143<1000000,CONCATENATE(N143/1000,\"K\")))))","v":"603-MFR-12FTF52-47R"},{"$f":"RIGHT(C143,LEN(C143)-4)","v":"MFR-12FTF52-47R"},"Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,{"$f":"IF(MID(A143,FIND(\"Ω\",A143)-1,1)=\"k\",LEFT(A143,FIND(\"k\",A143)-1)*1000,LEFT(A143,FIND(\"Ω\",A143)-1)*1)","v":47}]
["100 Ω","Resistor",{"$f":"CONCATENATE(\"603-MFR-12FTF52-\",IF(N144<1000,CONCATENATE(N144,\"R\"),IF(N144<10000,CONCATENATE(TRUNC(N144/1000),\"K\",TRUNC((N144/1000-TRUNC(N144/1000))*10+0.01)),IF(N144<1000000,CONCATENATE(N144/1000,\"K\")))))","v":"603-MFR-12FTF52-100R"},{"$f":"RIGHT(C144,LEN(C144)-4)","v":"MFR-12FTF52-100R"},"Mouser","Mouser",1,0.10199999999999999,10,0.06,100,2.5999999999999999E-2,null,{"$f":"IF(MID(A144,FIND(\"Ω\",A144)-1,1)=\"k\",LEFT(A144,FIND(\"k\",A144)-1)*1000,LEFT(A144,FIND(\"Ω\",A144)-1)*1)","v":100}]
["220 Ω","Resistor","603-MFR-12FTF52-220R","MFR-12FTF52-220R","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,220]
["430 Ω","Resistor","603-MFR-12FTF52-430R","MFR-12FTF52-430R","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,430]
["470 Ω","Resistor","603-MFR-12FTF52-470R","MFR-12FTF52-470R","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,470]
["510 Ω","Resistor","603-MFR-12FTF52-510R","MFR-12FTF52-510R","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,510]
["560 Ω","Resistor","603-MFR-12FTF52-560R","MFR-12FTF52-560R","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,560]
["620 Ω","Resistor","603-MFR-12FTF52-620R","MFR-12FTF52-620R","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,620]
["750 Ω","Resistor","603-MFR-12FTF52-750R","MFR-12FTF52-750R","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,750]
["820 Ω","Resistor","603-MFR-12FTF52-820R","MFR-12FTF52-820R","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,820]
["1 kΩ","Resistor","603-MFR-12FTF52-1K","MFR-12FTF52-1K","Mouser","Mouser",1,8.5000000000000006E-2,10,4.5999999999999999E-2,100,1.6E-2,null,1000]
["1.5 kΩ","Resistor","603-MFR-12FTF52-1K5","MFR-12FTF52-1K5","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,1500]
["1.6 kΩ","Resistor","603-MFR-12FTF52-1K6","MFR-12FTF52-1K6","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,1600]
["2 kΩ","Resistor","603-MFR-12FTF52-2K0","MFR-12FTF52-2K0","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,2000]
["2.2 kΩ","Resistor","603-MFR-12FTF52-2K2","MFR-12FTF52-2K2","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,2200]
["2.4 kΩ","Resistor","603-MFR-12FTF52-2K4","MFR-12FTF52-2K4","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,2400]
["2.7 kΩ","Resistor","603-MFR-12FTF52-2K7","MFR-12FTF52-2K7","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,2700]
["3.3 kΩ","Resistor","603-MFR-12FTF52-3K3","MFR-12FTF52-3K3","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,3300]
["3.9 kΩ","Resistor","603-MFR-12FTF52-3K9","MFR-12FTF52-3K9","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,3900]
["4.7 kΩ","Resistor","603-MFR-12FTF52-4K7","MFR-12FTF52-4K7","Mouser","Mouser",1,8.5000000000000006E-2,10,4.5999999999999999E-2,100,1.6E-2,null,4700]
["5.1 kΩ","Resistor","603-MFR-12FTF52-5K1","MFR-12FTF52-5K1","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,5100]
["5.6 kΩ","Resistor","603-MFR-12FTF52-5K6","MFR-12FTF52-5K6","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,5600]
["6.2 kΩ","Resistor","603-MFR-12FTF52-6K2","MFR-12FTF52-6K2","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,6200]
["6.8 kΩ","Resistor","603-MFR-12FTF52-6K8","MFR-12FTF52-6K8","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,6800]
["7.5 kΩ","Resistor","603-MFR-12FTF52-7K5","MFR-12FTF52-7K5","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,7500]
["8.2 kΩ","Resistor","603-MFR-12FTF52-8K2","MFR-12FTF52-8K2","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,8200]
["10 kΩ","Resistor","603-MFR-12FTF52-10K","MFR-12FTF52-10K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,10000]
["12 kΩ","Resistor","603-MFR-12FTF52-12K","MFR-12FTF52-12K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,12000]
["13 kΩ","Resistor","603-MFR-12FTF52-13K","MFR-12FTF52-13K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,13000]
["15 kΩ","Resistor","603-MFR-12FTF52-15K","MFR-12FTF52-15K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,15000]
["18 kΩ","Resistor","603-MFR-12FTF52-18K","MFR-12FTF52-18K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,18000]
["20 kΩ","Resistor","603-MFR-12FTF52-20K","MFR-12FTF52-20K","Mouser","Mouser",1,8.5000000000000006E-2,10,4.5999999999999999E-2,100,1.6E-2,null,20000]
["22 kΩ","Resistor","603-MFR-12FTF52-22K","MFR-12FTF52-22K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,22000]
["24 kΩ","Resistor","603-MFR-12FTF52-24K","MFR-12FTF52-24K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,24000]
["27 kΩ","Resistor","603-MFR-12FTF52-27K","MFR-12FTF52-27K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,27000]
["30 kΩ","Resistor","603-MFR-12FTF52-30K","MFR-12FTF52-30K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,30000]
["33 kΩ","Resistor","603-MFR-12FTF52-33K","MFR-12FTF52-33K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,33000]
["36 kΩ","Resistor","603-MFR-12FTF52-36K","MFR-12FTF52-36K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,36000]
["39 kΩ","Resistor","603-MFR-12FTF52-39K","MFR-12FTF52-39K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,39000]
["47 kΩ","Resistor","603-MFR-12FTF52-47K","MFR-12FTF52-47K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,47000]
["51 kΩ","Resistor","603-MFR-12FTF52-51K","MFR-12FTF52-51K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,51000]
["56 kΩ","Resistor","603-MFR-12FTF52-56K","MFR-12FTF52-56K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,56000]
["62 kΩ","Resistor","603-MFR-12FTF52-62K","MFR-12FTF52-62K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,62000]
["75 kΩ","Resistor","603-MFR-12FTF52-75K","MFR-12FTF52-75K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,75000]
["91 kΩ","Resistor","603-MFR-12FTF52-91K","MFR-12FTF52-91K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,91000]
["100 kΩ","Resistor","603-MFR-12FTF52-100K","MFR-12FTF52-100K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,100000]
["120 kΩ","Resistor","603-MFR-12FTF52-120K","MFR-12FTF52-120K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,120000]
["150 kΩ","Resistor","603-MFR-12FTF52-150K","MFR-12FTF52-150K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,150000]
["180 kΩ","Resistor","603-MFR-12FTF52-180K","MFR-12FTF52-180K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,180000]
["200 kΩ","Resistor","603-MFR-12FTF52-200K","MFR-12FTF52-200K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,200000]
["220 kΩ","Resistor","603-MFR-12FTF52-220K","MFR-12FTF52-220K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,220000]
["330 kΩ","Resistor","603-MFR-12FTF52-330K","MFR-12FTF52-330K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,330000]
["360 kΩ","Resistor","603-MFR-12FTF52-360K","MFR-12FTF52-360K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,360000]
["390 kΩ","Resistor","603-MFR-12FTF52-390K","MFR-12FTF52-390K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,390000]
["430 kΩ","Resistor","603-MFR-12FTF52-430K","MFR-12FTF52-430K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,430000]
["470 kΩ","Resistor","603-MFR-12FTF52-470K","MFR-12FTF52-470K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,470000]
["820 kΩ","Resistor","603-MFR-12FTF52-820K","MFR-12FTF52-820K","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,820000]
["1 MΩ","Resistor","603-MFR-12FTF52-1M","MFR-12FTF52-1M","Mouser","Mouser",1,0.11899999999999999,10,0.06,100,2.1000000000000001E-2,null,1000000]
["1.5 MΩ","Resistor","603-MFR-12FTF52-1M5","MFR-12FTF52-1M5","Mouser","Mouser",1,0.17899999999999999,10,0.111,100,3.6999999999999998E-2,null,1500000]
["2 MΩ","Resistor","603-MFR-12FTF52-2M","MFR-12FTF52-2M","Mouser","Mouser",1,0.14499999999999999,10,9.8000000000000004E-2,100,8.5999999999999993E-2,null,2000000]
["2.2 MΩ, 5%","Resistor","603-MFR-12FTF52-2M2","MFR-12FTF52-2M2","Mouser","Mouser",1,0.17899999999999999,10,0.111,100,3.6999999999999998E-2,null,2200000]
["3.3 MΩ, 5%","Resistor","603-MFR-12FTF52-3M3","MFR-12FTF52-3M3","Mouser","Mouser",1,0.17899999999999999,10,0.111,100,3.6999999999999998E-2,null,3300000]
["4.7 MΩ, 5%","Resistor","603-MFR-12FTF52-4M7","MFR-12FTF52-4M7","Mouser","Mouser",1,0.17899999999999999,10,0.111,100,3.6999999999999998E-2,null,4700000]
["6.8 MΩ","Resistor","603-MFR-12FTF52-6M8","MFR-12FTF52-6M8","Mouser","Mouser",1,0.13600000000000001,10,8.3000000000000004E-2,100,2.7E-2,null,6800000]
["196 Ω","Resistor-F","603-MFR-25FBF52-196R","MFR-25FBF52-196R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,196]
["237 Ω","Resistor-F","603-MFR-25FBF52-237R",{"$f":"RIGHT(C208,LEN(C208)-4)","v":"MFR-25FBF52-237R"},"Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,{"$f":"IF(MID(A208,FIND(\"Ω\",A208)-1,1)=\"k\",LEFT(A208,FIND(\"k\",A208)-1)*1000,LEFT(A208,FIND(\"Ω\",A208)-1)*1)","v":237}]
["249 Ω","Resistor-F","603-MFR-25FBF52-249R","MFR-25FBF52-249R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,249]
["287 Ω","Resistor-F","603-MFR-25FBF52-287R","MFR-25FBF52-287R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,287]
["301 Ω","Resistor-F","603-MFR-25FBF52-301R","MFR-25FBF52-301R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,301]
["316 Ω","Resistor-F","603-MFR-25FBF52-316R","MFR-25FBF52-316R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,316]
["348 Ω","Resistor-F","603-MFR-25FBF52-348R","MFR-25FBF52-348R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,348]
["365 Ω","Resistor-F","603-MFR-25FBF52-365R","MFR-25FBF52-365R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,365]
["383 Ω","Resistor-F","603-MFR-25FBF52-383R","MFR-25FBF52-383R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,383]
["402 Ω","Resistor-F","603-MFR-25FBF52-402R","MFR-25FBF52-402R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,402]
["422 Ω","Resistor-F","603-MFR-25FBF52-422R","MFR-25FBF52-422R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,422]
["442 Ω","Resistor-F","603-MFR-25FBF52-442R","MFR-25FBF52-442R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,442]
["464 Ω","Resistor-F","603-MFR-25FBF52-464R","MFR-25FBF52-464R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,464]
["487 Ω","Resistor-F","603-MFR-25FBF52-487R","MFR-25FBF52-487R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,487]
["511 Ω","Resistor-F","603-MFR-25FBF52-511R","MFR-25FBF52-511R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,511]
["536 Ω","Resistor-F","603-MFR-25FBF52-536R","MFR-25FBF52-536R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,536]
["562 Ω","Resistor-F","603-MFR-25FBF52-562R","MFR-25FBF52-562R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,562]
["590 Ω","Resistor-F","603-MFR-25FBF52-590R","MFR-25FBF52-590R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,590]
["619 Ω","Resistor-F","603-MFR-25FBF52-619R","MFR-25FBF52-619R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,619]
["649 Ω","Resistor-F","603-MFR-25FBF52-649R","MFR-25FBF52-649R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,649]
["681 Ω","Resistor-F","603-MFR-25FBF52-681R","MFR-25FBF52-681R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,681]
["715 Ω","Resistor-F","603-MFR-25FBF52-715R","MFR-25FBF52-715R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,715]
["750 Ω","Resistor-F","603-MFR-25FBF52-750R","MFR-25FBF52-750R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,750]
["787 Ω","Resistor-F","603-MFR-25FRF52-787R","MFR-25FRF52-787R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,787]
["825 Ω","Resistor-F","603-MFR-25FBF52-825R","MFR-25FBF52-825R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,825]
["866 Ω","Resistor-F","603-MFR-25FBF52-866R","MFR-25FBF52-866R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,866]
["909 Ω","Resistor-F","603-MFR-25FBF52-909R","MFR-25FBF52-909R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,909]
["953 Ω","Resistor-F","603-MFR-25FBF52-953R","MFR-25FBF52-953R","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,953]
["1 kΩ","Resistor-F","603-MFR-25FBF52-1K","MFR-25FBF52-1K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1000]
["1.05 kΩ","Resistor-F","603-MFR-25FBF52-1K05","MFR-25FBF52-1K05","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1050]
["1.1 kΩ","Resistor-F","603-MFR-25FBF52-1K1","MFR-25FBF52-1K1","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1100]
["1.15 kΩ","Resistor-F","603-MFR-25FBF52-1K15","MFR-25FBF52-1K15","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1150]
["1.21 kΩ","Resistor-F","603-MFR-25FBF52-1K21","MFR-25FBF52-1K21","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1210]
["1.27 kΩ","Resistor-F","603-MFR-25FBF52-1K27","MFR-25FBF52-1K27","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1270]
["1.33 kΩ","Resistor-F","603-MFR-25FBF52-1K33","MFR-25FBF52-1K33","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1330]
["1.4 kΩ","Resistor-F","603-MFR-25FBF52-1K4","MFR-25FBF52-1K4","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1400]
["1.69 kΩ","Resistor-F","603-MFR-25FBF52-1K69","MFR-25FBF52-1K69","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1690]
["1.78 kΩ","Resistor-F","603-MFR-25FBF52-1K78","MFR-25FBF52-1K78","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,1780]
["6.81 kΩ","Resistor-F","603-MFR-25FBF52-6K81","MFR-25FBF52-6K81","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,6810]
["8.66 kΩ","Resistor-F","603-MFR-25FBF52-8K66","MFR-25FBF52-8K66","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,8660]
["9.09 kΩ","Resistor-F","603-MFR-25FBF52-9K09","MFR-25FBF52-9K09","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,9090]
["11 kΩ","Resistor-F","603-MFR-25FBF52-11K","MFR-25FBF52-11K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,11000]
["11.5 kΩ","Resistor-F","603-MFR-25FBF52-11K5","MFR-25FBF52-11K5","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,11500]
["12.1 kΩ","Resistor-F","603-MFR-25FBF52-12K1","MFR-25FBF52-12K1","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,12100]
["14 kΩ","Resistor-F","603-MFR-25FBF52-14K","MFR-25FBF52-14K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,14000]
["14.7 kΩ","Resistor-F","603-MFR-25FBF52-14K7","MFR-25FBF52-14K7","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,14700]
["15.4 kΩ","Resistor-F","603-MFR-25FBF52-15K4","MFR-25FBF52-15K4","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,15400]
["16.2 kΩ","Resistor-F","603-MFR-25FBF52-16K2","MFR-25FBF52-16K2","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,16200]
["17.8 kΩ","Resistor-F","603-MFR-25FBF52-17K8","MFR-25FBF52-17K8","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,17800]
["18.7 kΩ","Resistor-F","603-MFR-25FBF52-18K7","MFR-25FBF52-18K7","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,18700]
["19.6 kΩ","Resistor-F","603-MFR-25FBF52-19K6","MFR-25FBF52-19K6","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,19600]
["20.5 kΩ","Resistor-F","603-MFR-25FBF52-20K5","MFR-25FBF52-20K5","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,20500]
["22.6 kΩ","Resistor-F","603-MFR-25FBF52-22K6","MFR-25FBF52-22K6","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,22600]
["23.7 kΩ","Resistor-F","603-MFR-25FBF52-23K7","MFR-25FBF52-23K7","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,23700]
["24.9 kΩ","Resistor-F","603-MFR-25FBF52-24K9","MFR-25FBF52-24K9","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,24900]
["26.1 kΩ","Resistor-F","603-MFR-25FBF52-26K1","MFR-25FBF52-26K1","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,26100]
["28.7 kΩ","Resistor-F","603-MFR-25FBF52-28K7","MFR-25FBF52-28K7","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,28700]
["30.1 kΩ","Resistor-F","603-MFR-25FBF52-30K1","MFR-25FBF52-30K1","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,30100]
["31.6 kΩ","Resistor-F","603-MFR-25FBF52-31K6","MFR-25FBF52-31K6","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,31600]
["33.2 kΩ","Resistor-F","603-MFR-25FBF52-33K2","MFR-25FBF52-33K2","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,33200]
["36.5 kΩ","Resistor-F","603-MFR-25FBF52-36K5","MFR-25FBF52-36K5","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,36500]
["38.3 kΩ","Resistor-F","603-MFR-25FBF52-38K3","MFR-25FBF52-38K3","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,38300]
["40.2 kΩ","Resistor-F","603-MFR-25FBF52-40K2","MFR-25FBF52-40K2","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,40200]
["42.2 kΩ","Resistor-F","603-MFR-25FBF52-42K2","MFR-25FBF52-42K2","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,42200]
["46.4 kΩ","Resistor-F","603-MFR-25FBF52-46K4","MFR-25FBF52-46K4","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,46400]
["48.7 kΩ","Resistor-F","603-MFR-25FBF52-48K7",{"$f":"RIGHT(C272,LEN(C272)-4)","v":"MFR-25FBF52-48K7"},"Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,{"$f":"IF(MID(A272,FIND(\"Ω\",A272)-1,1)=\"k\",LEFT(A272,FIND(\"k\",A272)-1)*1000,LEFT(A272,FIND(\"Ω\",A272)-1)*1)","v":48700}]
["51.1 kΩ","Resistor-F","603-MFR-25FBF52-51K1","MFR-25FBF52-51K1","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,51100]
["53.6 kΩ","Resistor-F","603-MFR-25FTE52-53K6","MFR-25FTE52-53K6","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,53600]
["59 kΩ","Resistor-F","603-MFR-25FBF52-59K","MFR-25FBF52-59K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,59000]
["61.9 kΩ","Resistor-F","603-MFR-25FBF52-61K9","MFR-25FBF52-61K9","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,61900]
["64.9 kΩ","Resistor-F","603-MFR-25FBF52-64K9","MFR-25FBF52-64K9","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,64900.000000000007]
["68.1 kΩ","Resistor-F","603-MFR-25FBF52-68K1","MFR-25FBF52-68K1","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,68100]
["75 kΩ","Resistor-F","603-MFR-25FBF52-75K","MFR-25FBF52-75K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,75000]
["78.7 kΩ","Resistor-F","603-MFR-25FRF52-78K7","MFR-25FRF52-78K7","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,78700]
["82.5 kΩ","Resistor-F","603-MFR-25FBF52-82K5","MFR-25FBF52-82K5","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,82500]
["86.6 kΩ","Resistor-F","603-MFR-25FBF52-86K6","MFR-25FBF52-86K6","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,86600]
["95.3 kΩ","Resistor-F","603-MFR-25FBF52-95K3","MFR-25FBF52-95K3","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,95300]
["105 kΩ","Resistor-F","603-MFR-25FBF52-105K","MFR-25FBF52-105K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,105000]
["110 kΩ","Resistor-F","603-MFR-25FBF52-110K","MFR-25FBF52-110K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,110000]
["121 kΩ","Resistor-F","603-MFR-25FBF52-121K","MFR-25FBF52-121K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,121000]
["133 kΩ","Resistor-F","603-MFR-25FBF52-133K","MFR-25FBF52-133K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,133000]
["169 kΩ","Resistor-F","603-MFR-25FBF52-169K","MFR-25FBF52-169K","Mouser","Mouser",1,0.10199999999999999,10,5.3999999999999999E-2,100,1.9E-2,null,169000]
["100 Ω","Resistor",1565270,"MFR3-100RFC","Farnell2","Farnell",10,4.0599999999999997E-2,100,2.2700000000000001E-2]
["220 Ω","Resistor",1565294,"MFR3-220RFC","Farnell2","Farnell",10,4.9000000000000002E-2,100,2.3E-2]
["470 Ω","Resistor",1565316,"MFR3-470RFC","Farnell2","Farnell",10,3.0099999999999998E-2,100,1.9E-2]
["1 kΩ","Resistor",1565287,"MFR3-1K0FC","Farnell2","Farnell",10,4.1000000000000002E-2,100,2.29E-2]
["2.2 kΩ","Resistor",1565301,"MFR3-2K2FC","Farnell2","Farnell",10,3.04E-2,100,1.9199999999999998E-2]
["2.7 kΩ","Resistor",1565302,"MFR3-2K7FC","Farnell2","Farnell",10,3.0099999999999998E-2,100,1.9E-2]
["3.3 kΩ","Resistor",1565313,"MFR3-3K3FC","Farnell2","Farnell",10,3.0099999999999998E-2,100,1.9E-2]
["3.9 kΩ","Resistor",1565314,"MFR3-3K9FC","Farnell2","Farnell",10,3.0099999999999998E-2,100,1.9E-2]
["4.7 kΩ","Resistor",1565318,"MFR3-4K7FC","Farnell2","Farnell",10,4.1000000000000002E-2,100,2.29E-2]
["5.6 kΩ","Resistor",1565324,"MFR3-5K6FC","Farnell2","Farnell",10,4.0599999999999997E-2,100,2.2700000000000001E-2]
["6.8 kΩ","Resistor",1565329,"MFR3-6K8FC","Farnell2","Farnell",10,3.04E-2,100,1.9199999999999998E-2]
["8.2 kΩ","Resistor",1565335,"MFR3-8K2FC","Farnell2","Farnell",10,3.04E-2,100,1.9199999999999998E-2]
["10 kΩ","Resistor",1565271,"MFR3-10KFC","Farnell2","Farnell",10,4.1000000000000002E-2,100,2.29E-2]
["12 kΩ","Resistor",1565275,"MFR3-12KFC","Farnell2","Farnell",10,4.0599999999999997E-2,100,2.2700000000000001E-2]
["15 kΩ","Resistor",1565281,"MFR3-15KFC","Farnell2","Farnell",10,4.0599999999999997E-2,100,2.2700000000000001E-2]
["18 kΩ","Resistor",1565285,"MFR3-18KFC","Farnell2","Farnell",10,3.0099999999999998E-2,100,1.9E-2]
["22 kΩ","Resistor",1565295,"MFR3-22KFC","Farnell2","Farnell",10,4.0599999999999997E-2,100,2.2700000000000001E-2]
["27 kΩ","Resistor",1565299,"MFR3-27KFC","Farnell2","Farnell",10,3.8800000000000001E-2,100,2.4400000000000002E-2]
["33 kΩ","Resistor",1565305,"MFR3-33KFC","Farnell2","Farnell",10,4.0599999999999997E-2,100,2.2700000000000001E-2]
["39 kΩ","Resistor",1565311,"MFR3-39KFC","Farnell2","Farnell",10,3.0099999999999998E-2,100,1.9E-2]
["47 kΩ","Resistor",1565317,"MFR3-47KFC","Farnell2","Farnell",10,3.04E-2,100,1.9199999999999998E-2]
["56 kΩ","Resistor",1565322,"MFR3-56KFC","Farnell2","Farnell",10,3.0099999999999998E-2,100,1.9E-2]
["100 kΩ","Resistor",1565269,"MFR3-100KFC","Farnell2","Farnell",10,4.1000000000000002E-2,100,2.29E-2]
["120 kΩ","Resistor",1565273,"MFR3-120KFC","Farnell2","Farnell",10,3.04E-2,100,1.9199999999999998E-2]
["220 kΩ","Resistor",1565293,"MFR3-220KFC","Farnell2","Farnell",10,3.04E-2,100,1.9199999999999998E-2]
["330 kΩ","Resistor",1565303,"MFR3-330KFC","Farnell2","Farnell",10,4.0599999999999997E-2,100,2.2700000000000001E-2]
["470 kΩ","Resistor",1565315,"MFR3-470KFC","Farnell2","Farnell",10,3.0099999999999998E-2,100,1.9E-2]